Installation

| PIX Firewall & VPN Concentrator Simulators

PIX Firewall

Basic PIX Configuration

Config NAT Stats and Conduits

Configure Multiple Interfaces

Configure the PIX as a DHCP Server

Configuring PIX as a DHCP client

Configuring Logging

Configuring Logging - Verification

Denying outbound Traffic

Allowing Outbound Traffic

Configure PIX to work with WebSense

Installing WebSense

Configure WebSence to block by URL

Configure Websense to block by workstation

Configure the Fixup Protocol on PIX

Configuring PIX for IDS signature

CSACS Install and Add User

Configuring Authentication

Config the Primary PIX Firewall

Configure IKE and IPSec on the PIX

Verify IPSec Configuration

Password Recovery & Image Update

Configuring the CSIS Feature Set

Configure Cisco Secure ACS Set

Configure AAA and Authentication Proxy

Verify Authentication Proxy Configuration

- Introduction
- PIX Firewall
- VPN Concentrator

CD Problems and Help files

If there are any errors or items that are unclear in this help file please email so that they can be corrected or the information improved.

Any comments appreciated.

Copyright © 2005 CiscoSid