
routerIGRPC.addSC("default", "Set a command to its defaults");
routerIGRPC.addSC("default-information", "Control distribution of default information");
	routerIGRPC["default-information"].addSC("allowed", "Allow default information");
	routerIGRPC["default-information"].addSC("in", "Accept default routing information");
	routerIGRPC["default-information"].addSC("out", "Output default routing information");
routerIGRPC.addSC("default-metric", "Set metric of redistributed routes");
	routerIGRPC["default-metric"].addSC("<1-4294967295>", "Bandwidth in Kbits per second");
routerIGRPC.addSC("distance", "Define an administrative distance");
	routerIGRPC.distance.addSC("<1-255>", "Administrative distance");
routerIGRPC.addSC("distribute-list", "Filter networks in routing updates");
	routerIGRPC["distribute-list"].addSC("<1-199>", "IP access list number");
	routerIGRPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
	routerIGRPC["distribute-list"].addSC("WORD", "Access-list name");
	routerIGRPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
	routerIGRPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
routerIGRPC.addSC("exit", "Exit from routing protocol configuration mode");
routerIGRPC.addSC("help", "Description of the interactive help system");
routerIGRPC.addSC("input-queue", "Specify input queue depth");
	routerIGRPC["input-queue"].addSC("<0-1024>", "queue depth");
routerIGRPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerIGRPC["maximum-paths"].addSC("<1-6>", "Number of paths");
routerIGRPC.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerIGRPC.metric.addSC("holddown", "Enable IGRP holddown");
	routerIGRPC.metric.addSC("maximum-hops", "Advertise IGRP routes greater than <hops> as unreachable");
	routerIGRPC.metric.addSC("weights", "Modify IGRP metric coefficients");
routerIGRPC.addSC("mpls", "Configure MPLS routing protocol parameters");
routerIGRPC.addSC("neighbor", "Specify a neighbor router");
	routerIGRPC.neighbor.addSC("A.B.C.D", "Neighbor address");
routerIGRPC.addSC("network", "Enable routing on an IP network");
	routerIGRPC.network.addSC("A.B.C.D", "Network number");
routerIGRPC.addSC("no", "Negate a command or set its defaults");
	routerIGRPC.no.addSC("default-information", "Control distribution of default information");
	routerIGRPC.no.addSC("default-metric", "Set metric of redistributed routes");
	routerIGRPC.no.addSC("distance", "Define an administrative distance");
	routerIGRPC.no.addSC("distribute-list", "Filter networks in routing updates");
	routerIGRPC.no.addSC("input-queue", "Specify input queue depth");
	routerIGRPC.no.addSC("maximum-paths", "Forward packets over multiple paths");
	routerIGRPC.no.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerIGRPC.no.addSC("mpls", "Configure MPLS routing protocol parameters");
	routerIGRPC.no.addSC("neighbor", "Specify a neighbor router");
	routerIGRPC.no.addSC("network", "Enable routing on an IP network");
	routerIGRPC.no.addSC("validate-update-sour", "");
routerIGRPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
	routerIGRPC["offset-list"].addSC("<0-99>", "Access list of networks to apply offset (0 selects all networks)");
	routerIGRPC["offset-list"].addSC("<1300-1999>", "Access list of networks to apply offset (expanded range)");
	routerIGRPC["offset-list"].addSC("WORD", "Access-list name");
routerIGRPC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerIGRPC["passive-interface"].addSC("Async", "Async interface");
	routerIGRPC["passive-interface"].addSC("BRI", "ISDN Basic Rate Interface");
	routerIGRPC["passive-interface"].addSC("BVI", "Bridge-Group Virtual Interface");
	routerIGRPC["passive-interface"].addSC("CTunnel", "CTunnel interface");
	routerIGRPC["passive-interface"].addSC("Dialer", "Dialer interface");
	routerIGRPC["passive-interface"].addSC("Ethernet", "IEEE 802.3");
	routerIGRPC["passive-interface"].addSC("Group-Async", "Async Group interface");
	routerIGRPC["passive-interface"].addSC("Lex", "Lex interface");
	routerIGRPC["passive-interface"].addSC("Loopback", "Loopback interface");
	routerIGRPC["passive-interface"].addSC("Multilink", "Multilink-group interface");
	routerIGRPC["passive-interface"].addSC("Null", "Null interface");
	routerIGRPC["passive-interface"].addSC("Serial", "Serial");
	routerIGRPC["passive-interface"].addSC("Tunnel", "Tunnel interface");
	routerIGRPC["passive-interface"].addSC("Vif", "PGM Multicast Host interface");
	routerIGRPC["passive-interface"].addSC("Virtual-Template", "Virtual Template interface");
	routerIGRPC["passive-interface"].addSC("Virtual-TokenRing", "Virtual TokenRing");
	routerIGRPC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerIGRPC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerIGRPC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
	routerIGRPC.redistribute.addSC("connected", "Connected");
	routerIGRPC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
	routerIGRPC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
	routerIGRPC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
	routerIGRPC.redistribute.addSC("isis", "ISO IS-IS");
	routerIGRPC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
	routerIGRPC.redistribute.addSC("metric", "Metric for redistributed routes");
	routerIGRPC.redistribute.addSC("mobile", "Mobile routes");
	routerIGRPC.redistribute.addSC("odr", "On Demand stub Routes");
	routerIGRPC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
	routerIGRPC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
	routerIGRPC.redistribute.addSC("route-map", "Route map reference");
	routerIGRPC.redistribute.addSC("static", "Static routes");
routerIGRPC.addSC("timers", "Adjust routing timers");
	routerIGRPC.timers.addSC("basic", "Basic routing protocol update timers");
routerIGRPC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerIGRPC["traffic-share"].addSC("balanced", "Share inversely proportional to metric");
	routerIGRPC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
routerIGRPC.addSC("validate-update-source", "Perform sanity checks against source address of routing updates");
routerIGRPC.addSC("variance", "Control load balancing variance");
	routerIGRPC.variance.addSC("<1-128>", "Metric variance multiplier");
