intVlanC.addSC("access-expression", "Build a bridge boolean access expression");
	intVlanC["access-expression"].addSC("input", "Filter input packets");
		intVlanC["access-expression"].input.addSC("LINE", "A boolean expression of bridge access lists");
	intVlanC["access-expression"].addSC("output", "Filter output packets");
		intVlanC["access-expression"].output.addSC("LINE", "A boolean expression of bridge access lists");
intVlanC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intVlanC.arp.addSC("arpa", "Standard arp protocol");
	intVlanC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	intVlanC.arp.addSC("probe", "HP style arp protocol");
	intVlanC.arp.addSC("snap", "IEEE 802.3 style arp");
	intVlanC.arp.addSC("timeout", "Set ARP cache timeout");
		intVlanC.arp.timeout.addSC("<0-2147483>", "Seconds");
intVlanC.addSC("bandwidth", "Set bandwidth informational parameter");
	intVlanC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intVlanC.addSC("bridge-group", "Transparent bridging interface parameters");
	intVlanC["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
		intVlanC["bridge-group"]["<1-255>"].addSC("circuit-group", "Associate serial interface with a circuit group");
			intVlanC["bridge-group"]["<1-255>"]["circuit-group"].addSC("<1-9>", "Circuit group number");
		intVlanC["bridge-group"]["<1-255>"].addSC("input-address-list", "Filter packets by source address");
			intVlanC["bridge-group"]["<1-255>"]["input-address-list"].addSC("<700-799>", "Ethernet address access list");
		intVlanC["bridge-group"]["<1-255>"].addSC("input-lat-service-deny", "Deny input LAT service advertisements matching a group list");
			intVlanC["bridge-group"]["<1-255>"]["input-lat-service-deny"].addSC("<grouplist>", "A list of LAT service advertisements");
			intVlanC["bridge-group"]["<1-255>"]["input-lat-service-deny"].addSC("all", "All LAT groups");
				intVlanC["bridge-group"]["<1-255>"]["input-lat-service-deny"].all.addSC("disabled", "Remove from existing group code list");
				intVlanC["bridge-group"]["<1-255>"]["input-lat-service-deny"].all.addSC("enabled", "Add to existing group code list");
		intVlanC["bridge-group"]["<1-255>"].addSC("input-lat-service-permit", "Permit input LAT service advertisements matching a group list");
			intVlanC["bridge-group"]["<1-255>"]["input-lat-service-permit"].addSC("<grouplist>", "A list of LAT service advertisements");
			intVlanC["bridge-group"]["<1-255>"]["input-lat-service-permit"].addSC("all", "All LAT groups");
				intVlanC["bridge-group"]["<1-255>"]["input-lat-service-permit"].all.addSC("disabled", "Remove from existing group code list");
				intVlanC["bridge-group"]["<1-255>"]["input-lat-service-permit"].all.addSC("enabled", "Add to existing group code list");
		intVlanC["bridge-group"]["<1-255>"].addSC("input-lsap-list", "Filter incoming IEEE 802.3 encapsulated packets");
			intVlanC["bridge-group"]["<1-255>"]["input-lsap-list"].addSC("<200-299>", "Ethernet type access list");
		intVlanC["bridge-group"]["<1-255>"].addSC("input-pattern-list", "Filter input with a pattern list");
			intVlanC["bridge-group"]["<1-255>"]["input-pattern-list"].addSC("<1100-1199>", "Pattern access list number");
		intVlanC["bridge-group"]["<1-255>"].addSC("input-type-list", "Filter incoming Ethernet packets by type code");
			intVlanC["bridge-group"]["<1-255>"]["input-type-list"].addSC("<200-299>", "Ethernet type access list");
		intVlanC["bridge-group"]["<1-255>"].addSC("lat-compression", "Enable LAT compression over serial or ATM interfaces");
		intVlanC["bridge-group"]["<1-255>"].addSC("output-address-list", "Filter packets by destination address");
			intVlanC["bridge-group"]["<1-255>"]["output-address-list"].addSC("<700-799>", "Ethernet address access list");
		intVlanC["bridge-group"]["<1-255>"].addSC("output-lat-service-deny", "Deny output LAT service advertisements matching a group list");
			intVlanC["bridge-group"]["<1-255>"]["output-lat-service-deny"].addSC("<grouplist>", "A list of LAT service advertisements");
			intVlanC["bridge-group"]["<1-255>"]["output-lat-service-deny"].addSC("all", "All LAT groups");
				intVlanC["bridge-group"]["<1-255>"]["output-lat-service-deny"].all.addSC("disabled", "Remove from existing group code list");
				intVlanC["bridge-group"]["<1-255>"]["output-lat-service-deny"].all.addSC("enabled", "Add to existing group code list");
		intVlanC["bridge-group"]["<1-255>"].addSC("output-lat-service-permit", "Permit output LAT service advertisements matching a group list");
			intVlanC["bridge-group"]["<1-255>"]["output-lat-service-permit"].addSC("<grouplist>", "A list of LAT service advertisements");
			intVlanC["bridge-group"]["<1-255>"]["output-lat-service-permit"].addSC("all", "All LAT groups");
				intVlanC["bridge-group"]["<1-255>"]["output-lat-service-permit"].all.addSC("disabled", "Remove from existing group code list");
				intVlanC["bridge-group"]["<1-255>"]["output-lat-service-permit"].all.addSC("enabled", "Add to existing group code list");
		intVlanC["bridge-group"]["<1-255>"].addSC("output-lsap-list", "Filter outgoing IEEE 802.3 encapsulated packets");
			intVlanC["bridge-group"]["<1-255>"]["output-lsap-list"].addSC("<200-299>", "Ethernet type access list");
		intVlanC["bridge-group"]["<1-255>"].addSC("output-pattern-list", "Filter output with a pattern list");
			intVlanC["bridge-group"]["<1-255>"]["output-pattern-list"].addSC("<1100-1199>", "Pattern access list number");
		intVlanC["bridge-group"]["<1-255>"].addSC("output-type-list", "Filter outgoing Ethernet packets by type code");
			intVlanC["bridge-group"]["<1-255>"]["output-type-list"].addSC("<200-299>", "Ethernet type access list");
		intVlanC["bridge-group"]["<1-255>"].addSC("path-cost", "Set interface path cost");
			intVlanC["bridge-group"]["<1-255>"]["path-cost"].addSC("<0-65535>", "Path cost (higher values are higher costs)");
		intVlanC["bridge-group"]["<1-255>"].addSC("priority", "Set interface priority");
			intVlanC["bridge-group"]["<1-255>"].priority.addSC("<0-255>", "");
		intVlanC["bridge-group"]["<1-255>"].addSC("spanning-disabled", "Disable spanning tree on a bridge group");
		intVlanC["bridge-group"]["<1-255>"].addSC("subscriber-loop-control", "Configure subscriber loop control");
intVlanC.addSC("cdp", "CDP interface subcommands");
	intVlanC.cdp.addSC("enable", "Enable CDP on interface");
intVlanC.addSC("custom-queue-list", "Assign a custom queue list to an interface");
	intVlanC["custom-queue-list"].addSC("<1-16>", "Custom queue list number");
intVlanC.addSC("default", "Set a command to its defaults");

intVlanC.addSC("delay", "Specify interface throughput delay");
	intVlanC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
intVlanC.addSC("description", "Interface specific description");
	intVlanC.description.addSC("LINE", "Up to 240 characters describing this interface");
intVlanC.addSC("exit", "Exit from interface configuration mode");
intVlanC.addSC("fair-queue", "Enable Fair Queuing on an Interface");
	intVlanC["fair-queue"].addSC("<1-4096>", "Congestive Discard Threshold");
		intVlanC["fair-queue"]["<1-4096>"].addSC("<16-4096>", "Number Dynamic Conversation Queues");
			intVlanC["fair-queue"]["<1-4096>"]["<16-4096>"].addSC("<0-1000>", "Number Reservable Conversation Queues");
intVlanC.addSC("help", "Description of the interactive help system");
intVlanC.addSC("hold-queue", "Set hold queue depth");
	intVlanC["hold-queue"].addSC("<0-4096>", "Queue length");
		intVlanC["hold-queue"]["<0-4096>"].addSC("in", "Input queue");
		intVlanC["hold-queue"]["<0-4096>"].addSC("out", "Output queue");

intVlanC.addSC("ip", "Interface Internet Protocol config commands");
	intVlanC.ip.addSC("access-group", "Specify access control for packets");
		intVlanC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intVlanC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
			intVlanC.ip["access-group"]["<1-199>"].addSC("out", "outbound packets");
		intVlanC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			intVlanC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
			intVlanC.ip["access-group"]["<1300-2699>"].addSC("out", "outbound packets");
		intVlanC.ip["access-group"].addSC("WORD", "Access-list name");
			intVlanC.ip["access-group"].WORD.addSC("in", "inbound packets");
			intVlanC.ip["access-group"].WORD.addSC("out", "outbound packets");
	intVlanC.ip.addSC("accounting", "Enable IP accounting on this interface");
		intVlanC.ip.accounting.addSC("access-violations", "Account for IP packets violating access lists on this interface");
		intVlanC.ip.accounting.addSC("mac-address", "Account for MAC addresses seen on this interface");
			intVlanC.ip.accounting["mac-address"].addSC("input", "Source MAC address on received packets");
			intVlanC.ip.accounting["mac-address"].addSC("output", "Destination MAC address on transmitted packets");
		intVlanC.ip.accounting.addSC("output-packets", "Account for IP packets output on this interface");
		intVlanC.ip.accounting.addSC("precedence", "Count packets by IP precedence on this interface");
			intVlanC.ip.accounting.precedence.addSC("input", "received packets");
			intVlanC.ip.accounting.precedence.addSC("output", "transmitted packets");
	intVlanC.ip.addSC("address", "Set the IP address of an interface");
		intVlanC.ip.address.addSC("A.B.C.D", "IP address");
			intVlanC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intVlanC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	intVlanC.ip.addSC("authentication", "authentication subcommands");
		intVlanC.ip.authentication.addSC("key-chain", "key-chain");
			intVlanC.ip.authentication["key-chain"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.ip.authentication["key-chain"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intVlanC.ip.authentication.addSC("mode", "mode");
			intVlanC.ip.authentication.mode.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.ip.authentication.mode.eigrp.addSC("<1-65535>", "Autonomous system number");
	intVlanC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		intVlanC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intVlanC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intVlanC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>", "Maximum bandwidth percentage that EIGRP may use");
	intVlanC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intVlanC.ip["broadcast-address"].addSC("A.B.C.D", "IP broadcast address");
	intVlanC.ip.addSC("cef", "Cisco Express Fowarding interface commands");
		intVlanC.ip.cef.addSC("accounting", "CEF accounting features for interface");
			intVlanC.ip.cef.accounting.addSC("non-recursive", "CEF non-recursive accounting features");
				intVlanC.ip.cef.accounting["non-recursive"].addSC("external", "Count input traffic in non-recursive external bin");
				intVlanC.ip.cef.accounting["non-recursive"].addSC("internal", "Count input traffic in non-recursive internal bin");
	intVlanC.ip.addSC("cgmp", "Enable/disable CGMP");
		intVlanC.ip.cgmp.addSC("proxy", "CGMP for hosts and proxy for multicast routers");
		intVlanC.ip.cgmp.addSC("router-only", "CGMP proxy for multicast routers only");
	intVlanC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intVlanC.ip["directed-broadcast"].addSC("<1-199>", "A standard IP access list number");
		intVlanC.ip["directed-broadcast"].addSC("<1300-2699>", "A standard IP expanded access list number");

	intVlanC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		intVlanC.ip["hello-interval"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intVlanC.ip["hello-interval"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intVlanC.ip["hello-interval"].eigrp["<1-65535>"].addSC("<1-65535>", "Seconds between hello transmissions");
	intVlanC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		intVlanC.ip["helper-address"].addSC("A.B.C.D", "IP destination address");
	intVlanC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		intVlanC.ip["hold-time"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intVlanC.ip["hold-time"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intVlanC.ip["hold-time"].eigrp["<1-65535>"].addSC("<1-65535>", "Seconds before neighbor is considered down");
	intVlanC.ip.addSC("igmp", "IGMP interface commands");
		intVlanC.ip.igmp.addSC("access-group", "IGMP group access group");
		intVlanC.ip.igmp.addSC("helper-address", "IGMP helper address");
			intVlanC.ip.igmp["helper-address"].addSC("A.B.C.D", "IGMP helper address");
		intVlanC.ip.igmp.addSC("join-group", "IGMP join multicast group");
			intVlanC.ip.igmp["join-group"].addSC("A.B.C.D", "IP group address");
		intVlanC.ip.igmp.addSC("last-member-query-interval", "IGMP last member query interval");
			intVlanC.ip.igmp["last-member-query-interval"].addSC("<100-65535>", "Last member query interval in milliseconds");
		intVlanC.ip.igmp.addSC("querier-timeout", "IGMP previous querier timeout");
			intVlanC.ip.igmp["querier-timeout"].addSC("<60-300>", "timeout value in seconds");
		intVlanC.ip.igmp.addSC("query-interval", "IGMP host query interval");
			intVlanC.ip.igmp["query-interval"].addSC("<1-65535>", "Query interval in seconds");
		intVlanC.ip.igmp.addSC("query-max-response-time", "IGMP max query response value");
			intVlanC.ip.igmp["query-max-response-time"].addSC("<1-25>", "query response value in seconds");
		intVlanC.ip.igmp.addSC("static-group", "IGMP static multicast group");
			intVlanC.ip.igmp["static-group"].addSC("*", "Populated for all groups");
			intVlanC.ip.igmp["static-group"].addSC("A.B.C.D", "IP group address");
		intVlanC.ip.igmp.addSC("unidirectional-link", "IGMP unidirectional link multicast routing");
		intVlanC.ip.igmp.addSC("version", "IGMP version");
			intVlanC.ip.igmp.version.addSC("<1-2>", "version number");


	intVlanC.ip.addSC("load-sharing", "Style of load sharing");
		intVlanC.ip["load-sharing"].addSC("per-destination", "Deterministic distribution");
		intVlanC.ip["load-sharing"].addSC("per-packet", "Random distribution");
	intVlanC.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
	intVlanC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	intVlanC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		intVlanC.ip.mrm.addSC("test-receiver", "Enable IP MRM test receiver operation");
		intVlanC.ip.mrm.addSC("test-sender", "Enable IP MRM test sender operation");
		intVlanC.ip.mrm.addSC("test-sender-receiver", "Enable IP MRM test sender and receiver operation");
	intVlanC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	intVlanC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intVlanC.ip.mtu.addSC("<68-1000000>", "MTU (bytes)");
	intVlanC.ip.addSC("multicast", "IP multicast interface commands");
		intVlanC.ip.multicast.addSC("boundary", "Boundary for administratively scoped multicast addresses");
			intVlanC.ip.multicast.boundary.addSC("<1-99>", "Access-list number");
			intVlanC.ip.multicast.boundary.addSC("<1300-1999>", "<access-list> (expanded range)");
			intVlanC.ip.multicast.boundary.addSC("WORD", "IP Named Standard Access list");
		intVlanC.ip.multicast.addSC("helper-map", "Broadcast to Multicast map OR Multicast to Broadcast map");
			intVlanC.ip.multicast["helper-map"].addSC("A.B.C.D", "IP multicast address");
				intVlanC.ip.multicast["helper-map"]["A.B.C.D"].addSC("A.B.C.D", "IP multicast address or IP broadcast address");
			intVlanC.ip.multicast["helper-map"].addSC("broadcast", "Broadcast address");
				intVlanC.ip.multicast["helper-map"].broadcast.addSC("A.B.C.D", "IP multicast address or IP broadcast address");
		intVlanC.ip.multicast.addSC("rate-limit", "Rate limit multicast data packets");
			intVlanC.ip.multicast["rate-limit"].addSC("in", "Rate limit incoming packets");

	intVlanC.ip.addSC("ospf", "OSPF interface commands");
		intVlanC.ip.ospf.addSC("authentication", "Enable authentication");
			intVlanC.ip.ospf.authentication.addSC("message-digest", "Use message-digest authentication");
			intVlanC.ip.ospf.authentication.addSC("null", "Use no authentication");
		intVlanC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
			intVlanC.ip.ospf["authentication-key"].addSC("<0-7>", "Encryption type (0 for not yet encrypted, 7 for proprietary)");
			intVlanC.ip.ospf["authentication-key"].addSC("LINE", "The OSPF password (key)");
		intVlanC.ip.ospf.addSC("cost", "Interface cost");
			intVlanC.ip.ospf.cost.addSC("<1-65535>", "Cost");
		intVlanC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
			intVlanC.ip.ospf["database-filter"].addSC("all", "Filter all LSA");
				intVlanC.ip.ospf["database-filter"].all.addSC("out", "Outgoing LSA");
		intVlanC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			intVlanC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		intVlanC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		intVlanC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			intVlanC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		intVlanC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
			intVlanC.ip.ospf["message-digest-key"].addSC("<1-255>", "Key ID");
				intVlanC.ip.ospf["message-digest-key"]["<1-255>"].addSC("md5", "Use MD5 algorithm");
		intVlanC.ip.ospf.addSC("mtu-ignore", "Ignores the MTU in DBD packets");
		intVlanC.ip.ospf.addSC("network", "Network type");
			intVlanC.ip.ospf.network.addSC("broadcast", "Specify OSPF broadcast multi-access network");
			intVlanC.ip.ospf.network.addSC("non-broadcast", "Specify OSPF NBMA network");
			intVlanC.ip.ospf.network.addSC("point-to-multipoint", "Specify OSPF point-to-multipoint network");
				intVlanC.ip.ospf.network["point-to-multipoint"].addSC("non-broadcast", "Specify non-broadcast point-to-mpoint network");
			intVlanC.ip.ospf.network.addSC("point-to-point", "Specify OSPF point-to-point network");
		intVlanC.ip.ospf.addSC("priority", "Router priority");
			intVlanC.ip.ospf.priority.addSC("<0-255>", "Priority");
		intVlanC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
			intVlanC.ip.ospf["retransmit-interval"].addSC("<1-65535>", "Seconds");
		intVlanC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
			intVlanC.ip.ospf["transmit-delay"].addSC("<1-65535>", "Seconds");
	intVlanC.ip.addSC("pim", "PIM interface commands");
		intVlanC.ip.pim.addSC("bsr-border", "Border of PIM domain");
		intVlanC.ip.pim.addSC("dense-mode", "Enable PIM dense-mode operation");
			intVlanC.ip.pim["dense-mode"].addSC("proxy-register", "Send proxy registers");
				intVlanC.ip.pim["dense-mode"]["proxy-register"].addSC("list", "Access list");
				intVlanC.ip.pim["dense-mode"]["proxy-register"].addSC("route-map", "Route-map");
		intVlanC.ip.pim.addSC("nbma-mode", "Use Non-Broadcast Multi-Access (NBMA) mode on interface");
		intVlanC.ip.pim.addSC("neighbor-filter", "PIM peering filter");
			intVlanC.ip.pim["neighbor-filter"].addSC("<1-99>", "Access list number");
			intVlanC.ip.pim["neighbor-filter"].addSC("WORD", "IP Named Standard Access list");
		intVlanC.ip.pim.addSC("query-interval", "PIM router query interval");
			intVlanC.ip.pim["query-interval"].addSC("<0-65535>", "Query interval in seconds");
		intVlanC.ip.pim.addSC("sparse-dense-mode", "Enable PIM sparse-dense-mode operation");
		intVlanC.ip.pim.addSC("sparse-mode", "Enable PIM sparse-mode operation");
		intVlanC.ip.pim.addSC("version", "PIM version");
			intVlanC.ip.pim.version.addSC("<1-2>", "version number");
	intVlanC.ip.addSC("probe", "Enable HP Probe support");
		intVlanC.ip.probe.addSC("proxy", "Proxy support");
	intVlanC.ip.addSC("proxy-arp", "Enable proxy ARP");
	intVlanC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intVlanC.ip["rarp-server"].addSC("A.B.C.D", "IP server address");
	intVlanC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");

	intVlanC.ip.addSC("rip", "Router Information Protocol");
		intVlanC.ip.rip.addSC("authentication", "Authentication control");
			intVlanC.ip.rip.authentication.addSC("key-chain", "Authentication key-chain");
				intVlanC.ip.rip.authentication["key-chain"].addSC("LINE", "name of key-chain");
			intVlanC.ip.rip.authentication.addSC("mode", "Authentication mode");
				intVlanC.ip.rip.authentication.mode.addSC("md5", "Keyed message digest");
				intVlanC.ip.rip.authentication.mode.addSC("text", "Clear text authentication");
		intVlanC.ip.rip.addSC("receive", "advertisement reception");
			intVlanC.ip.rip.receive.addSC("version", "version control");
				intVlanC.ip.rip.receive.version.addSC("<1-1>", "RIP version 1");
				intVlanC.ip.rip.receive.version.addSC("<2-2>", "RIP version 2");
		intVlanC.ip.rip.addSC("send", "advertisement transmission");
			intVlanC.ip.rip.send.addSC("version", "version control");
				intVlanC.ip.rip.send.version.addSC("<1-1>", "RIP version 1");
				intVlanC.ip.rip.send.version.addSC("<2-2>", "RIP version 2");
		intVlanC.ip.rip.addSC("v2-broadcast", "send ip broadcast v2 update");
	intVlanC.ip.addSC("sap", "Session Advertisement Protocol interface commands");
		intVlanC.ip.sap.addSC("listen", "Listen for sap packets on interface");
	intVlanC.ip.addSC("split-horizon", "Perform split horizon");
		intVlanC.ip["split-horizon"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intVlanC.ip["split-horizon"].eigrp.addSC("<1-65535>", "Autonomous system number");
	intVlanC.ip.addSC("summary-address", "Perform address summarization");
		intVlanC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intVlanC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intVlanC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
		intVlanC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
			intVlanC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
				intVlanC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");




intVlanC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intVlanC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intVlanC.addSC("logging", "Configure logging for interface");
	intVlanC.logging.addSC("event", "Interface events");
		intVlanC.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
intVlanC.addSC("loopback", "Configure internal loopback on an interface");
intVlanC.addSC("mac-address", "Manually set interface MAC address");
	intVlanC["mac-address"].addSC("H.H.H", "MAC address");
intVlanC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intVlanC["max-reserved-bandwidth"].addSC("<1-100>", "Max. reservable bandwidth as % of interface bandwidth");
intVlanC.addSC("mls", "Configure MultiLayer Switching characteristics");
intVlanC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intVlanC.mtu.addSC("<64-2025>", "MTU size in bytes");
intVlanC.addSC("no", "Negate a command or set its defaults");
	intVlanC.no.addSC("access-expression", "Build a bridge boolean access expression");
		intVlanC.no["access-expression"].addSC("input", "Filter input packets");
		intVlanC.no["access-expression"].addSC("output", "Filter output packets");
	intVlanC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intVlanC.no.arp.addSC("arpa", "Standard arp protocol");
		intVlanC.no.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		intVlanC.no.arp.addSC("probe", "HP style arp protocol");
		intVlanC.no.arp.addSC("snap", "IEEE 802.3 style arp");
		intVlanC.no.arp.addSC("timeout", "Set ARP cache timeout");
	intVlanC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intVlanC.no.addSC("bridge-group", "Transparent bridging interface parameters");
		intVlanC.no["bridge-group"].addSC("<1-255>", "Assign an interface to a Bridge Group.");
	intVlanC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intVlanC.no.addSC("cdp", "CDP interface subcommands");
		intVlanC.no.cdp.addSC("enable", "Enable CDP on interface");
	intVlanC.no.addSC("custom-queue-list", "Assign a custom queue list to an interface");
	intVlanC.no.addSC("delay", "Specify interface throughput delay");
	intVlanC.no.addSC("description", "Interface specific description");
	intVlanC.no.addSC("fair-queue", "Enable Fair Queuing on an Interface");
		intVlanC.no["fair-queue"].addSC("<1-4096>", "Congestive Discard Threshold");
	intVlanC.no.addSC("hold-queue", "Set hold queue depth");
		intVlanC.no["hold-queue"].addSC("<0-4096>", "Queue length");
		intVlanC.no["hold-queue"].addSC("in", "Input queue");
		intVlanC.no["hold-queue"].addSC("out", "Output queue");
	intVlanC.no.addSC("ip", "Interface Internet Protocol config commands");
		intVlanC.no.ip.addSC("access-group", "Specify access control for packets");
			intVlanC.no.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intVlanC.no.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
		intVlanC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
			intVlanC.no.ip.accounting.addSC("access-violations", "Account for IP packets violating access lists on this interface");
		intVlanC.no.ip.addSC("address", "Set the IP address of an interface");
			intVlanC.no.ip.address.addSC("A.B.C.D", "IP address");
				intVlanC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
		intVlanC.no.ip.addSC("authentication", "authentication subcommands");
			intVlanC.no.ip.authentication.addSC("key-chain", "key-chain");
				intVlanC.no.ip.authentication["key-chain"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intVlanC.no.ip.authentication.addSC("mode", "mode");
				intVlanC.no.ip.authentication.mode.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		intVlanC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			intVlanC.no.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.no.ip["bandwidth-percent"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intVlanC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intVlanC.no.ip.addSC("cef", "Cisco Express Fowarding interface commands");
			intVlanC.no.ip.cef.addSC("accounting", "CEF accounting features for interface");
				intVlanC.no.ip.cef.accounting.addSC("non-recursive", "CEF non-recursive accounting features");
		intVlanC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		intVlanC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intVlanC.no.ip.addSC("dvmrp", "DVMRP interface commands");
			intVlanC.no.ip.dvmrp.addSC("accept-filter", "DVMRP incoming Report filters");
		intVlanC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
			intVlanC.no.ip["hello-interval"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.no.ip["hello-interval"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intVlanC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
			intVlanC.no.ip["helper-address"].addSC("A.B.C.D", "IP destination address");
		intVlanC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
			intVlanC.no.ip["hold-time"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.no.ip["hold-time"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intVlanC.no.ip.addSC("igmp", "IGMP interface commands");
			intVlanC.no.ip.igmp.addSC("access-group", "IGMP group access group");
			intVlanC.no.ip.addSC("load-sharing", "Style of load sharing");
			intVlanC.no.ip["load-sharing"].addSC("per-packet", "Random distribution");
		intVlanC.no.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
		intVlanC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		intVlanC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		intVlanC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		intVlanC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intVlanC.no.ip.addSC("multicast", "IP multicast interface commands");
			intVlanC.no.ip.multicast.addSC("boundary", "Boundary for administratively scoped multicast addresses");
			intVlanC.no.ip.multicast.addSC("helper-map", "Broadcast to Multicast map OR Multicast to Broadcast map");
		intVlanC.no.ip.addSC("ospf", "OSPF interface commands");
			intVlanC.no.ip.ospf.addSC("authentication", "Enable authentication");
			intVlanC.no.ip.ospf.addSC("authentication-key", "Authentication password (key)");
			intVlanC.no.ip.ospf.addSC("cost", "Interface cost");
			intVlanC.no.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
			intVlanC.no.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
		intVlanC.no.ip.addSC("pim", "PIM interface commands");
			intVlanC.no.ip.pim.addSC("bsr-border", "Border of PIM domain");
			intVlanC.no.ip.pim.addSC("dense-mode", "Enable PIM dense-mode operation");
		intVlanC.no.ip.addSC("probe", "Enable HP Probe support");
			intVlanC.no.ip.probe.addSC("proxy", "Proxy support");
		intVlanC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		intVlanC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intVlanC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		intVlanC.no.ip.addSC("rgmp", "Enable/disable RGMP");
		intVlanC.no.ip.addSC("rip", "Router Information Protocol");
			intVlanC.no.ip.rip.addSC("authentication", "Authentication control");
				intVlanC.no.ip.rip.authentication.addSC("key-chain", "Authentication key-chain");
				intVlanC.no.ip.rip.authentication.addSC("mode", "Authentication mode");
			intVlanC.no.ip.rip.addSC("receive", "advertisement reception");
		intVlanC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
			intVlanC.no.ip["route-cache"].addSC("cef", "Enable Cisco Express Forwarding");
			intVlanC.no.ip["route-cache"].addSC("flow", "Enable Flow fast-switching cache");
			intVlanC.no.ip["route-cache"].addSC("policy", "Enable fast-switching policy cache for outgoing packets");
			intVlanC.no.ip["route-cache"].addSC("same-interface", "Enable fast-switching on the same interface");
		intVlanC.no.ip.addSC("sap", "Session Advertisement Protocol interface commands");
			intVlanC.no.ip.sap.addSC("listen", "Listen for sap packets on interface");
		intVlanC.no.ip.addSC("sdr", "Session Directory Protocol interface commands");
			intVlanC.no.ip.sdr.addSC("listen", "Listen for sap packets on interface");
		intVlanC.no.ip.addSC("security", "DDN IP Security Option");
			intVlanC.no.ip.security.addSC("add", "Ensure all outgoing packets have a basic security option");
			intVlanC.no.ip.security.addSC("aeso", "Specify AESO sources");
		intVlanC.no.ip.addSC("split-horizon", "Perform split horizon");
			intVlanC.no.ip["split-horizon"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.no.ip["split-horizon"].eigrp.addSC("<1-65535>", "Autonomous system number");
		intVlanC.no.ip.addSC("summary-address", "Perform address summarization");
			intVlanC.no.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intVlanC.no.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
			intVlanC.no.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
				intVlanC.no.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
		intVlanC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intVlanC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		intVlanC.no.ip.addSC("verify", "Enable per packet validation");
			intVlanC.no.ip.verify.addSC("unicast", "Enable per packet validation for unicast");
				intVlanC.no.ip.verify.unicast.addSC("reverse-path", "Reverse path validation of source address");
	intVlanC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intVlanC.no.addSC("logging", "Configure logging for interface");
		intVlanC.no.logging.addSC("event", "Interface events");
			intVlanC.no.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
	intVlanC.no.addSC("loopback", "Configure internal loopback on an interface");
	intVlanC.no.addSC("mac-address", "Manually set interface MAC address");
	intVlanC.no.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
		intVlanC.no["max-reserved-bandwidth"].addSC("<1-100>", "Max. reservable bandwidth as % of interface bandwidth");
	intVlanC.no.addSC("mls", "Configure MultiLayer Switching characteristics");
	intVlanC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");

	intVlanC.no.addSC("shutdown", "Shutdown the selected interface");

intVlanC.addSC("ntp", "Configure NTP");


intVlanC.addSC("priority-group", "Assign a priority group to an interface");
	intVlanC["priority-group"].addSC("<1-16>", "Priority group");

intVlanC.addSC("random-detect", "Enable Weighted Random Early Detection (WRED) on an Interface");
intVlanC.addSC("rmon", "Configure Remote Monitoring on an interface");
	intVlanC.rmon.addSC("collection", "Configure Remote Monitoring Collection on an interface");
		intVlanC.rmon.collection.addSC("history", "Configure history");
			intVlanC.rmon.collection.history.addSC("<1-65535>", "Set RMON collection control index");
				intVlanC.rmon.collection.history["<1-65535>"].addSC("buckets", "Requested buckets of intervals. Default is 50 buckets");
				intVlanC.rmon.collection.history["<1-65535>"].addSC("interval", "Interval to sample data for each bucket. Default is 1800 seconds");
				intVlanC.rmon.collection.history["<1-65535>"].addSC("owner", "Set the owner of this RMON collection");
		intVlanC.rmon.collection.addSC("stats", "Configure statistics");
			intVlanC.rmon.collection.stats.addSC("<1-65535>", "Set RMON collection control index");
				intVlanC.rmon.collection.stats["<1-65535>"].addSC("owner", "Configure the owner of this RMON collection");
	intVlanC.rmon.addSC("native", "Monitor the interface in native mode");
	intVlanC.rmon.addSC("promiscuous", "Monitor the interface in promiscuous mode");
intVlanC.addSC("service-policy", "Configure QoS Service Policy");
	intVlanC["service-policy"].addSC("history", "Keep history of QoS metrics");
	intVlanC["service-policy"].addSC("input", "Assign policy-map to the input of an interface");
		intVlanC["service-policy"].input.addSC("WORD", "policy-map name");
	intVlanC["service-policy"].addSC("output", "Assign policy-map to the output of an interface");
		intVlanC["service-policy"].output.addSC("WORD", "policy-map name");


intVlanC.addSC("shutdown", "Shutdown the selected interface");
intVlanC.addSC("snmp", "Modify SNMP interface parameters");
	intVlanC.snmp.addSC("trap", "Allow a specific SNMP trap");
		intVlanC.snmp.trap.addSC("link-status", "Allow SNMP LINKUP and LINKDOWN traps");
intVlanC.addSC("spanning-tree", "Spanning Tree Subsystem");
	intVlanC["spanning-tree"].addSC("cost", "Change an interface's spanning tree port path cost");
		intVlanC["spanning-tree"].cost.addSC("<1-200000000>", "port path cost");
	intVlanC["spanning-tree"].addSC("guard", "Change an interface's spanning tree guard mode");
		intVlanC["spanning-tree"].guard.addSC("none", "Set guard mode to none");
		intVlanC["spanning-tree"].guard.addSC("root", "Set guard mode to root guard on interface");
	intVlanC["spanning-tree"].addSC("port-priority", "Change an interface's spanning tree port priority");
		intVlanC["spanning-tree"]["port-priority"].addSC("<0-255>", "port priority");
	intVlanC["spanning-tree"].addSC("portfast", "Enable an interface to move directly to forwarding on link up");
	intVlanC["spanning-tree"].addSC("stack-port", "Enable stack port");

intVlanC.addSC("standby", "Hot standby interface subcommands");
	intVlanC.standby.addSC("<0-255>", "group number");
	intVlanC.standby.addSC("authentication", "Authentication string");
		intVlanC.standby.authentication.addSC("WORD", "authentication string");
	intVlanC.standby.addSC("ip", "Enable hot standby protocol for IP");
		intVlanC.standby.ip.addSC("A.B.C.D", "Hot standby IP address");
			intVlanC.standby.ip["A.B.C.D"].addSC("secondary", "Specify an additional Hot standby IP address");
	intVlanC.standby.addSC("mac-address", "Specify virtual MAC address for the virtual router");
		intVlanC.standby["mac-address"].addSC("H.H.H", "Standby MAC address");
	intVlanC.standby.addSC("mac-refresh", "Refresh MAC cache on switch by periodically sendingpacket from virtual mac address");
		intVlanC.standby["mac-refresh"].addSC("<0-255>", "Interval to refresh MAC cache");
	intVlanC.standby.addSC("name", "Name string");
		intVlanC.standby.name.addSC("WORD", "name string");

intVlanC.addSC("timeout", "Define timeout values for this interface");
	intVlanC.timeout.addSC("absolute", "Define session timeout value for this interface");
		intVlanC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
			intVlanC.timeout.absolute["<0-35790>"].addSC("<0-59>", "Session lifetime (in seconds)");
