
routerOSPFC.addSC("area", "OSPF area parameters");
	routerOSPFC.area.addSC("<0-4294967295>", "OSPF area ID as a decimal value");
		routerOSPFC.area["<0-4294967295>"].addSC("authentication", "Enable authentication");
			routerOSPFC.area["<0-4294967295>"].authentication.addSC("message-digest", "Use message-digest authentication");
		routerOSPFC.area["<0-4294967295>"].addSC("default-cost", "Set the summary default-cost of a NSSA/stub area");
			routerOSPFC.area["<0-4294967295>"]["default-cost"].addSC("<0-16777215>", "Stub's advertised external route metric");
		routerOSPFC.area["<0-4294967295>"].addSC("filter-list", "Filter networks between OSPF areas");
			routerOSPFC.area["<0-4294967295>"]["filter-list"].addSC("prefix", "Filter prefixes between OSPF areas");
				routerOSPFC.area["<0-4294967295>"]["filter-list"].prefix.addSC("WORD", "Name of an IP prefix-list");

		routerOSPFC.area["<0-4294967295>"].addSC("nssa", "Specify a NSSA area");
			routerOSPFC.area["<0-4294967295>"].nssa.addSC("default-information-originate", "Originate Type 7 default into NSSA area");
				routerOSPFC.area["<0-4294967295>"].nssa["default-information-originate"].addSC("metric", "OSPF default metric");
					routerOSPFC.area["<0-4294967295>"].nssa["default-information-originate"].metric.addSC("<0-16777214>", "OSPF metric");
				routerOSPFC.area["<0-4294967295>"].nssa["default-information-originate"].addSC("metric-type", "OSPF metric type for default routes");
					routerOSPFC.area["<0-4294967295>"].nssa["default-information-originate"]["metric-type"].addSC("<1-2>", "OSPF Link State type");
			routerOSPFC.area["<0-4294967295>"].nssa.addSC("no-redistribution", "No redistribution into this NSSA area");
				routerOSPFC.area["<0-4294967295>"].nssa["no-redistribution"].addSC("default-information-originate", "Originate Type 7 default into NSSA area");

			routerOSPFC.area["<0-4294967295>"].nssa.addSC("no-summary", "Do not send summary LSA into NSSA");
		routerOSPFC.area["<0-4294967295>"].addSC("range", "Summarize routes matching address/mask (border routers only)");
			routerOSPFC.area["<0-4294967295>"].range.addSC("A.B.C.D", "IP address to match");
				routerOSPFC.area["<0-4294967295>"].range["A.B.C.D"].addSC("A.B.C.D", "IP mask for address");

		routerOSPFC.area["<0-4294967295>"].addSC("stub", "Specify a stub area");
			routerOSPFC.area["<0-4294967295>"].stub.addSC("no-summary", "Do not send summary LSA into stub area");
		routerOSPFC.area["<0-4294967295>"].addSC("virtual-link", "Define a virtual link and its parameters");
			routerOSPFC.area["<0-4294967295>"]["virtual-link"].addSC("A.B.C.D", "ID (IP addr) associated with virtual link neighbor");

	routerOSPFC.area.addSC("A.B.C.D", "OSPF area ID in IP address format");
		routerOSPFC.area["A.B.C.D"].addSC("authentication", "Enable authentication");
			routerOSPFC.area["A.B.C.D"].authentication.addSC("message-digest", "Use message-digest authentication");
		routerOSPFC.area["A.B.C.D"].addSC("default-cost", "Set the summary default-cost of a NSSA/stub area");
			routerOSPFC.area["A.B.C.D"]["default-cost"].addSC("<0-16777215>", "Stub's advertised external route metric");
		routerOSPFC.area["A.B.C.D"].addSC("filter-list", "Filter networks between OSPF areas");
			routerOSPFC.area["A.B.C.D"]["filter-list"].addSC("prefix", "Filter prefixes between OSPF areas");
				routerOSPFC.area["A.B.C.D"]["filter-list"].prefix.addSC("WORD", "Name of an IP prefix-list");
					routerOSPFC.area["A.B.C.D"]["filter-list"].prefix.WORD.addSC("in", "Filter networks sent to this area");
					routerOSPFC.area["A.B.C.D"]["filter-list"].prefix.WORD.addSC("out", "Filter networks sent from this area");
		routerOSPFC.area["A.B.C.D"].addSC("nssa", "Specify a NSSA area");

		routerOSPFC.area["A.B.C.D"].addSC("range", "Summarize routes matching address/mask (border routers only)");

		routerOSPFC.area["A.B.C.D"].addSC("stub", "Specify a stub area");
			routerOSPFC.area["A.B.C.D"].stub.addSC("no-summary", "Do not send summary LSA into stub area");
		routerOSPFC.area["A.B.C.D"].addSC("virtual-link", "Define a virtual link and its parameters");
			routerOSPFC.area["A.B.C.D"]["virtual-link"].addSC("A.B.C.D", "ID (IP addr) associated with virtual link neighbor");

routerOSPFC.addSC("auto-cost", "Calculate OSPF interface cost according to bandwidth");
	routerOSPFC["auto-cost"].addSC("reference-bandwidth", "Use reference bandwidth method to assign OSPF cost");
		routerOSPFC["auto-cost"]["reference-bandwidth"].addSC("<1-4294967>", "The reference bandwidth in terms of Mbits per second");
routerOSPFC.addSC("capability", "Enable specific OSPF feature");
	routerOSPFC.capability.addSC("opaque", "Opaque LSA");
routerOSPFC.addSC("compatible", "OSPF compatibility list");
	routerOSPFC.compatible.addSC("rfc1583", "compatible with RFC 1583");
routerOSPFC.addSC("default", "Set a command to its defaults");
	routerOSPFC["default"].addSC("area", "OSPF area parameters");
		routerOSPFC["default"].area.addSC("<0-4294967295>", "OSPF area ID as a decimal value");
		routerOSPFC["default"].area.addSC("A.B.C.D", "OSPF area ID in IP address format");
	routerOSPFC["default"].addSC("auto-cost", "Calculate OSPF interface cost according to bandwidth");
		routerOSPFC["default"]["auto-cost"].addSC("reference-bandwidth", "Use reference bandwidth method to assign OSPF cost");
	routerOSPFC["default"].addSC("capability", "Enable specific OSPF feature");
		routerOSPFC["default"].capability.addSC("opaque", "Opaque LSA");
	routerOSPFC["default"].addSC("compatible", "OSPF compatibility list");
		routerOSPFC["default"].compatible.addSC("rfc1583", "compatible with RFC 1583");
routerOSPFC.addSC("default-information", "Control distribution of default information");
	routerOSPFC["default-information"].addSC("originate", "Distribute a default route");
		routerOSPFC["default-information"].originate.addSC("always", "Always advertise default route");
		routerOSPFC["default-information"].originate.addSC("metric", "OSPF default metric");
			routerOSPFC["default-information"].originate.metric.addSC("<0-16777214>", "OSPF metric");
				routerOSPFC["default-information"].originate.metric["<0-16777214>"].addSC("always", "Always advertise default route");
		routerOSPFC["default-information"].originate.addSC("metric-type", "OSPF metric type for default routes");
			routerOSPFC["default-information"].originate["metric-type"].addSC("<1-2>", "OSPF Link State type");

		routerOSPFC["default-information"].originate.addSC("route-map", "Route-map reference");
			routerOSPFC["default-information"].originate["route-map"].addSC("WORD", "Route map name");

routerOSPFC.addSC("default-metric", "Set metric of redistributed routes");
	routerOSPFC["default-metric"].addSC("<1-4294967295>", "Default metric");
routerOSPFC.addSC("discard-route", "Enable or disable discard-route installation");
	routerOSPFC["discard-route"].addSC("external", "Discard route for redistributed summarised routes");
	routerOSPFC["discard-route"].addSC("internal", "Discard route for summarised internal routes");
routerOSPFC.addSC("distance", "Define an administrative distance");
	routerOSPFC.distance.addSC("<1-255>", "Administrative distance");
		routerOSPFC.distance["<1-255>"].addSC("A.B.C.D", "IP Source address");
			routerOSPFC.distance["<1-255>"]["A.B.C.D"].addSC("A.B.C.D", "IP address mask");
				routerOSPFC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-99>", "IP Standard access list number");
				routerOSPFC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1300-1999>", "IP Standard expanded access list number");
	routerOSPFC.distance.addSC("ospf", "OSPF distance");
		routerOSPFC.distance.ospf.addSC("external", "External type 5 and type 7 routes");
			routerOSPFC.distance.ospf.external.addSC("<1-255>", "Distance for external type 5 and type 7 routes");
		routerOSPFC.distance.ospf.addSC("inter-area", "Inter-area routes");
			routerOSPFC.distance.ospf["inter-area"].addSC("<1-255>", "Distance for inter-area routes");
				routerOSPFC.distance.ospf["inter-area"]["<1-255>"].addSC("external", "External type 5 and type 7 routes");
					routerOSPFC.distance.ospf["inter-area"]["<1-255>"].external.addSC("<1-255>", "Distance for external type 5 and type 7 routes");
		routerOSPFC.distance.ospf.addSC("intra-area", "Intra-area routes");
			routerOSPFC.distance.ospf["intra-area"].addSC("<1-255>", "Distance for intra-area routes");

routerOSPFC.addSC("distribute-list", "Filter networks in routing updates");
	routerOSPFC["distribute-list"].addSC("<1-199>", "IP access list number");
		routerOSPFC["distribute-list"]["<1-199>"].addSC("in", "Filter incoming routing updates");
			routerOSPFC["distribute-list"]["<1-199>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerOSPFC["distribute-list"]["<1-199>"]["in"].GigabitEthernet.addSC("<0-2>", "GigabitEthernet interface number");
			routerOSPFC["distribute-list"]["<1-199>"]["in"].addSC("Null", "Null interface");
				routerOSPFC["distribute-list"]["<1-199>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerOSPFC["distribute-list"]["<1-199>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerOSPFC["distribute-list"]["<1-199>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerOSPFC["distribute-list"]["<1-199>"].addSC("out", "Filter outgoing routing updates");

	routerOSPFC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
		routerOSPFC["distribute-list"]["<1300-2699>"].addSC("in", "Filter incoming routing updates");


		routerOSPFC["distribute-list"]["<1300-2699>"].addSC("out", "Filter outgoing routing updates");

	routerOSPFC["distribute-list"].addSC("WORD", "Access-list name");
		routerOSPFC["distribute-list"].WORD.addSC("in", "Filter incoming routing updates");

		routerOSPFC["distribute-list"].WORD.addSC("out", "Filter outgoing routing updates");

	routerOSPFC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
		routerOSPFC["distribute-list"].gateway.addSC("WORD", "Name of an IP prefix-list");
			routerOSPFC["distribute-list"].gateway.WORD.addSC("in", "Filter incoming routing updates");

			routerOSPFC["distribute-list"].gateway.WORD.addSC("out", "Filter outgoing routing updates");

	routerOSPFC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
		routerOSPFC["distribute-list"].prefix.addSC("WORD", "Name of an IP prefix-list");
			routerOSPFC["distribute-list"].prefix.WORD.addSC("gateway", "Filtering incoming updates based on gateway");
			routerOSPFC["distribute-list"].prefix.WORD.addSC("in", "Filter incoming routing updates");

			routerOSPFC["distribute-list"].prefix.WORD.addSC("out", "Filter outgoing routing updates");

routerOSPFC.addSC("domain-id", "OSPF domain-id");
	routerOSPFC["domain-id"].addSC("A.B.C.D", "OSPF domain ID in IP address format");
routerOSPFC.addSC("domain-tag", "OSPF domain-tag");
	routerOSPFC["domain-tag"].addSC("<0-4294967295>", "OSPF domain tag - 32-bit value");
routerOSPFC.addSC("exit", "Exit from routing protocol configuration mode");
routerOSPFC.addSC("help", "Description of the interactive help system");
routerOSPFC.addSC("ignore", "Do not complain about specific event");
	routerOSPFC.ignore.addSC("lsa", "Do not complain upon receiving LSA of the specified type");
		routerOSPFC.ignore.lsa.addSC("mospf", "MOSPF Type 6 LSA");
routerOSPFC.addSC("log-adjacency-changes", "Log changes in adjacency state");
	routerOSPFC["log-adjacency-changes"].addSC("detail", "Log all state changes");
routerOSPFC.addSC("max-metric", "Set maximum metric");
	routerOSPFC["max-metric"].addSC("router-lsa", "Maximum metric in self-originated router-LSAs");
		routerOSPFC["max-metric"]["router-lsa"].addSC("on-startup", "Set maximum metric temporarily after reboot");
routerOSPFC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerOSPFC["maximum-paths"].addSC("<1-6>", "Number of paths");
routerOSPFC.addSC("neighbor", "Specify a neighbor router");
	routerOSPFC.neighbor.addSC("A.B.C.D", "Neighbor address");
		routerOSPFC.neighbor["A.B.C.D"].addSC("cost", "OSPF cost for point-to-multipoint neighbor");
			routerOSPFC.neighbor["A.B.C.D"].cost.addSC("<1-65535>", "metric");
		routerOSPFC.neighbor["A.B.C.D"].addSC("database-filter", "Filter OSPF LSA during synchronization and flooding for point-to-multipoint neighbor");
			routerOSPFC.neighbor["A.B.C.D"]["database-filter"].addSC("all", "Filter all LSA");

		routerOSPFC.neighbor["A.B.C.D"].addSC("poll-interval", "OSPF dead-router polling interval");
			routerOSPFC.neighbor["A.B.C.D"]["poll-interval"].addSC("<0-4294967295>", "Seconds");
		routerOSPFC.neighbor["A.B.C.D"].addSC("priority", "OSPF priority of non-broadcast neighbor");
			routerOSPFC.neighbor["A.B.C.D"].priority.addSC("<0-255>", "Priority");
				routerOSPFC.neighbor["A.B.C.D"].priority["<0-255>"].addSC("poll-interval", "OSPF dead-router polling interval");
					routerOSPFC.neighbor["A.B.C.D"].priority["<0-255>"]["poll-interval"].addSC("<0-4294967295>", "Seconds");
routerOSPFC.addSC("network", "Enable routing on an IP network");
	routerOSPFC.network.addSC("A.B.C.D", "Network number");
		routerOSPFC.network["A.B.C.D"].addSC("A.B.C.D", "OSPF wild card bits");
			routerOSPFC.network["A.B.C.D"]["A.B.C.D"].addSC("area", "Set the OSPF area ID");
				routerOSPFC.network["A.B.C.D"]["A.B.C.D"].area.addSC("<0-4294967295>", "OSPF area ID as a decimal value");
				routerOSPFC.network["A.B.C.D"]["A.B.C.D"].area.addSC("A.B.C.D", "OSPF area ID in IP address format");
routerOSPFC.addSC("no", "Negate a command or set its defaults");
	routerOSPFC.no.addSC("area", "OSPF area parameters");
		routerOSPFC.no.area.addSC("<0-4294967295>", "OSPF area ID as a decimal value");
		routerOSPFC.no.area.addSC("A.B.C.D", "OSPF area ID in IP address format");
	routerOSPFC.no.addSC("auto-cost", "Calculate OSPF interface cost according to bandwidth");
		routerOSPFC.no["auto-cost"].addSC("reference-bandwidth", "Use reference bandwidth method to assign OSPF cost");
	routerOSPFC.no.addSC("capability", "Enable specific OSPF feature");
		routerOSPFC.no.capability.addSC("opaque", "Opaque LSA");
	routerOSPFC.no.addSC("compatible", "OSPF compatibility list");
		routerOSPFC.no.compatible.addSC("rfc1583", "compatible with RFC 1583");
	routerOSPFC.no.addSC("default-information", "Control distribution of default information");
		routerOSPFC.no["default-information"].addSC("originate", "Distribute a default route");
	routerOSPFC.no.addSC("default-metric", "Set metric of redistributed routes");
	routerOSPFC.no.addSC("discard-route", "Enable or disable discard-route installation");
		routerOSPFC.no["discard-route"].addSC("external", "Discard route for redistributed summarised routes");
		routerOSPFC.no["discard-route"].addSC("internal", "Discard route for summarised internal routes");
	routerOSPFC.no.addSC("distance", "Define an administrative distance");
		routerOSPFC.no.distance.addSC("<1-255>", "Administrative distance");
		routerOSPFC.no.distance.addSC("ospf", "OSPF distance");
	routerOSPFC.no.addSC("distribute-list", "Filter networks in routing updates");
		routerOSPFC.no["distribute-list"].addSC("<1-199>", "IP access list number");
		routerOSPFC.no["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
		routerOSPFC.no["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
		routerOSPFC.no["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
	routerOSPFC.no.addSC("domain-id", "OSPF domain-id");
	routerOSPFC.no.addSC("domain-tag", "OSPF domain-tag");
	routerOSPFC.no.addSC("ignore", "Do not complain about specific event");
		routerOSPFC.no.ignore.addSC("lsa", "Do not complain upon receiving LSA of the specified type");
	routerOSPFC.no.addSC("log-adjacency-changes", "Log changes in adjacency state");
		routerOSPFC.no["log-adjacency-changes"].addSC("detail", "Log all state changes");
	routerOSPFC.no.addSC("max-metric", "Set maximum metric");
		routerOSPFC.no["max-metric"].addSC("router-lsa", "Maximum metric in self-originated router-LSAs");
	routerOSPFC.no.addSC("maximum-paths", "Forward packets over multiple paths");
	routerOSPFC.no.addSC("neighbor", "Specify a neighbor router");
		routerOSPFC.no.neighbor.addSC("A.B.C.D", "Neighbor address");
	routerOSPFC.no.addSC("network", "Enable routing on an IP network");
		routerOSPFC.no.network.addSC("A.B.C.D", "Network number");
routerOSPFC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerOSPFC["passive-interface"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
		routerOSPFC["passive-interface"].GigabitEthernet.addSC("<0-2>", "GigabitEthernet interface number");
	routerOSPFC["passive-interface"].addSC("Null", "Null interface");
		routerOSPFC["passive-interface"].Null.addSC("<0-0>", "Null interface number");
	routerOSPFC["passive-interface"].addSC("Vlan", "Catalyst Vlans");
		routerOSPFC["passive-interface"].Vlan.addSC("<1-1001>", "Vlan interface number");
	routerOSPFC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerOSPFC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerOSPFC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
		routerOSPFC.redistribute.bgp.addSC("<1-65535>", "Autonomous system number");
	routerOSPFC.redistribute.addSC("connected", "Connected");
	routerOSPFC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
		routerOSPFC.redistribute.egp.addSC("<0-65535>", "Remote autonomous system number");
	routerOSPFC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		routerOSPFC.redistribute.eigrp.addSC("<1-65535>", "Autonomous system number");
	routerOSPFC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
		routerOSPFC.redistribute.igrp.addSC("<1-65535>", "Autonomous system number");
	routerOSPFC.redistribute.addSC("isis", "ISO IS-IS");
		routerOSPFC.redistribute.isis.addSC("level-1", "IS-IS level-1 routes only");
		routerOSPFC.redistribute.isis.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
		routerOSPFC.redistribute.isis.addSC("level-2", "IS-IS level-2 routes only");
		routerOSPFC.redistribute.isis.addSC("WORD", "ISO routing area tag");
			routerOSPFC.redistribute.isis.WORD.addSC("level-1", "IS-IS level-1 routes only");
			routerOSPFC.redistribute.isis.WORD.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
			routerOSPFC.redistribute.isis.WORD.addSC("level-2", "IS-IS level-2 routes only");
	routerOSPFC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
		routerOSPFC.redistribute["iso-igrp"].addSC("WORD", "ISO routing area tag");
	routerOSPFC.redistribute.addSC("metric", "Metric for redistributed routes");
		routerOSPFC.redistribute.metric.addSC("<0-16777214>", "OSPF default metric");
	routerOSPFC.redistribute.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
		routerOSPFC.redistribute["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

		routerOSPFC.redistribute["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("mobile", "Mobile routes");
		routerOSPFC.redistribute.mobile.addSC("metric", "Metric for redistributed routes");
			routerOSPFC.redistribute.mobile.metric.addSC("<0-16777214>", "OSPF default metric");
		routerOSPFC.redistribute.mobile.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
			routerOSPFC.redistribute.mobile["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

			routerOSPFC.redistribute.mobile["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("odr", "On Demand stub Routes");
		routerOSPFC.redistribute.odr.addSC("metric", "Metric for redistributed routes");
			routerOSPFC.redistribute.odr.metric.addSC("<0-16777214>", "OSPF default metric");
		routerOSPFC.redistribute.odr.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
			routerOSPFC.redistribute.odr["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

			routerOSPFC.redistribute.odr["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
		routerOSPFC.redistribute.ospf.addSC("<1-65535>", "Process ID");
			routerOSPFC.redistribute.ospf["<1-65535>"].addSC("match", "Redistribution of OSPF routes");

			routerOSPFC.redistribute.ospf["<1-65535>"].addSC("metric", "Metric for redistributed routes");

			routerOSPFC.redistribute.ospf["<1-65535>"].addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");

			routerOSPFC.redistribute.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
				routerOSPFC.redistribute.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");


	routerOSPFC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
		routerOSPFC.redistribute.rip.addSC("metric", "Metric for redistributed routes");
			routerOSPFC.redistribute.rip.metric.addSC("<0-16777214>", "OSPF default metric");
		routerOSPFC.redistribute.rip.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
			routerOSPFC.redistribute.rip["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

			routerOSPFC.redistribute.rip["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("route-map", "Route map reference");
		routerOSPFC.redistribute["route-map"].addSC("WORD", "Pointer to route-map entries");
			routerOSPFC.redistribute["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
				routerOSPFC.redistribute["route-map"].WORD.metric.addSC("<0-16777214>", "OSPF default metric");
			routerOSPFC.redistribute["route-map"].WORD.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
				routerOSPFC.redistribute["route-map"].WORD["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

				routerOSPFC.redistribute["route-map"].WORD["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("static", "Static routes");
		routerOSPFC.redistribute.static.addSC("metric", "Metric for redistributed routes");
			routerOSPFC.redistribute.static.metric.addSC("<0-16777214>", "OSPF default metric");
		routerOSPFC.redistribute.static.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
			routerOSPFC.redistribute.static["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

			routerOSPFC.redistribute.static["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

		routerOSPFC.redistribute.static.addSC("route-map", "Route map reference");
			routerOSPFC.redistribute.static["route-map"].addSC("WORD", "Pointer to route-map entries");
				routerOSPFC.redistribute.static["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
					routerOSPFC.redistribute.static["route-map"].WORD.metric.addSC("<0-16777214>", "OSPF default metric");
				routerOSPFC.redistribute.static["route-map"].WORD.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
					routerOSPFC.redistribute.static["route-map"].WORD["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

					routerOSPFC.redistribute.static["route-map"].WORD["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("subnets", "Consider subnets for redistribution into OSPF");
		routerOSPFC.redistribute.subnets.addSC("metric", "Metric for redistributed routes");
			routerOSPFC.redistribute.subnets.metric.addSC("<0-16777214>", "OSPF default metric");
		routerOSPFC.redistribute.subnets.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
			routerOSPFC.redistribute.subnets["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

			routerOSPFC.redistribute.subnets["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

		routerOSPFC.redistribute.subnets.addSC("route-map", "Route map reference");
			routerOSPFC.redistribute.subnets["route-map"].addSC("WORD", "Pointer to route-map entries");
				routerOSPFC.redistribute.subnets["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
					routerOSPFC.redistribute.subnets["route-map"].WORD.metric.addSC("<0-16777214>", "OSPF default metric");
				routerOSPFC.redistribute.subnets["route-map"].WORD.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
					routerOSPFC.redistribute.subnets["route-map"].WORD["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

					routerOSPFC.redistribute.subnets["route-map"].WORD["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

	routerOSPFC.redistribute.addSC("tag", "Set tag for routes redistributed into OSPF");
		routerOSPFC.redistribute.tag.addSC("<0-4294967295>", "32-bit tag value");
			routerOSPFC.redistribute.tag["<0-4294967295>"].addSC("metric", "Metric for redistributed routes");
				routerOSPFC.redistribute.tag["<0-4294967295>"].metric.addSC("<0-16777214>", "OSPF default metric");
			routerOSPFC.redistribute.tag["<0-4294967295>"].addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");
				routerOSPFC.redistribute.tag["<0-4294967295>"]["metric-type"].addSC("<1-1>", "Set OSPF External Type 1 metrics");

				routerOSPFC.redistribute.tag["<0-4294967295>"]["metric-type"].addSC("<2-2>", "Set OSPF External Type 2 metrics");

			routerOSPFC.redistribute.tag["<0-4294967295>"].addSC("route-map", "Route map reference");
				routerOSPFC.redistribute.tag["<0-4294967295>"]["route-map"].addSC("WORD", "Pointer to route-map entries");
					routerOSPFC.redistribute.tag["<0-4294967295>"]["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
						routerOSPFC.redistribute.tag["<0-4294967295>"]["route-map"].WORD.metric.addSC("<0-16777214>", "OSPF default metric");
					routerOSPFC.redistribute.tag["<0-4294967295>"]["route-map"].WORD.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");

			routerOSPFC.redistribute.tag["<0-4294967295>"].addSC("subnets", "Consider subnets for redistribution into OSPF");
				routerOSPFC.redistribute.tag["<0-4294967295>"].subnets.addSC("metric", "Metric for redistributed routes");

				routerOSPFC.redistribute.tag["<0-4294967295>"].subnets.addSC("metric-type", "OSPF/IS-IS exterior metric type for redistributed routes");

				routerOSPFC.redistribute.tag["<0-4294967295>"].subnets.addSC("route-map", "Route map reference");


routerOSPFC.addSC("router-id", "router-id for this OSPF process");
	routerOSPFC["router-id"].addSC("A.B.C.D", "OSPF router-id in IP address format");
routerOSPFC.addSC("summary-address", "Configure IP address summaries");
	routerOSPFC["summary-address"].addSC("A.B.C.D", "IP summary address");
		routerOSPFC["summary-address"]["A.B.C.D"].addSC("A.B.C.D", "Summary mask");

routerOSPFC.addSC("timers", "Adjust routing timers");
	routerOSPFC.timers.addSC("lsa-group-pacing", "OSPF LSA group pacing timer");
		routerOSPFC.timers["lsa-group-pacing"].addSC("<10-1800>", "Interval between group of LSA being refreshed or maxaged");
	routerOSPFC.timers.addSC("spf", "OSPF SPF timers");
		routerOSPFC.timers.spf.addSC("<0-4294967295>", "Delay between receiving a change to SPF calculation");
			routerOSPFC.timers.spf["<0-4294967295>"].addSC("<0-4294967295>", "Hold time between consecutive SPF calculations");
routerOSPFC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerOSPFC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
		routerOSPFC["traffic-share"].min.addSC("across-interfaces", "Use different interfaces for equal-cost paths");
