Output=RTB%23show+running%2Dconfig%0Ahostname+RTB%0A%0Aip+subnet%2Dzero%0A%0Ainterface+Serial0%0A+ip+address+203%2E250%2E15%2E2+255%2E255%2E255%2E252%0A%0Ainterface+Serial1%0A+ip+address+192%2E208%2E10%2E6+255%2E255%2E255%2E252%0A%0Arouter+ospf+10%0A+redistribute+bgp+100+metric+1000+subnets%0A+passive%2Dinterface+Serial1%0A+network+203%2E250%2E0%2E0+0%2E0%2E255%2E255+area+0%0A+network+192%2E208%2E0%2E0+0%2E0%2E255%2E255+area+0%0A%0Arouter+bgp+100%0A+no+synchronization%0A+network+203%2E250%2E15%2E0%0A+neighbor+192%2E208%2E10%2E5+remote%2Das+300%0A+neighbor+203%2E250%2E13%2E41+remote%2Das+100%0A%0ARTB%23%0A