RouterC#show ip route

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, * - candidate default

Gateway of last resort is 168.71.9.1 to network 10.0.0.0

I* 10.0.0.0 [100/82125] via 168.71.9.1, 00:01:06, Serial1
168.71.0.0 255.255.255.0 is subnetted, 5 subnets
C 168.71.9.0 is directly connected, Serial1
C 168.71.8.0 is directly connected, Ethernet0
C 168.71.7.0 is directly connected, Serial0
I 168.71.5.0 [100/10002001] via 168.71.9.1, 00:01:07, Serial1

RouterC#
