
intFC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
intFC.addSC("bandwidth", "Set bandwidth informational parameter");
	intFC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intFC.addSC("carrier-delay", "Specify delay for interface transitions");
intFC.addSC("cdp", "CDP interface subcommands");
intFC.addSC("custom-queue-list", "Assign a custom queue list to an interface");
intFC.addSC("default", "Set a command to its defaults");
intFC.addSC("delay", "Specify interface throughput delay");
intFC.addSC("description", "Interface specific description");
intFC.addSC("duplex", "Configure duplex operation.");
intFC.addSC("exit", "Exit from interface configuration mode");
intFC.addSC("fair-queue", "Enable Fair Queuing on an Interface");
intFC.addSC("help", "Description of the interactive help system");
intFC.addSC("hold-queue", "Set hold queue depth");
intFC.addSC("keepalive", "Enable keepalive");
intFC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intFC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intFC.addSC("logging", "Configure logging for interface");
intFC.addSC("loopback", "Configure internal loopback on an interface");
intFC.addSC("mac-address", "Manually set interface MAC address");
intFC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
intFC.addSC("media-type", "Interface media type");
intFC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
intFC.addSC("negotiation", "Select Autonegotiation mode");
intFC.addSC("no", "Negate a command or set its defaults");
	intFC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intFC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intFC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intFC.no.addSC("cdp", "CDP interface subcommands");
	intFC.no.addSC("custom-queue-list", "Assign a custom queue list to an interface");
	intFC.no.addSC("delay", "Specify interface throughput delay");
	intFC.no.addSC("description", "Interface specific description");
	intFC.no.addSC("duplex", "Configure duplex operation.");
	intFC.no.addSC("fair-queue", "Enable Fair Queuing on an Interface");
	intFC.no.addSC("hold-queue", "Set hold queue depth");
	intFC.no.addSC("keepalive", "Enable keepalive");
	intFC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intFC.no.addSC("logging", "Configure logging for interface");
	intFC.no.addSC("loopback", "Configure internal loopback on an interface");
	intFC.no.addSC("mac-address", "Manually set interface MAC address");
	intFC.no.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intFC.no.addSC("media-type", "Interface media type");
	intFC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intFC.no.addSC("negotiation", "Select Autonegotiation mode");
intFC.addSC("port", "Perform switch port configuration");
intFC.addSC("priority-group", "Assign a priority group to an interface");
intFC.addSC("random-detect", "Enable Weighted Random Early Detection (WRED) on an Interface");
intFC.addSC("rmon", "Configure Remote Monitoring on an interface");
intFC.addSC("service-policy", "Configure QoS Service Policy");
intFC.addSC("shutdown", "Shutdown the selected interface");
intFC.addSC("snmp", "Modify SNMP interface parameters");
intFC.addSC("spanning-tree", "Spanning Tree Subsystem");
intFC.addSC("speed", "Configure speed operation.");
intFC.addSC("switchport", "Set switching mode characteristics");
intFC.addSC("timeout", "Define timeout values for this interface");
intFC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
intFC.addSC("tx-queue-limit", "Configure card level transmit queue limit");
intFC.addSC("udld", "Configure UDLD enabled or disabled and ignore global UDLD setting");
