Output=Router+B%23show+running%2Dconfig%0ARouter+B+Configuration%0Ainterface+serial+0%0Aip+address+170%2E10%2E62%2E2+255%2E255%2E255%2E0%0A%0Ainterface+serial+1%0Aip+address+170%2E10%2E64%2E2+255%2E255%2E255%2E0%0A%0Ainterface+ethernet+0%0Aip+address+170%2E10%2E17%2E2+255%2E255%2E255%2E0%0A%0Ainterface+tokenring+0%0Aip+address+170%2E10%2E16%2E2+255%2E255%2E255%2E0%0A%0Arouter+rip%0Anetwork+170%2E10%2E0%2E0%0A%0ARouter+B%23%0A++