
routerIGRPC.addSC("default", "Set a command to its defaults");
routerIGRPC.addSC("default-information", "Control distribution of default information");
	routerIGRPC["default-information"].addSC("allowed", "Allow default information");
	routerIGRPC["default-information"].addSC("in", "Accept default routing information");
		routerIGRPC["default-information"]["in"].addSC("<1-99>", "A standard IP access list number");
		routerIGRPC["default-information"]["in"].addSC("<1300-1999>", "A standard expanded IP access list number");
		routerIGRPC["default-information"]["in"].addSC("WORD", "Standard Access-list name");
	routerIGRPC["default-information"].addSC("out", "Output default routing information");
		routerIGRPC["default-information"].out.addSC("<1-99>", "A standard IP access list number");
		routerIGRPC["default-information"].out.addSC("<1300-1999>", "A standard expanded IP access list number");
		routerIGRPC["default-information"].out.addSC("WORD", "Standard Access-list name");
routerIGRPC.addSC("default-metric", "Set metric of redistributed routes");
routerIGRPC.addSC("distance", "Define an administrative distance");
	routerIGRPC.distance.addSC("<1-255>", "Administrative distance");
		routerIGRPC.distance["<1-255>"].addSC("A.B.C.D", "IP Source address");
			routerIGRPC.distance["<1-255>"]["A.B.C.D"].addSC("A.B.C.D", "IP address mask");
				routerIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-99>", "IP Standard access list number");
				routerIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1300-1999>", "IP Standard expanded access list number");
				routerIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("WORD", "Standard access-list name");
routerIGRPC.addSC("distribute-list", "Filter networks in routing updates");
	routerIGRPC["distribute-list"].addSC("<1-199>", "IP access list number");
		routerIGRPC["distribute-list"]["<1-199>"].addSC("in", "Filter incoming routing updates");
			routerIGRPC["distribute-list"]["<1-199>"]["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1-199>"]["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerIGRPC["distribute-list"]["<1-199>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1-199>"]["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerIGRPC["distribute-list"]["<1-199>"]["in"].addSC("Loopback", "Loopback interface");
				routerIGRPC["distribute-list"]["<1-199>"]["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerIGRPC["distribute-list"]["<1-199>"]["in"].addSC("Null", "Null interface");
				routerIGRPC["distribute-list"]["<1-199>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerIGRPC["distribute-list"]["<1-199>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerIGRPC["distribute-list"]["<1-199>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerIGRPC["distribute-list"]["<1-199>"].addSC("out", "Filter outgoing routing updates");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1-199>"].out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1-199>"].out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("Loopback", "Loopback interface");
				routerIGRPC["distribute-list"]["<1-199>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("Null", "Null interface");
				routerIGRPC["distribute-list"]["<1-199>"].out.Null.addSC("<0-0>", "Null interface number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("Vlan", "Catalyst Vlans");
				routerIGRPC["distribute-list"]["<1-199>"].out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerIGRPC["distribute-list"]["<1-199>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("connected", "Connected");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerIGRPC["distribute-list"]["<1-199>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerIGRPC["distribute-list"]["<1-199>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerIGRPC["distribute-list"]["<1-199>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerIGRPC["distribute-list"]["<1-199>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerIGRPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerIGRPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerIGRPC["distribute-list"]["<1-199>"].out.addSC("static", "Static routes");
	routerIGRPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
		routerIGRPC["distribute-list"]["<1300-2699>"].addSC("in", "Filter incoming routing updates");
			routerIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1300-2699>"]["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1300-2699>"]["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("Loopback", "Loopback interface");
				routerIGRPC["distribute-list"]["<1300-2699>"]["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("Null", "Null interface");
				routerIGRPC["distribute-list"]["<1300-2699>"]["in"].Null.addSC("<0-0>", "Null interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"]["in"].addSC("Vlan", "Catalyst Vlans");
				routerIGRPC["distribute-list"]["<1300-2699>"]["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerIGRPC["distribute-list"]["<1300-2699>"].addSC("out", "Filter outgoing routing updates");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1300-2699>"].out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Loopback", "Loopback interface");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Null", "Null interface");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.Null.addSC("<0-0>", "Null interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Vlan", "Catalyst Vlans");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("connected", "Connected");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerIGRPC["distribute-list"]["<1300-2699>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerIGRPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerIGRPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerIGRPC["distribute-list"]["<1300-2699>"].out.addSC("static", "Static routes");
	routerIGRPC["distribute-list"].addSC("WORD", "Access-list name");
		routerIGRPC["distribute-list"].WORD.addSC("in", "Filter incoming routing updates");
			routerIGRPC["distribute-list"].WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerIGRPC["distribute-list"].WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerIGRPC["distribute-list"].WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerIGRPC["distribute-list"].WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerIGRPC["distribute-list"].WORD["in"].addSC("Loopback", "Loopback interface");
				routerIGRPC["distribute-list"].WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerIGRPC["distribute-list"].WORD["in"].addSC("Null", "Null interface");
				routerIGRPC["distribute-list"].WORD["in"].Null.addSC("<0-0>", "Null interface number");
			routerIGRPC["distribute-list"].WORD["in"].addSC("Vlan", "Catalyst Vlans");
				routerIGRPC["distribute-list"].WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
		routerIGRPC["distribute-list"].WORD.addSC("out", "Filter outgoing routing updates");
			routerIGRPC["distribute-list"].WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
				routerIGRPC["distribute-list"].WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
			routerIGRPC["distribute-list"].WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
				routerIGRPC["distribute-list"].WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
			routerIGRPC["distribute-list"].WORD.out.addSC("Loopback", "Loopback interface");
				routerIGRPC["distribute-list"].WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerIGRPC["distribute-list"].WORD.out.addSC("Null", "Null interface");
				routerIGRPC["distribute-list"].WORD.out.Null.addSC("<0-0>", "Null interface number");
			routerIGRPC["distribute-list"].WORD.out.addSC("Vlan", "Catalyst Vlans");
				routerIGRPC["distribute-list"].WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
			routerIGRPC["distribute-list"].WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerIGRPC["distribute-list"].WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"].WORD.out.addSC("connected", "Connected");
			routerIGRPC["distribute-list"].WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerIGRPC["distribute-list"].WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerIGRPC["distribute-list"].WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerIGRPC["distribute-list"].WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"].WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerIGRPC["distribute-list"].WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerIGRPC["distribute-list"].WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerIGRPC["distribute-list"].WORD.out.ospf.addSC("<1-65535>", "Process ID");
					routerIGRPC["distribute-list"].WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerIGRPC["distribute-list"].WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerIGRPC["distribute-list"].WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
			routerIGRPC["distribute-list"].WORD.out.addSC("static", "Static routes");
	routerIGRPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
		routerIGRPC["distribute-list"].gateway.addSC("WORD", "Name of an IP prefix-list");
			routerIGRPC["distribute-list"].gateway.WORD.addSC("in", "Filter incoming routing updates");
				routerIGRPC["distribute-list"].gateway.WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerIGRPC["distribute-list"].gateway.WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerIGRPC["distribute-list"].gateway.WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerIGRPC["distribute-list"].gateway.WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerIGRPC["distribute-list"].gateway.WORD["in"].addSC("Loopback", "Loopback interface");
					routerIGRPC["distribute-list"].gateway.WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerIGRPC["distribute-list"].gateway.WORD["in"].addSC("Null", "Null interface");
					routerIGRPC["distribute-list"].gateway.WORD["in"].Null.addSC("<0-0>", "Null interface number");
				routerIGRPC["distribute-list"].gateway.WORD["in"].addSC("Vlan", "Catalyst Vlans");
					routerIGRPC["distribute-list"].gateway.WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
			routerIGRPC["distribute-list"].gateway.WORD.addSC("out", "Filter outgoing routing updates");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerIGRPC["distribute-list"].gateway.WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerIGRPC["distribute-list"].gateway.WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("Loopback", "Loopback interface");
					routerIGRPC["distribute-list"].gateway.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("Null", "Null interface");
					routerIGRPC["distribute-list"].gateway.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("Vlan", "Catalyst Vlans");
					routerIGRPC["distribute-list"].gateway.WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerIGRPC["distribute-list"].gateway.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("connected", "Connected");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerIGRPC["distribute-list"].gateway.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerIGRPC["distribute-list"].gateway.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerIGRPC["distribute-list"].gateway.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerIGRPC["distribute-list"].gateway.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerIGRPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerIGRPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerIGRPC["distribute-list"].gateway.WORD.out.addSC("static", "Static routes");
	routerIGRPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
		routerIGRPC["distribute-list"].prefix.addSC("WORD", "Name of an IP prefix-list");
			routerIGRPC["distribute-list"].prefix.WORD.addSC("gateway", "Filtering incoming updates based on gateway");
			routerIGRPC["distribute-list"].prefix.WORD.addSC("in", "Filter incoming routing updates");
				routerIGRPC["distribute-list"].prefix.WORD["in"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerIGRPC["distribute-list"].prefix.WORD["in"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerIGRPC["distribute-list"].prefix.WORD["in"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerIGRPC["distribute-list"].prefix.WORD["in"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerIGRPC["distribute-list"].prefix.WORD["in"].addSC("Loopback", "Loopback interface");
					routerIGRPC["distribute-list"].prefix.WORD["in"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerIGRPC["distribute-list"].prefix.WORD["in"].addSC("Null", "Null interface");
					routerIGRPC["distribute-list"].prefix.WORD["in"].Null.addSC("<0-0>", "Null interface number");
				routerIGRPC["distribute-list"].prefix.WORD["in"].addSC("Vlan", "Catalyst Vlans");
					routerIGRPC["distribute-list"].prefix.WORD["in"].Vlan.addSC("<1-1001>", "Vlan interface number");
			routerIGRPC["distribute-list"].prefix.WORD.addSC("out", "Filter outgoing routing updates");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routerIGRPC["distribute-list"].prefix.WORD.out["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routerIGRPC["distribute-list"].prefix.WORD.out.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("Loopback", "Loopback interface");
					routerIGRPC["distribute-list"].prefix.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("Null", "Null interface");
					routerIGRPC["distribute-list"].prefix.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("Vlan", "Catalyst Vlans");
					routerIGRPC["distribute-list"].prefix.WORD.out.Vlan.addSC("<1-1001>", "Vlan interface number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerIGRPC["distribute-list"].prefix.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("connected", "Connected");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerIGRPC["distribute-list"].prefix.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerIGRPC["distribute-list"].prefix.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerIGRPC["distribute-list"].prefix.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerIGRPC["distribute-list"].prefix.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerIGRPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerIGRPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerIGRPC["distribute-list"].prefix.WORD.out.addSC("static", "Static routes");
routerIGRPC.addSC("exit", "Exit from routing protocol configuration mode");
routerIGRPC.addSC("help", "Description of the interactive help system");
routerIGRPC.addSC("input-queue", "Specify input queue depth");
routerIGRPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerIGRPC["maximum-paths"].addSC("<1-8>", "Number of paths");
routerIGRPC.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerIGRPC.metric.addSC("holddown", "Enable IGRP holddown");
	routerIGRPC.metric.addSC("maximum-hops", "Advertise IGRP routes greater than <hops> as unreachable");
		routerIGRPC.metric["maximum-hops"].addSC("<1-255>", "Hop count");
	routerIGRPC.metric.addSC("weights", "Modify IGRP metric coefficients");
		routerIGRPC.metric.weights.addSC("<0-8>", "Type Of Service (Only TOS 0 supported)");
			routerIGRPC.metric.weights["<0-8>"].addSC("<0-4294967295>", "K1");
				routerIGRPC.metric.weights["<0-8>"]["<0-4294967295>"].addSC("<0-4294967295>", "K2");
					routerIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K3");
						routerIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K4");
							routerIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K5");
routerIGRPC.addSC("neighbor", "Specify a neighbor router");
	routerIGRPC.neighbor.addSC("A.B.C.D", "Neighbor address");
routerIGRPC.addSC("network", "Enable routing on an IP network");
	routerIGRPC.network.addSC("A.B.C.D", "Network number");
routerIGRPC.addSC("no", "Negate a command or set its defaults");
routerIGRPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
routerIGRPC.addSC("passive-interface", "Suppress routing updates on an interface");
	routerIGRPC["passive-interface"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
		routerIGRPC["passive-interface"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
	routerIGRPC["passive-interface"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
		routerIGRPC["passive-interface"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
	routerIGRPC["passive-interface"].addSC("Loopback", "Loopback interface");
		routerIGRPC["passive-interface"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
	routerIGRPC["passive-interface"].addSC("Null", "Null interface");
		routerIGRPC["passive-interface"].Null.addSC("<0-0>", "Null interface number");
	routerIGRPC["passive-interface"].addSC("Vlan", "Catalyst Vlans");
		routerIGRPC["passive-interface"].Vlan.addSC("<1-1001>", "Vlan interface number");
	routerIGRPC["passive-interface"].addSC("default", "Suppress routing updates on all interfaces");
routerIGRPC.addSC("redistribute", "Redistribute information from another routing protocol");
	routerIGRPC.redistribute.addSC("bgp", "Border Gateway Protocol (BGP)");
		routerIGRPC.redistribute.bgp.addSC("<1-65535>", "Autonomous system number");
	routerIGRPC.redistribute.addSC("connected", "Connected");
	routerIGRPC.redistribute.addSC("egp", "Exterior Gateway Protocol (EGP)");
		routerIGRPC.redistribute.egp.addSC("<0-65535>", "Remote autonomous system number");
	routerIGRPC.redistribute.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
		routerIGRPC.redistribute.eigrp.addSC("<1-65535>", "Autonomous system number");
	routerIGRPC.redistribute.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
		routerIGRPC.redistribute.igrp.addSC("<1-65535>", "Autonomous system number");
	routerIGRPC.redistribute.addSC("isis", "ISO IS-IS");
		routerIGRPC.redistribute.isis.addSC("level-1", "IS-IS level-1 routes only");
		routerIGRPC.redistribute.isis.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
		routerIGRPC.redistribute.isis.addSC("level-2", "IS-IS level-2 routes only");
		routerIGRPC.redistribute.isis.addSC("WORD", "ISO routing area tag");
			routerIGRPC.redistribute.isis.WORD.addSC("level-1", "IS-IS level-1 routes only");
			routerIGRPC.redistribute.isis.WORD.addSC("level-1-2", "IS-IS level-1 and level-2 routes");
			routerIGRPC.redistribute.isis.WORD.addSC("level-2", "IS-IS level-2 routes only");
	routerIGRPC.redistribute.addSC("iso-igrp", "IGRP for OSI networks");
		routerIGRPC.redistribute["iso-igrp"].addSC("WORD", "ISO routing area tag");
	routerIGRPC.redistribute.addSC("metric", "Metric for redistributed routes");
		routerIGRPC.redistribute.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
			routerIGRPC.redistribute.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
				routerIGRPC.redistribute.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
					routerIGRPC.redistribute.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
						routerIGRPC.redistribute.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerIGRPC.redistribute.addSC("mobile", "Mobile routes");
		routerIGRPC.redistribute.mobile.addSC("metric", "Metric for redistributed routes");
			routerIGRPC.redistribute.mobile.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerIGRPC.redistribute.mobile.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerIGRPC.redistribute.mobile.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerIGRPC.redistribute.mobile.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerIGRPC.redistribute.mobile.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerIGRPC.redistribute.addSC("odr", "On Demand stub Routes");
		routerIGRPC.redistribute.odr.addSC("metric", "Metric for redistributed routes");
			routerIGRPC.redistribute.odr.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerIGRPC.redistribute.odr.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerIGRPC.redistribute.odr.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerIGRPC.redistribute.odr.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerIGRPC.redistribute.odr.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerIGRPC.redistribute.addSC("ospf", "Open Shortest Path First (OSPF)");
		routerIGRPC.redistribute.ospf.addSC("<1-65535>", "Process ID");
			routerIGRPC.redistribute.ospf["<1-65535>"].addSC("match", "Redistribution of OSPF routes");
				routerIGRPC.redistribute.ospf["<1-65535>"].match.addSC("external", "Redistribute OSPF external routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match.external.addSC("<1-1>", "Redistribute external type 1 routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerIGRPC.redistribute.ospf["<1-65535>"].match.addSC("internal", "Redistribute OSPF internal routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match.internal.addSC("external", "Redistribute OSPF external routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
				routerIGRPC.redistribute.ospf["<1-65535>"].match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
			routerIGRPC.redistribute.ospf["<1-65535>"].addSC("metric", "Metric for redistributed routes");
				routerIGRPC.redistribute.ospf["<1-65535>"].metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
					routerIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
						routerIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
							routerIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
								routerIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
									routerIGRPC.redistribute.ospf["<1-65535>"].metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"]["<1-4294967295>"].addSC("match", "Redistribution of OSPF routes");
			routerIGRPC.redistribute.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
				routerIGRPC.redistribute.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
					routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.addSC("match", "Redistribution of OSPF routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("external", "Redistribute OSPF external routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.external.addSC("<1-1>", "Redistribute external type 1 routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("internal", "Redistribute OSPF internal routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.addSC("external", "Redistribute OSPF external routes");
								routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match.addSC("nssa-external", "Redistribute OSPF NSSA external routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("<1-1>", "Redistribute NSSA external type 1 routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("<2-2>", "Redistribute NSSA external type 2 routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("external", "Redistribute OSPF external routes");
								routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].external.addSC("<1-1>", "Redistribute external type 1 routes");
								routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].external.addSC("<2-2>", "Redistribute external type 2 routes");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].addSC("internal", "Redistribute OSPF internal routes");
								routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.addSC("external", "Redistribute OSPF external routes");
									routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.external.addSC("<1-1>", "Redistribute external type 1 routes");
									routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.match["nssa-external"].internal.external.addSC("<2-2>", "Redistribute external type 2 routes");
					routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.addSC("metric", "Metric for redistributed routes");
						routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
							routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
								routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
									routerIGRPC.redistribute.ospf["<1-65535>"].vrf.WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
	routerIGRPC.redistribute.addSC("rip", "Routing Information Protocol (RIP)");
		routerIGRPC.redistribute.rip.addSC("metric", "Metric for redistributed routes");
			routerIGRPC.redistribute.rip.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerIGRPC.redistribute.rip.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerIGRPC.redistribute.rip.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerIGRPC.redistribute.rip.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerIGRPC.redistribute.rip.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerIGRPC.redistribute.addSC("route-map", "Route map reference");
		routerIGRPC.redistribute["route-map"].addSC("WORD", "Pointer to route-map entries");
			routerIGRPC.redistribute["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
				routerIGRPC.redistribute["route-map"].WORD.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
					routerIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
						routerIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
							routerIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
								routerIGRPC.redistribute["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routerIGRPC.redistribute.addSC("static", "Static routes");
		routerIGRPC.redistribute.static.addSC("metric", "Metric for redistributed routes");
			routerIGRPC.redistribute.static.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
				routerIGRPC.redistribute.static.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
					routerIGRPC.redistribute.static.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
						routerIGRPC.redistribute.static.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
							routerIGRPC.redistribute.static.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
		routerIGRPC.redistribute.static.addSC("route-map", "Route map reference");
			routerIGRPC.redistribute.static["route-map"].addSC("WORD", "Pointer to route-map entries");
				routerIGRPC.redistribute.static["route-map"].WORD.addSC("metric", "Metric for redistributed routes");
					routerIGRPC.redistribute.static["route-map"].WORD.metric.addSC("<1-4294967295>", "Bandwidth metric in Kbits per second");
						routerIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"].addSC("<0-4294967295>", "IGRP delay metric, in 10 microsecond units");
							routerIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
								routerIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
									routerIGRPC.redistribute.static["route-map"].WORD.metric["<1-4294967295>"]["<0-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
routerIGRPC.addSC("timers", "Adjust routing timers");
	routerIGRPC.timers.addSC("basic", "Basic routing protocol update timers");
		routerIGRPC.timers.basic.addSC("<0-4294967295>", "Interval between updates");
			routerIGRPC.timers.basic["<0-4294967295>"].addSC("<1-4294967295>", "Invalid");
				routerIGRPC.timers.basic["<0-4294967295>"]["<1-4294967295>"].addSC("<0-4294967295>", "Holddown");
					routerIGRPC.timers.basic["<0-4294967295>"]["<1-4294967295>"]["<0-4294967295>"].addSC("<1-4294967295>", "Flush");
						routerIGRPC.timers.basic["<0-4294967295>"]["<1-4294967295>"]["<0-4294967295>"]["<1-4294967295>"].addSC("<1-4294967295>", "Sleep time, in milliseconds");
routerIGRPC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerIGRPC["traffic-share"].addSC("balanced", "Share inversely proportional to metric");
	routerIGRPC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
		routerIGRPC["traffic-share"].min.addSC("across-interfaces", "Use different interfaces for equal-cost paths");
routerIGRPC.addSC("validate-update-source", "Perform sanity checks against source address of routing updates");
routerIGRPC.addSC("variance", "Control load balancing variance");
	routerIGRPC.variance.addSC("<1-128>", "Metric variance multiplier");
