
enableC.addSC("access-enable", "Create a temporary Access-List entry");
enableC.addSC("access-template", "Create a temporary Access-List entry");
enableC.addSC("archive", "manage archive files");
enableC.addSC("cd", "Change current directory");
enableC.addSC("clear", "Reset functions");
	enableC.clear.addSC("access-list", "Clear access list statistical information");
	enableC.clear.addSC("access-template", "Access-template");
	enableC.clear.addSC("arp-cache", "Clear the entire ARP cache");
	enableC.clear.addSC("cdp", "Reset cdp information");
	enableC.clear.addSC("cgmp", "Reset CGMP information");
	enableC.clear.addSC("controllers", "Clear interface controller info");
	enableC.clear.addSC("counters", "Clear counters on one or all interfaces");
	enableC.clear.addSC("host", "Delete host table entries");
	enableC.clear.addSC("interface", "Clear the hardware logic on an interface");
	enableC.clear.addSC("ip", "IP");
		enableC.clear.ip.addSC("access-list", "Clear access list statistical information");
		enableC.clear.ip.addSC("access-template", "Access-template");
		enableC.clear.ip.addSC("accounting", "Clear IP accounting database");
		enableC.clear.ip.addSC("address", "Delete interface's IP address");
		enableC.clear.ip.addSC("nat", "Clear NAT");
			enableC.clear.ip.nat.addSC("statistics", "Clear translation statistics");
			enableC.clear.ip.nat.addSC("translation", "Clear dynamic translation");
				enableC.clear.ip.nat.translation.addSC("*", "Delete all dynamic translations");
				enableC.clear.ip.nat.translation.addSC("inside", "Inside addresses (and ports)");
				enableC.clear.ip.nat.translation.addSC("outside", "Outside addresses (and ports)");
				enableC.clear.ip.nat.translation.addSC("tcp", "Transmission Control Protocol");
				enableC.clear.ip.nat.translation.addSC("udp", "User Datagram Protocol");
		enableC.clear.ip.addSC("redirect", "Redirect cache");
	enableC.clear.addSC("line", "Reset a terminal line");
	enableC.clear.addSC("logging", "Clear logging buffer");
	enableC.clear.addSC("mac-address-table", "MAC forwarding table");
	enableC.clear.addSC("tcp", "Clear a TCP connection or statistics");
	enableC.clear.addSC("vmps", "VMPS statistics");
	enableC.clear.addSC("vtp", "Clear VTP items");
enableC.addSC("clock", "Manage the system clock");
enableC.addSC("cluster", "cluster exec mode commands");
enableC.addSC("configure", "Enter configuration mode");
enableC.addSC("connect", "Open a terminal connection");
enableC.addSC("copy", "Copy from one file to another");
	enableC.copy.addSC("/erase", "Erase destination file system.");
	enableC.copy.addSC("bs:", "Copy from bs: file system");
	enableC.copy.addSC("flash:", "Copy from flash: file system");
	enableC.copy.addSC("null:", "Copy from null: file system");
	enableC.copy.addSC("nvram:", "Copy from nvram: file system");
	enableC.copy.addSC("rcp:", "Copy from rcp: file system");
	enableC.copy.addSC("running-config", "Copy from current system configuration");
		enableC.copy["running-config"].addSC("flash:", "Copy to flash: file system");
		enableC.copy["running-config"].addSC("null:", "Copy to null: file system");
		enableC.copy["running-config"].addSC("nvram:", "Copy to nvram: file system");
		enableC.copy["running-config"].addSC("rcp:", "Copy to rcp: file system");
		enableC.copy["running-config"].addSC("running-config", "Update (merge with) current system configuration");
		enableC.copy["running-config"].addSC("startup-config", "Copy to startup configuration");
		enableC.copy["running-config"].addSC("system:", "Copy to system: file system");
		enableC.copy["running-config"].addSC("tftp:", "Copy to tftp: file system");
		enableC.copy["running-config"].addSC("zflash:", "Copy to zflash: file system");
	enableC.copy.addSC("startup-config", "Copy from startup configuration");
		enableC.copy["startup-config"].addSC("flash:", "Copy to flash: file system");
		enableC.copy["startup-config"].addSC("null:", "Copy to null: file system");
		enableC.copy["startup-config"].addSC("nvram:", "Copy to nvram: file system");
		enableC.copy["startup-config"].addSC("rcp:", "Copy to rcp: file system");
		enableC.copy["startup-config"].addSC("running-config", "Update (merge with) current system configuration");
		enableC.copy["startup-config"].addSC("startup-config", "Copy to startup configuration");
		enableC.copy["startup-config"].addSC("system:", "Copy to system: file system");
		enableC.copy["startup-config"].addSC("tftp:", "Copy to tftp: file system");
		enableC.copy["startup-config"].addSC("zflash:", "Copy to zflash: file system");
	enableC.copy.addSC("system:", "Copy from system: file system");
	enableC.copy.addSC("tftp:", "Copy from tftp: file system");
	enableC.copy.addSC("xmodem:", "Copy from xmodem: file system");
	enableC.copy.addSC("ymodem:", "Copy from ymodem: file system");
	enableC.copy.addSC("zflash:", "Copy from zflash: file system");
enableC.addSC("debug", "Debugging functions (see also 'undebug')");
	enableC.debug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
	enableC.debug.addSC("all", "Enable all debugging");
	enableC.debug.addSC("arp", "IP ARP and HP Probe transactions");
	enableC.debug.addSC("cdp", "CDP information");
	enableC.debug.addSC("cgmp", "CGMP protocol activity");
	enableC.debug.addSC("cluster", "Cluster information");
	enableC.debug.addSC("condition", "Condition");
	enableC.debug.addSC("cpu-interface", "CPU interface driver debug flag");
	enableC.debug.addSC("custom-queue", "Custom output queueing");
	enableC.debug.addSC("domain", "Domain Name System");
	enableC.debug.addSC("esp", "Expansion Slot Protocol Debug");
	enableC.debug.addSC("ethernet-controller", "Ethernet controller driver debug flags");
	enableC.debug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.debug.addSC("interface", "interface");
	enableC.debug.addSC("ip", "IP information");
		enableC.debug.ip.addSC("error", "IP error debugging");
		enableC.debug.ip.addSC("html", "HTML connections");
		enableC.debug.ip.addSC("http", "HTTP connections");
		enableC.debug.ip.addSC("icmp", "ICMP transactions");
		enableC.debug.ip.addSC("mpacket", "IP multicast packet debugging");
		enableC.debug.ip.addSC("nat", "NAT events");
		enableC.debug.ip.addSC("packet", "General IP debugging and IPSO security transactions");
		enableC.debug.ip.addSC("peer", "IP peer address activity");
		enableC.debug.ip.addSC("security", "IP security options");
		enableC.debug.ip.addSC("socket", "Socket event");
		enableC.debug.ip.addSC("tcp", "TCP information");
		enableC.debug.ip.addSC("tempacl", "IP temporary ACL");
		enableC.debug.ip.addSC("udp", "UDP based transactions");
	enableC.debug.addSC("list", "Set interface or/and access list for the next debug command");
	enableC.debug.addSC("mat", "MAC address table");
	enableC.debug.addSC("modem", "Modem control/process activation");
	enableC.debug.addSC("module", "Module debug flags");
	enableC.debug.addSC("ntp", "NTP information");
	enableC.debug.addSC("nvram", "Debug NVRAM behavior");
	enableC.debug.addSC("packet", "Log unknown packets");
	enableC.debug.addSC("port", "Switch port");
	enableC.debug.addSC("priority", "Priority output queueing");
	enableC.debug.addSC("snmp", "SNMP information");
	enableC.debug.addSC("spantree", "Spanning tree information");
	enableC.debug.addSC("standby", "Hot standby protocol");
	enableC.debug.addSC("sw-vlan", "vlan manager");
	enableC.debug.addSC("tacacs", "TACACS authentication and authorization");
	enableC.debug.addSC("telnet", "Incoming telnet connections");
	enableC.debug.addSC("tftp", "TFTP debugging");
	enableC.debug.addSC("udld", "UDLD protocol");
enableC.addSC("delete", "Delete a file");
enableC.addSC("dir", "List files on a filesystem");
enableC.addSC("disable", "Turn off privileged commands");
enableC.addSC("disconnect", "Disconnect an existing network connection");
enableC.addSC("enable", "Turn on privileged commands");
	enableC.enable.addSC("<0-15>", "Enable level");
enableC.addSC("erase", "Erase a filesystem");
enableC.addSC("exit", "Exit from the EXEC");
enableC.addSC("format", "Format a filesystem");
enableC.addSC("fsck", "Fsck a filesystem");
enableC.addSC("help", "Description of the interactive help system");
enableC.addSC("hw-module", "Commands to manipulate a target module");
enableC.addSC("lock", "Lock the terminal");
enableC.addSC("login", "Log in as a particular user");
enableC.addSC("logout", "Exit from the EXEC");
enableC.addSC("mkdir", "Create new directory");
enableC.addSC("more", "Display the contents of a file");
enableC.addSC("name-connection", "Name an existing network connection");
enableC.addSC("no", "Disable debugging functions");
enableC.addSC("ping", "Send echo messages");
	enableC.ping.addSC("WORD", "Ping destination address or hostname");
	enableC.ping.addSC("ip", "IP echo");
		enableC.ping.ip.addSC("WORD", "Ping destination address or hostname");
	enableC.ping.addSC("tag", "Tag encapsulated IP echo");
		enableC.ping.tag.addSC("WORD", "Ping destination address or hostname");
enableC.addSC("pwd", "Display current working directory");
enableC.addSC("rcommand", "Run command on remote switch");
enableC.addSC("reload", "Halt and perform a cold restart");
enableC.addSC("rename", "Rename a file");
enableC.addSC("resume", "Resume an active network connection");
enableC.addSC("rmdir", "Remove existing directory");
enableC.addSC("rsh", "Execute a remote command");
enableC.addSC("send", "Send a message to other tty lines");
enableC.addSC("session", "Start remote console session");
enableC.addSC("set", "Set system parameter (not config)");
enableC.addSC("setup", "Run the SETUP command facility");
enableC.addSC("show", "Show running system information");
	enableC.show.addSC("access-lists", "List access lists");
	enableC.show.addSC("accounting", "Accounting data for active sessions");
	enableC.show.addSC("aliases", "Display alias commands");
	enableC.show.addSC("arp", "ARP table");
	enableC.show.addSC("boot", "show boot attributes");
	enableC.show.addSC("buffers", "Buffer pool statistics");
	enableC.show.addSC("cdp", "CDP information");
	enableC.show.addSC("cgmp", "Display CGMP information");
	enableC.show.addSC("class-map", "Show QoS Class Map");
	enableC.show.addSC("clock", "Display the system clock");
	enableC.show.addSC("cluster", "Cluster information");
	enableC.show.addSC("configuration", "Contents of Non-Volatile memory");
	enableC.show.addSC("controllers", "Interface controller status");
	enableC.show.addSC("debugging", "State of each debugging option");
	enableC.show.addSC("diags", "Show runtime diagnostic info");
	enableC.show.addSC("exception", "exception informations");
	enableC.show.addSC("file", "Show filesystem information");
	enableC.show.addSC("flash:", "display information about flash: file system");
	enableC.show.addSC("forward", "Show Controller forwarding map");
	enableC.show.addSC("history", "Display the session command history");
	enableC.show.addSC("hosts", "IP domain-name, lookup style, nameservers, and host table");
	enableC.show.addSC("html", "HTML helper commands");
	enableC.show.addSC("interfaces", "Interface status and configuration");
	enableC.show.addSC("ip", "IP information");
		enableC.show.ip.addSC("access-lists", "List IP access lists");
		enableC.show.ip.addSC("accounting", "The active IP accounting database");
		enableC.show.ip.addSC("aliases", "IP alias table");
		enableC.show.ip.addSC("arp", "IP ARP table");
		enableC.show.ip.addSC("interface", "IP interface status and configuration");
		enableC.show.ip.addSC("local", "IP local options");
		enableC.show.ip.addSC("nat", "IP NAT information");
			enableC.show.ip.nat.addSC("statistics", "Translation statistics");
			enableC.show.ip.nat.addSC("translations", "Translation entries");
				enableC.show.ip.nat.translations.addSC("verbose", "Show extra information");
		enableC.show.ip.addSC("redirects", "IP redirects");
		enableC.show.ip.addSC("sockets", "Open IP sockets");
		enableC.show.ip.addSC("traffic", "IP protocol statistics");
	enableC.show.addSC("line", "TTY line information");
		enableC.show.line.addSC("<0-16>", "First Line range");
			enableC.show.line["<0-16>"].addSC("<1-16>", "Last Line range");
		enableC.show.line.addSC("console", "Primary terminal line");
			enableC.show.line.console.addSC("<0-0>", "First Line range");
		enableC.show.line.addSC("summary", "Quick line status summary");
		enableC.show.line.addSC("vty", "Virtual terminal");
			enableC.show.line.vty.addSC("<0-15>", "First Line range");
				enableC.show.line.vty["<0-15>"].addSC("<1-15>", "Last Line range");
				enableC.show.line.vty["<0-15>"].addSC("summary", "Quick line status summary");
	enableC.show.addSC("location", "Display the system location");
	enableC.show.addSC("logging", "Show the contents of logging buffers");
	enableC.show.addSC("mac-address-table", "MAC forwarding table");
	enableC.show.addSC("memory", "Memory statistics");
	enableC.show.addSC("ntp", "Network time protocol");
	enableC.show.addSC("policy-map", "Show QoS Policy Map");
		enableC.show["policy-map"].addSC("WORD", "policy-map name");
			enableC.show["policy-map"].WORD.addSC("class", "Show Qos Policy actions for a indvidual class");
				enableC.show["policy-map"].WORD.class.addSC("WORD", "class-map name");
		enableC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
			enableC.show["policy-map"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				enableC.show["policy-map"].interface.FastEthernet.addSC("<0-2>", "FastEthernet interface number");
			enableC.show["policy-map"].interface.addSC("Null", "Null interface");
				enableC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
			enableC.show["policy-map"].interface.addSC("VLAN", "Switch VLAN Virtual Interface");
				enableC.show["policy-map"].interface.VLAN.addSC("<1-1001>", "VLAN interface number");
	enableC.show.addSC("port", "Show switch port configuration");
	enableC.show.addSC("post", "Power On Self Test results");
	enableC.show.addSC("privilege", "Show current privilege level");
	enableC.show.addSC("processes", "Active process statistics");
	enableC.show.addSC("queue", "Show queue contents");
	enableC.show.addSC("queueing", "Show queueing configuration");
	enableC.show.addSC("registry", "Function registry information");
	enableC.show.addSC("reload", "Scheduled reload information");
	enableC.show.addSC("rhosts", "Remote-host+user equivalences");
	enableC.show.addSC("rmon", "rmon statistics");
	enableC.show.addSC("running-config", "Current operating configuration");
		enableC.show["running-config"].addSC("interface", "Show interface configuration");
			enableC.show["running-config"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				enableC.show["running-config"].interface.FastEthernet.addSC("<0-2>", "FastEthernet interface number");
			enableC.show["running-config"].interface.addSC("Null", "Null interface");
				enableC.show["running-config"].interface.Null.addSC("<0-0>", "Null interface number");
			enableC.show["running-config"].interface.addSC("VLAN", "Switch VLAN Virtual Interface");
				enableC.show["running-config"].interface.VLAN.addSC("<1-1001>", "VLAN interface number");
	enableC.show.addSC("sessions", "Information about Telnet connections");
	enableC.show.addSC("snmp", "snmp statistics");
	enableC.show.addSC("spanning-tree", "Spanning tree topology");
	enableC.show.addSC("stacks", "Process stack utilization");
	enableC.show.addSC("standby", "Hot standby protocol information");
	enableC.show.addSC("startup-config", "Contents of startup configuration");
	enableC.show.addSC("subsys", "Show subsystem information");
	enableC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	enableC.show.addSC("tcp", "Status of TCP connections");
	enableC.show.addSC("tech-support", "Show system information for Tech-Support");
	enableC.show.addSC("terminal", "Display terminal configuration parameters");
	enableC.show.addSC("time-range", "Time range");
	enableC.show.addSC("udld", "UDLD information");
	enableC.show.addSC("users", "Display information about terminal lines");
	enableC.show.addSC("version", "System hardware and software status");
	enableC.show.addSC("vlan", "VTP VLAN status");
		enableC.show.vlan.addSC("brief", "VTP all VLAN status in brief");
		enableC.show.vlan.addSC("id", "VTP VLAN status by VLAN id");
			enableC.show.vlan.id.addSC("<1-1005>", "A VTP VLAN number");
		enableC.show.vlan.addSC("name", "VTP VLAN status by VLAN name");
			enableC.show.vlan.name.addSC("WORD", "A VTP VLAN name");
	enableC.show.addSC("vmps", "VMPS version information");
	enableC.show.addSC("vtp", "VTP information");
enableC.addSC("systat", "Display information about terminal lines");
enableC.addSC("telnet", "Open a telnet connection");
enableC.addSC("terminal", "Set terminal line parameters");
enableC.addSC("test", "Test subsystems, memory, and interfaces");
enableC.addSC("traceroute", "Trace route to destination");
	enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("appletalk", "AppleTalk Trace");
		enableC.traceroute.appletalk.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("clns", "ISO CLNS Trace");
		enableC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ip", "IP Trace");
		enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipx", "IPX Trace");
		enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("oldvines", "Vines Trace (Cisco)");
		enableC.traceroute.oldvines.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("vines", "Vines Trace (Banyan)");
		enableC.traceroute.vines.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
enableC.addSC("udld", "UDLD protocol commands");
enableC.addSC("undebug", "Disable debugging functions (see also 'debug')");
	enableC.undebug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
	enableC.undebug.addSC("all", "Enable all debugging");
	enableC.undebug.addSC("arp", "IP ARP and HP Probe transactions");
	enableC.undebug.addSC("cdp", "CDP information");
	enableC.undebug.addSC("cgmp", "CGMP protocol activity");
	enableC.undebug.addSC("cluster", "Cluster information");
	enableC.undebug.addSC("condition", "Condition");
	enableC.undebug.addSC("cpu-interface", "CPU interface driver debug flag");
	enableC.undebug.addSC("custom-queue", "Custom output queueing");
	enableC.undebug.addSC("domain", "Domain Name System");
	enableC.undebug.addSC("esp", "Expansion Slot Protocol Debug");
	enableC.undebug.addSC("ethernet-controller", "Ethernet controller driver debug flags");
	enableC.undebug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.undebug.addSC("interface", "interface");
	enableC.undebug.addSC("ip", "IP information");
	enableC.undebug.addSC("list", "Set interface or/and access list for the next debug command");
	enableC.undebug.addSC("mat", "MAC address table");
	enableC.undebug.addSC("modem", "Modem control/process activation");
	enableC.undebug.addSC("module", "Module debug flags");
	enableC.undebug.addSC("ntp", "NTP information");
	enableC.undebug.addSC("nvram", "Debug NVRAM behavior");
	enableC.undebug.addSC("packet", "Log unknown packets");
	enableC.undebug.addSC("port", "Switch port");
	enableC.undebug.addSC("priority", "Priority output queueing");
	enableC.undebug.addSC("snmp", "SNMP information");
	enableC.undebug.addSC("spantree", "Spanning tree information");
	enableC.undebug.addSC("standby", "Hot standby protocol");
	enableC.undebug.addSC("sw-vlan", "vlan manager");
	enableC.undebug.addSC("tacacs", "TACACS authentication and authorization");
	enableC.undebug.addSC("telnet", "Incoming telnet connections");
	enableC.undebug.addSC("tftp", "TFTP debugging");
	enableC.undebug.addSC("udld", "UDLD protocol");
enableC.addSC("verify", "Verify a file");
enableC.addSC("vlan", "Configure VLAN parameters");
enableC.addSC("vmps", "VMPS actions");
enableC.addSC("where", "List active connections");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
