Router-B#show ip bgp neighbors
BGP neighbor is 2.0.0.2,  remote AS 300, internal link
 Member of peer-group EXTERNALMAP for session parameters
  BGP version 4, remote router ID 12.0.0.1
  BGP state = Established, up for 01:00:58
  Last read 00:00:58, hold time is 180, keepalive interval is 60 seconds
  Neighbor capabilities:
    Route refresh: advertised and received
    Address family IPv4 Unicast: advertised and received
  Received 203 messages, 0 notifications, 0 in queue
  Sent 207 messages, 0 notifications, 0 in queue
  Route refresh request: received 0, sent 0
  Minimum time between advertisement runs is 5 seconds

 For address family: IPv4 Unicast
  BGP table version 12, neighbor version 12
  Index 1, Offset 0, Mask 0x2
  EXTERNALMAP peer-group member
  NEXT_HOP is always this router
  Outgoing update network filter list is 1
  1 accepted prefixes consume 36 bytes
  Prefix advertised 7, suppressed 0, withdrawn 3

  Connections established 2; dropped 0
  Last reset 01:01:09, due to Member added to peergroup
Connection state is ESTAB, I/O status: 1, unread input bytes: 0
Local host: 2.0.0.1, Local port: 11032
Foreign host: 2.0.0.2, Foreign port: 179

Enqueued packets for retransmit: 0, input: 0  mis-ordered: 0 (0 bytes)

Event Timers (current time is 0xD6DE94):
Timer          Starts    Wakeups            Next
Retrans            65          0             0x0
TimeWait            0          0             0x0
AckHold            65         18             0x0
SendWnd             0          0             0x0
KeepAlive           0          0             0x0
GiveUp              0          0             0x0
PmtuAger            0          0             0x0
DeadWait            0          0             0x0

iss: 2835463828  snduna: 2835465177  sndnxt: 2835465177     sndwnd:  15036
irs: 2595724234  rcvnxt: 2595725526  rcvwnd:      15093  delrcvwnd:   1291

SRTT: 300 ms, RTTO: 607 ms, RTV: 3 ms, KRTT: 0 ms
minRTT: 16 ms, maxRTT: 300 ms, ACK hold: 200 ms
Flags: higher precedence, nagle

Datagrams (max data segment is 1460 bytes):
Rcvd: 114 (out of order: 0), with data: 65, total data bytes: 1291
Sent: 84 (retransmit: 0), with data: 64, total data bytes: 1348

BGP neighbor is 3.0.0.2,  remote AS 200, external link
  BGP version 4, remote router ID 11.0.0.1
  BGP state = Established, up for 02:18:17
  Last read 00:00:18, hold time is 180, keepalive interval is 60 seconds
  Neighbor capabilities:
    Route refresh: advertised and received
    Address family IPv4 Unicast: advertised and received
  Received 173 messages, 0 notifications, 0 in queue
  Sent 176 messages, 0 notifications, 0 in queue
  Route refresh request: received 0, sent 0
  Minimum time between advertisement runs is 30 seconds

 For address family: IPv4 Unicast
  BGP table version 12, neighbor version 12
  Index 2, Offset 0, Mask 0x4
  1 accepted prefixes consume 36 bytes
  Prefix advertised 6, suppressed 0, withdrawn 1

  Connections established 4; dropped 3
  Last reset 02:18:38, due to Peer closed the session
Connection state is ESTAB, I/O status: 1, unread input bytes: 0
Local host: 3.0.0.1, Local port: 179
Foreign host: 3.0.0.2, Foreign port: 11005

Enqueued packets for retransmit: 0, input: 0  mis-ordered: 0 (0 bytes)

Event Timers (current time is 0xD6F39C):
Timer          Starts    Wakeups            Next
Retrans           146          0             0x0
TimeWait            0          0             0x0
AckHold           142         46             0x0
SendWnd             0          0             0x0
KeepAlive           0          0             0x0
GiveUp              0          0             0x0
PmtuAger            0          0             0x0
DeadWait            0          0             0x0

iss: 2496095970  snduna: 2496098833  sndnxt: 2496098833     sndwnd:  14986
irs: 2473456117  rcvnxt: 2473458869  rcvwnd:      15111  delrcvwnd:   1273

SRTT: 300 ms, RTTO: 607 ms, RTV: 3 ms, KRTT: 0 ms
minRTT: 16 ms, maxRTT: 300 ms, ACK hold: 200 ms
Flags: passive open, nagle, gen tcbs

Datagrams (max data segment is 1460 bytes):
Rcvd: 246 (out of order: 0), with data: 142, total data bytes: 2751
Sent: 193 (retransmit: 0), with data: 145, total data bytes: 2862
Router-B#
