access-expression Build a bridge boolean access expression arp Set arp type (arpa, probe, snap) or timeout atm Modify ATM parameters bandwidth Set bandwidth informational parameter bridge-group Transparent bridging interface parameters bundle Configure ATM VC Bundle carrier-delay Specify delay for interface transitions cdp CDP interface subcommands class-int Configure default vc-class name default Set a command to its defaults delay Specify interface throughput delay description Interface specific description dsl ADSL subcommands exit Exit from interface configuration mode h323-gateway Configure H323 Gateway help Description of the interactive help system hold-queue Set hold queue depth ip Interface Internet Protocol config commands ipx Novell/IPX interface subcommands llc2 LLC2 Interface Subcommands load-interval Specify interval for load calculation for an interface logging Configure logging for interface loopback Configure internal loopback on an interface mac-address Manually set interface MAC address map-group Configure static map group max-reserved-bandwidth Maximum Reservable Bandwidth on an Interface mtu Set the interface Maximum Transmission Unit (MTU) multilink-group Put interface in a multilink bundle netbios Use a defined NETBIOS access list or enable name-caching no Negate a command or set its defaults pvc Configure ATM PVC parameters service-policy Configure QoS Service Policy shutdown Shutdown the selected interface snapshot Configure snapshot support on the interface snmp Modify SNMP interface parameters standby Interface HSRP configuration commands timeout Define timeout values for this interface transmit-interface Assign a transmit interface to a receive-only interface ATM virtual circuit configuration commands: atm atm pvc commands broadcast Pseudo-broadcast cbr Enter Average Cell Rate in Kbps. class-vc Configure default vc-class name default Set a command to its defaults dialer set dialer pool this pvc belongs to encapsulation Select ATM Encapsulation for VC exit-vc Exit from ATM VC configuration mode ilmi Configure ILMI management inarp Change the inverse arp timer on the PVC no Negate a command or set its defaults oam Configure oam parameters oam-pvc Send oam cells on this pvc pppoe-client pppoe client protocol Map an upper layer protocol to this connection. random-detect Configure WRED service-policy Attach a policy-map to a VC tx-ring-limit Configure PA level transmit ring limit ubr Enter Unspecified Peak Cell Rate (pcr) in Kbps. vbr-nrt Enter Variable Bit Rate (pcr)(scr)(bcs) vbr-rt Enter Variable Bit Rate (pcr)(average) vcci VCC Identifier