Content

| 4.3 |  | Verifying RIP v2 Operation |
| 4.3.1 |  | Show commands |

Use the show ip protocols command to verify which routes the routing protocols are summarized for an interface carried on a router.

> Router#show ip protocols

Use the show ip rip database command to check summary address entries in the RIP database. These entries will appear in the database if there are only relevant child or specific routes being summarized. When the last child route for a summary address becomes invalid, the summary address is also removed from the routing table.

> Router#show ip rip database

Use the

show ip route EXEC command to display the current state of the routing table.

> Router#show ip route [address [mask] [longer-prefixes]] | [protocol [process-id]] | [list access-list-number | access-list-name]

| Lab Activity e-Lab Activity: Show Commands This lab is to lean some of show commands and what information they can present.

| Web Links Configuring RIP http://www.cisco.com/en/US/products/ sw/iosswrel/ps1828/products_configuration_ guide_chapter09186a00800ca569.htm