Output=RTC%23show+running%2Dconfig%0Aip+subnet%2Dzero%0Ainterface+Serial2%2F1%0Aip+address+172%2E16%2E20%2E1+255%2E255%2E255%2E0%0Arouter+bgp+1%0Aneighbor+172%2E16%2E20%2E2+remote%2Das+3%0Ano+auto%2Dsummary%0Aip+classless%0ARTC%23%0A