Output=RTA%23show+running%2Dconfig%0Aip+subnet%2Dzero%0Ainterface+Loopback0%0Aip+address+172%2E16%2E2%2E254+255%2E255%2E255%2E255%0Ainterface+Ethernet1%0Aip+address+172%2E16%2E1%2E1+255%2E255%2E255%2E0%0Ainterface+Serial0%0Aip+address+172%2E16%2E20%2E2+255%2E255%2E255%2E0%0Arouter+ospf+10%0Anetwork+172%2E16%2E0%2E0+0%2E0%2E255%2E255+area+0%0Arouter+bgp+3%0Ano+synchronization%0Aneighbor+172%2E16%2E1%2E2+remote%2Das+3%0Aneighbor+172%2E16%2E1%2E2+update%2Dsource+Loopback0%0Aneighbor+172%2E16%2E20%2E1+remote%2Das+1%0Ano+auto%2Dsummary%0Aip+classless%0ARTA%23%0A