Output=RouterE%23show+running%2Dconfig%0Ainterface+Serial0%0Aip+address+203%2E250%2E15%2E2+255%2E255%2E255%2E252%0A%0Arouter+ospf+10%0Anetwork+203%2E250%2E15%2E0+0%2E0%2E0%2E255+area+2%0A%0ARouterE%23%0A