
subintVlanC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
subintVlanC.addSC("bandwidth", "Set bandwidth informational parameter");
	subintVlanC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
subintVlanC.addSC("carrier-delay", "Specify delay for interface transitions");
subintVlanC.addSC("cdp", "CDP interface subcommands");
subintVlanC.addSC("default", "Set a command to its defaults");
subintVlanC.addSC("delay", "Specify interface throughput delay");
subintVlanC.addSC("description", "Interface specific description");
subintVlanC.addSC("exit", "Exit from interface configuration mode");
subintVlanC.addSC("ip", "Interface Internet Protocol config commands");
	subintVlanC.ip.addSC("access-group", "Specify access control for packets");
	subintVlanC.ip.addSC("accounting", "Enable IP accounting on this interface");
	subintVlanC.ip.addSC("address", "Set the IP address of an interface");
		subintVlanC.ip.address.addSC("A.B.C.D", "IP address");
			subintVlanC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				subintVlanC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	subintVlanC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	subintVlanC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
	subintVlanC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
	subintVlanC.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
	subintVlanC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	subintVlanC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
	subintVlanC.ip.addSC("probe", "Enable HP Probe support");
	subintVlanC.ip.addSC("proxy-arp", "Enable proxy ARP");
	subintVlanC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
	subintVlanC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	subintVlanC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
	subintVlanC.ip.addSC("security", "DDN IP Security Option");
	subintVlanC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	subintVlanC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	subintVlanC.ip.addSC("verify", "Enable per packet validation");
subintVlanC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
subintVlanC.addSC("no", "Negate a command or set its defaults");
	subintVlanC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintVlanC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	subintVlanC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	subintVlanC.no.addSC("cdp", "CDP interface subcommands");
	subintVlanC.no.addSC("delay", "Specify interface throughput delay");
	subintVlanC.no.addSC("description", "Interface specific description");
	subintVlanC.no.addSC("ip", "Interface Internet Protocol config commands");
		subintVlanC.no.ip.addSC("access-group", "Specify access control for packets");
		subintVlanC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
		subintVlanC.no.ip.addSC("address", "Set the IP address of an interface");
			subintVlanC.no.ip.address.addSC("A.B.C.D", "IP address");
				subintVlanC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					subintVlanC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		subintVlanC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		subintVlanC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		subintVlanC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		subintVlanC.no.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
		subintVlanC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		subintVlanC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		subintVlanC.no.ip.addSC("probe", "Enable HP Probe support");
		subintVlanC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		subintVlanC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		subintVlanC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		subintVlanC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		subintVlanC.no.ip.addSC("security", "DDN IP Security Option");
		subintVlanC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		subintVlanC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		subintVlanC.no.ip.addSC("verify", "Enable per packet validation");
	subintVlanC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
subintVlanC.addSC("ntp", "Configure NTP");
subintVlanC.addSC("service-policy", "Configure QoS Service Policy");
subintVlanC.addSC("shutdown", "Shutdown the selected interface");
subintVlanC.addSC("standby", "Hot standby interface subcommands");
subintVlanC.addSC("timeout", "Define timeout values for this interface");
