
routerEIGRPC.addSC("auto-summary", "Enable automatic network number summarization");
routerEIGRPC.addSC("default", "Set a command to its defaults");
	routerEIGRPC["default"].addSC("auto-summary", "Enable automatic network number summarization");
routerEIGRPC.addSC("default-information", "Control distribution of default information");
	routerEIGRPC["default-information"].addSC("allowed", "Allow default information");
	routerEIGRPC["default-information"].addSC("in", "Accept default routing information");
	routerEIGRPC["default-information"].addSC("out", "Output default routing information");
		routerEIGRPC["default-information"].out.addSC("<1-99>", "A standard IP access list number");
		routerEIGRPC["default-information"].out.addSC("<1300-1999>", "A standard expanded IP access list number");
		routerEIGRPC["default-information"].out.addSC("WORD", "Standard Access-list name");
routerEIGRPC.addSC("default-metric", "Set metric of redistributed routes");
	routerEIGRPC["default-metric"].addSC("<1-4294967295>", "Bandwidth in Kbits per second");
		routerEIGRPC["default-metric"]["<1-4294967295>"].addSC("<0-4294967295>", "Delay metric, in 10 microsecond units");
routerEIGRPC.addSC("distance", "Define an administrative distance");
	routerEIGRPC.distance.addSC("<1-255>", "Administrative distance");
		routerEIGRPC.distance["<1-255>"].addSC("A.B.C.D", "IP Source address");
			routerEIGRPC.distance["<1-255>"]["A.B.C.D"].addSC("A.B.C.D", "IP address mask");
				routerEIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-99>", "IP Standard access list number");
				routerEIGRPC.distance["<1-255>"]["A.B.C.D"]["A.B.C.D"].addSC("<1300-1999>", "IP Standard expanded access list number");
	routerEIGRPC.distance.addSC("eigrp", "IP-EIGRP distance");
		routerEIGRPC.distance.eigrp.addSC("<1-255>", "Distance for internal routes");
			routerEIGRPC.distance.eigrp["<1-255>"].addSC("<1-255>", "Distance for external routes");
routerEIGRPC.addSC("distribute-list", "Filter networks in routing updates");
	routerEIGRPC["distribute-list"].addSC("<1-199>", "IP access list number");
		routerEIGRPC["distribute-list"]["<1-199>"].addSC("in", "Filter incoming routing updates");
		routerEIGRPC["distribute-list"]["<1-199>"].addSC("out", "Filter outgoing routing updates");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Async", "Async interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Async.addSC("<1-5>", "Async interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("BVI", "Bridge-Group Virtual Interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.BVI.addSC("<1-255>", "BVI interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("CTunnel", "CTunnel interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Dialer", "Dialer interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Dialer.addSC("<0-255>", "Dialer interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				routerEIGRPC["distribute-list"]["<1-199>"].out.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Lex", "Lex interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Lex.addSC("<0-2147483647>", "Lex interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("MFR", "Multilink Frame Relay bundle interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.MFR.addSC("<0-2147483647>", "MFR interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Multilink", "Multilink-group interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Multilink.addSC("<1-2147483647>", "Multilink interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Serial", "Serial");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Serial.addSC("<0-1>", "Serial interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Tunnel", "Tunnel interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Vif", "PGM Multicast Host interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out.Vif.addSC("<1-1>", "Vif interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Virtual-Template", "Virtual Template interface");
				routerEIGRPC["distribute-list"]["<1-199>"].out["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("Virtual-TokenRing", "Virtual TokenRing");
				routerEIGRPC["distribute-list"]["<1-199>"].out["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("connected", "Connected");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerEIGRPC["distribute-list"]["<1-199>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerEIGRPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerEIGRPC["distribute-list"]["<1-199>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerEIGRPC["distribute-list"]["<1-199>"].out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("<1300-2699>", "IP expanded access list number");
		routerEIGRPC["distribute-list"]["<1300-2699>"].addSC("in", "Filter incoming routing updates");
		routerEIGRPC["distribute-list"]["<1300-2699>"].addSC("out", "Filter outgoing routing updates");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Async", "Async interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Async.addSC("<1-5>", "Async interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("BVI", "Bridge-Group Virtual Interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.BVI.addSC("<1-255>", "BVI interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("CTunnel", "CTunnel interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Dialer", "Dialer interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Dialer.addSC("<0-255>", "Dialer interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Lex", "Lex interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Lex.addSC("<0-2147483647>", "Lex interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("MFR", "Multilink Frame Relay bundle interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.MFR.addSC("<0-2147483647>", "MFR interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Multilink", "Multilink-group interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Multilink.addSC("<1-2147483647>", "Multilink interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Serial", "Serial");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Serial.addSC("<0-1>", "Serial interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Tunnel", "Tunnel interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Vif", "PGM Multicast Host interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.Vif.addSC("<1-1>", "Vif interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Virtual-Template", "Virtual Template interface");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("Virtual-TokenRing", "Virtual TokenRing");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("connected", "Connected");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerEIGRPC["distribute-list"]["<1300-2699>"].out.ospf.addSC("<1-65535>", "Process ID");
					routerEIGRPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerEIGRPC["distribute-list"]["<1300-2699>"].out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("rip", "Routing Information Protocol (RIP)");
			routerEIGRPC["distribute-list"]["<1300-2699>"].out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("WORD", "Access-list name");
		routerEIGRPC["distribute-list"].WORD.addSC("in", "Filter incoming routing updates");
		routerEIGRPC["distribute-list"].WORD.addSC("out", "Filter outgoing routing updates");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Async", "Async interface");
				routerEIGRPC["distribute-list"].WORD.out.Async.addSC("<1-5>", "Async interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("BVI", "Bridge-Group Virtual Interface");
				routerEIGRPC["distribute-list"].WORD.out.BVI.addSC("<1-255>", "BVI interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("CTunnel", "CTunnel interface");
				routerEIGRPC["distribute-list"].WORD.out.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Dialer", "Dialer interface");
				routerEIGRPC["distribute-list"].WORD.out.Dialer.addSC("<0-255>", "Dialer interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("FastEthernet", "FastEthernet IEEE 802.3");
				routerEIGRPC["distribute-list"].WORD.out.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Lex", "Lex interface");
				routerEIGRPC["distribute-list"].WORD.out.Lex.addSC("<0-2147483647>", "Lex interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Loopback", "Loopback interface");
				routerEIGRPC["distribute-list"].WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("MFR", "Multilink Frame Relay bundle interface");
				routerEIGRPC["distribute-list"].WORD.out.MFR.addSC("<0-2147483647>", "MFR interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Multilink", "Multilink-group interface");
				routerEIGRPC["distribute-list"].WORD.out.Multilink.addSC("<1-2147483647>", "Multilink interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Null", "Null interface");
				routerEIGRPC["distribute-list"].WORD.out.Null.addSC("<0-0>", "Null interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Serial", "Serial");
				routerEIGRPC["distribute-list"].WORD.out.Serial.addSC("<0-1>", "Serial interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Tunnel", "Tunnel interface");
				routerEIGRPC["distribute-list"].WORD.out.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Vif", "PGM Multicast Host interface");
				routerEIGRPC["distribute-list"].WORD.out.Vif.addSC("<1-1>", "Vif interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Virtual-Template", "Virtual Template interface");
				routerEIGRPC["distribute-list"].WORD.out["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("Virtual-TokenRing", "Virtual TokenRing");
				routerEIGRPC["distribute-list"].WORD.out["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
				routerEIGRPC["distribute-list"].WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("connected", "Connected");
			routerEIGRPC["distribute-list"].WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
				routerEIGRPC["distribute-list"].WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				routerEIGRPC["distribute-list"].WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				routerEIGRPC["distribute-list"].WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
			routerEIGRPC["distribute-list"].WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
				routerEIGRPC["distribute-list"].WORD.out.ospf.addSC("<1-65535>", "Process ID");
					routerEIGRPC["distribute-list"].WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
						routerEIGRPC["distribute-list"].WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
			routerEIGRPC["distribute-list"].WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
			routerEIGRPC["distribute-list"].WORD.out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("gateway", "Filtering incoming updates based on gateway");
		routerEIGRPC["distribute-list"].gateway.addSC("WORD", "Name of an IP prefix-list");
			routerEIGRPC["distribute-list"].gateway.WORD.addSC("in", "Filter incoming routing updates");
			routerEIGRPC["distribute-list"].gateway.WORD.addSC("out", "Filter outgoing routing updates");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Async", "Async interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Async.addSC("<1-5>", "Async interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("BVI", "Bridge-Group Virtual Interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.BVI.addSC("<1-255>", "BVI interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("CTunnel", "CTunnel interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Dialer", "Dialer interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Dialer.addSC("<0-255>", "Dialer interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("FastEthernet", "FastEthernet IEEE 802.3");
					routerEIGRPC["distribute-list"].gateway.WORD.out.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Lex", "Lex interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Lex.addSC("<0-2147483647>", "Lex interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Loopback", "Loopback interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("MFR", "Multilink Frame Relay bundle interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.MFR.addSC("<0-2147483647>", "MFR interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Multilink", "Multilink-group interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Null", "Null interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Serial", "Serial");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Serial.addSC("<0-1>", "Serial interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Tunnel", "Tunnel interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Vif", "PGM Multicast Host interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out.Vif.addSC("<1-1>", "Vif interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Virtual-Template", "Virtual Template interface");
					routerEIGRPC["distribute-list"].gateway.WORD.out["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("Virtual-TokenRing", "Virtual TokenRing");
					routerEIGRPC["distribute-list"].gateway.WORD.out["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("connected", "Connected");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerEIGRPC["distribute-list"].gateway.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerEIGRPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerEIGRPC["distribute-list"].gateway.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerEIGRPC["distribute-list"].gateway.WORD.out.addSC("static", "Static routes");
	routerEIGRPC["distribute-list"].addSC("prefix", "Filter prefixes in routing updates");
		routerEIGRPC["distribute-list"].prefix.addSC("WORD", "Name of an IP prefix-list");
			routerEIGRPC["distribute-list"].prefix.WORD.addSC("gateway", "Filtering incoming updates based on gateway");
			routerEIGRPC["distribute-list"].prefix.WORD.addSC("in", "Filter incoming routing updates");
			routerEIGRPC["distribute-list"].prefix.WORD.addSC("out", "Filter outgoing routing updates");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Async", "Async interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Async.addSC("<1-5>", "Async interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("BVI", "Bridge-Group Virtual Interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.BVI.addSC("<1-255>", "BVI interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("CTunnel", "CTunnel interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Dialer", "Dialer interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Dialer.addSC("<0-255>", "Dialer interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("FastEthernet", "FastEthernet IEEE 802.3");
					routerEIGRPC["distribute-list"].prefix.WORD.out.FastEthernet.addSC("<0-0>", "FastEthernet interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Lex", "Lex interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Lex.addSC("<0-2147483647>", "Lex interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Loopback", "Loopback interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("MFR", "Multilink Frame Relay bundle interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.MFR.addSC("<0-2147483647>", "MFR interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Multilink", "Multilink-group interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Multilink.addSC("<1-2147483647>", "Multilink interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Null", "Null interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Null.addSC("<0-0>", "Null interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Serial", "Serial");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Serial.addSC("<0-1>", "Serial interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Tunnel", "Tunnel interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Vif", "PGM Multicast Host interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out.Vif.addSC("<1-1>", "Vif interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Virtual-Template", "Virtual Template interface");
					routerEIGRPC["distribute-list"].prefix.WORD.out["Virtual-Template"].addSC("<1-200>", "Virtual-Template interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("Virtual-TokenRing", "Virtual TokenRing");
					routerEIGRPC["distribute-list"].prefix.WORD.out["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("bgp", "Border Gateway Protocol (BGP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.bgp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("connected", "Connected");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("egp", "Exterior Gateway Protocol (EGP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.egp.addSC("<0-65535>", "Remote autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.eigrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.igrp.addSC("<1-65535>", "Autonomous system number");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("ospf", "Open Shortest Path First (OSPF)");
					routerEIGRPC["distribute-list"].prefix.WORD.out.ospf.addSC("<1-65535>", "Process ID");
						routerEIGRPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
							routerEIGRPC["distribute-list"].prefix.WORD.out.ospf["<1-65535>"].vrf.addSC("WORD", "VPN Routing/Forwarding Instance (VRF) name");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("rip", "Routing Information Protocol (RIP)");
				routerEIGRPC["distribute-list"].prefix.WORD.out.addSC("static", "Static routes");
routerEIGRPC.addSC("eigrp", "EIGRP specific commands");
	routerEIGRPC.eigrp.addSC("log-neighbor-changes", "Enable/Disable IP-EIGRP neighbor logging");
	routerEIGRPC.eigrp.addSC("log-neighbor-warnings", "Enable/Disable IP-EIGRP neighbor warnings");
		routerEIGRPC.eigrp["log-neighbor-warnings"].addSC("<1-65535>", "Neighbor warning interval in seconds");
	routerEIGRPC.eigrp.addSC("router-id", "router-id for this EIGRP process");
		routerEIGRPC.eigrp["router-id"].addSC("A.B.C.D", "EIGRP Router-ID in IP address format");
	routerEIGRPC.eigrp.addSC("stub", "Set IP-EIGRP as stubbed router");
		routerEIGRPC.eigrp.stub.addSC("connected", "Do advertise connected routes");
		routerEIGRPC.eigrp.stub.addSC("receive-only", "Set IP-EIGRP as receive only neighbor");
		routerEIGRPC.eigrp.stub.addSC("static", "Do advertise static routes");
			routerEIGRPC.eigrp.stub.static.addSC("connected", "Do advertise connected routes");
		routerEIGRPC.eigrp.stub.addSC("summary", "Do advertise summary routes");
			routerEIGRPC.eigrp.stub.summary.addSC("connected", "Do advertise connected routes");
			routerEIGRPC.eigrp.stub.summary.addSC("static", "Do advertise static routes");
				routerEIGRPC.eigrp.stub.summary.static.addSC("connected", "Do advertise connected routes");
routerEIGRPC.addSC("exit", "Exit from routing protocol configuration mode");
routerEIGRPC.addSC("help", "Description of the interactive help system");
routerEIGRPC.addSC("maximum-paths", "Forward packets over multiple paths");
	routerEIGRPC["maximum-paths"].addSC("<1-6>", "Number of paths");
routerEIGRPC.addSC("metric", "Modify IGRP routing metrics and parameters");
	routerEIGRPC.metric.addSC("holddown", "Enable IGRP holddown");
	routerEIGRPC.metric.addSC("maximum-hops", "Advertise IGRP routes greater than <hops> as unreachable");
		routerEIGRPC.metric["maximum-hops"].addSC("<1-255>", "Hop count");
	routerEIGRPC.metric.addSC("weights", "Modify IGRP metric coefficients");
		routerEIGRPC.metric.weights.addSC("<0-8>", "Type Of Service (Only TOS 0 supported)");
			routerEIGRPC.metric.weights["<0-8>"].addSC("<0-4294967295>", "K1");
				routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"].addSC("<0-4294967295>", "K2");
					routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K3");
						routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K4");
							routerEIGRPC.metric.weights["<0-8>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"]["<0-4294967295>"].addSC("<0-4294967295>", "K5");
routerEIGRPC.addSC("neighbor", "Specify a neighbor router");
	routerEIGRPC.neighbor.addSC("A.B.C.D", "Neighbor address");
routerEIGRPC.addSC("network", "Enable routing on an IP network");
	routerEIGRPC.network.addSC("A.B.C.D", "Network number");
		routerEIGRPC.network["A.B.C.D"].addSC("A.B.C.D", "EIGRP wild card bits");
routerEIGRPC.addSC("no", "Negate a command or set its defaults");
routerEIGRPC.addSC("offset-list", "Add or subtract offset from IGRP or RIP metrics");
	routerEIGRPC["offset-list"].addSC("<0-99>", "Access list of networks to apply offset (0 selects all networks)");
		routerEIGRPC["offset-list"]["<0-99>"].addSC("in", "Perform offset on incoming updates");
		routerEIGRPC["offset-list"]["<0-99>"].addSC("out", "Perform offset on outgoing updates");
	routerEIGRPC["offset-list"].addSC("<1300-1999>", "Access list of networks to apply offset (expanded range)");
		routerEIGRPC["offset-list"]["<1300-1999>"].addSC("in", "Perform offset on incoming updates");
		routerEIGRPC["offset-list"]["<1300-1999>"].addSC("out", "Perform offset on outgoing updates");
	routerEIGRPC["offset-list"].addSC("WORD", "Access-list name");
		routerEIGRPC["offset-list"].WORD.addSC("in", "Perform offset on incoming updates");
		routerEIGRPC["offset-list"].WORD.addSC("out", "Perform offset on outgoing updates");
routerEIGRPC.addSC("passive-interface", "Suppress routing updates on an interface");
routerEIGRPC.addSC("redistribute", "Redistribute information from another routing protocol");
routerEIGRPC.addSC("timers", "Adjust routing timers");
	routerEIGRPC.timers.addSC("active-time", "EIGRP time limit for active state");
		routerEIGRPC.timers["active-time"].addSC("<1-4294967295>", "EIGRP active-state time limit in minutes");
		routerEIGRPC.timers["active-time"].addSC("disabled", "disable EIGRP time limit for active state");
routerEIGRPC.addSC("traffic-share", "How to compute traffic share over alternate paths");
	routerEIGRPC["traffic-share"].addSC("balanced", "Share inversely proportional to metric");
	routerEIGRPC["traffic-share"].addSC("min", "All traffic shared among min metric paths");
		routerEIGRPC["traffic-share"].min.addSC("across-interfaces", "Use different interfaces for equal-cost paths");
routerEIGRPC.addSC("variance", "Control load balancing variance");
	routerEIGRPC.variance.addSC("<1-128>", "Metric variance multiplier");
