Output=RouterC%23show+ip+route%0A%0ACodes%3A+C+%2D+connected%2C+S+%2D+static%2C+I+%2D+IGRP%2C+R+%2D+RIP%2C+M+%2D+mobile%2C+B+%2D+BGP%0AD+%2D+EIGRP%2C+EX+%2D+EIGRP+external%2C+O+%2D+OSPF%2C+IA+%2D+OSPF+inter+area%0AE1+%2D+OSPF+external+type+1%2C+E2+%2D+OSPF+external+type+2%2C+E+%2D+EGP%0Ai+%2D+IS%2DIS%2C+L1+%2D+IS%2DIS+level%2D1%2C+L2+%2D+IS%2DIS+level%2D2%2C+%2A+%2D+candidate+default%0A%0AGateway+of+last+resort+is+168%2E71%2E9%2E1+to+network+10%2E0%2E0%2E0%0A%0AI%2A+10%2E0%2E0%2E0+%5B100%2F82125%5D+via+168%2E71%2E9%2E1%2C+00%3A01%3A06%2C+Serial1%0A168%2E71%2E0%2E0+255%2E255%2E255%2E0+is+subnetted%2C+5+subnets%0AC+168%2E71%2E9%2E0+is+directly+connected%2C+Serial1%0AC+168%2E71%2E8%2E0+is+directly+connected%2C+Ethernet0%0AC+168%2E71%2E7%2E0+is+directly+connected%2C+Serial0%0AI+168%2E71%2E5%2E0+%5B100%2F10002001%5D+via+168%2E71%2E9%2E1%2C+00%3A01%3A07%2C+Serial1%0A%0ARouterC%23%0A