
routeMapC.addSC("default", "Set a command to its defaults");
routeMapC.addSC("description", "Route-map comment");
	routeMapC.description.addSC("LINE", "Comment up to 100 characters");
routeMapC.addSC("exit", "Exit from route-map configuration mode");
routeMapC.addSC("help", "Description of the interactive help system");
routeMapC.addSC("match", "Match values from routing table");
	
routeMapC.addSC("no", "Negate a command or set its defaults");
	routeMapC.no.addSC("description", "Route-map comment");
	routeMapC.no.addSC("match", "Match values from routing table");
		
routeMapC.addSC("set", "Set values in destination routing protocol");
	routeMapC.set.addSC("as-path", "Prepend string for a BGP AS-path attribute");
		routeMapC.set["as-path"].addSC("prepend", "Prepend to the as-path");
			routeMapC.set["as-path"].prepend.addSC("<1-65535>", "AS number");
		routeMapC.set["as-path"].addSC("tag", "Set the tag as an AS-path attribute");
	routeMapC.set.addSC("automatic-tag", "Automatically compute TAG value");
	routeMapC.set.addSC("comm-list", "set BGP community list (for deletion)");
		routeMapC.set["comm-list"].addSC("<1-99>", "Community-list number (standard)");
			routeMapC.set["comm-list"]["<1-99>"].addSC("delete", "Delete matching communities");
		routeMapC.set["comm-list"].addSC("<100-199>", "Communitly-list number (expanded)");
			routeMapC.set["comm-list"]["<100-199>"].addSC("delete", "Delete matching communities");
		routeMapC.set["comm-list"].addSC("WORD", "Community-list name");
			routeMapC.set["comm-list"].WORD.addSC("delete", "Delete matching communities");
	routeMapC.set.addSC("community", "BGP community attribute");
		routeMapC.set.community.addSC("<1-4294967295>", "community number");
		routeMapC.set.community.addSC("aa:nn", "community number in aa:nn format");
		routeMapC.set.community.addSC("additive", "Add to the existing community");
		routeMapC.set.community.addSC("local-AS", "Do not send outside local AS (well-known community)");
			routeMapC.set.community["local-AS"].addSC("<1-4294967295>", "community number");
			routeMapC.set.community["local-AS"].addSC("aa:nn", "community number in aa:nn format");
			routeMapC.set.community["local-AS"].addSC("additive", "Add to the existing community");
		routeMapC.set.community.addSC("no-advertise", "Do not advertise to any peer (well-known community)");
			routeMapC.set.community["no-advertise"].addSC("<1-4294967295>", "community number");
			routeMapC.set.community["no-advertise"].addSC("aa:nn", "community number in aa:nn format");
			routeMapC.set.community["no-advertise"].addSC("additive", "Add to the existing community");
			routeMapC.set.community["no-advertise"].addSC("local-AS", "Do not send outside local AS (well-known community)");
				routeMapC.set.community["no-advertise"]["local-AS"].addSC("<1-4294967295>", "community number");
				routeMapC.set.community["no-advertise"]["local-AS"].addSC("aa:nn", "community number in aa:nn format");
				routeMapC.set.community["no-advertise"]["local-AS"].addSC("additive", "Add to the existing community");
		routeMapC.set.community.addSC("no-export", "Do not export to next AS (well-known community)");
			routeMapC.set.community["no-export"].addSC("<1-4294967295>", "community number");
			routeMapC.set.community["no-export"].addSC("aa:nn", "community number in aa:nn format");
			routeMapC.set.community["no-export"].addSC("additive", "Add to the existing community");
			routeMapC.set.community["no-export"].addSC("local-AS", "Do not send outside local AS (well-known community)");
				routeMapC.set.community["no-export"]["local-AS"].addSC("<1-4294967295>", "community number");
				routeMapC.set.community["no-export"]["local-AS"].addSC("aa:nn", "community number in aa:nn format");
				routeMapC.set.community["no-export"]["local-AS"].addSC("additive", "Add to the existing community");
			routeMapC.set.community["no-export"].addSC("no-advertise", "Do not advertise to any peer (well-known community)");
				routeMapC.set.community["no-export"]["no-advertise"].addSC("<1-4294967295>", "community number");
				routeMapC.set.community["no-export"]["no-advertise"].addSC("aa:nn", "community number in aa:nn format");
				routeMapC.set.community["no-export"]["no-advertise"].addSC("additive", "Add to the existing community");
				routeMapC.set.community["no-export"]["no-advertise"].addSC("local-AS", "Do not send outside local AS (well-known community)");
					routeMapC.set.community["no-export"]["no-advertise"]["local-AS"].addSC("<1-4294967295>", "community number");
					routeMapC.set.community["no-export"]["no-advertise"]["local-AS"].addSC("aa:nn", "community number in aa:nn format");
					routeMapC.set.community["no-export"]["no-advertise"]["local-AS"].addSC("additive", "Add to the existing community");
		routeMapC.set.community.addSC("none", "No community attribute");
	routeMapC.set.addSC("dampening", "Set BGP route flap dampening parameters");
		routeMapC.set.dampening.addSC("<1-45>", "half-life time for the penalty");
			routeMapC.set.dampening["<1-45>"].addSC("<1-20000>", "penalty to start reusing a route");
				routeMapC.set.dampening["<1-45>"]["<1-20000>"].addSC("<1-20000>", "penalty to start suppressing a route");
					routeMapC.set.dampening["<1-45>"]["<1-20000>"]["<1-20000>"].addSC("<1-255>", "Maximum duration to suppress a stable route");
	routeMapC.set.addSC("extcommunity", "BGP extended community attribute");
		routeMapC.set.extcommunity.addSC("rt", "Route Target extended community");
			routeMapC.set.extcommunity.rt.addSC("ASN:nn or IP-address:nn", "VPN extended community");
		routeMapC.set.extcommunity.addSC("soo", "Site-of-Origin extended community");
			routeMapC.set.extcommunity.soo.addSC("ASN:nn or IP-address:nn", "VPN extended community");
	routeMapC.set.addSC("interface", "Output interface");
		routeMapC.set.interface.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
			routeMapC.set.interface["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
		routeMapC.set.interface.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
			routeMapC.set.interface.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
		routeMapC.set.interface.addSC("Loopback", "Loopback interface");
			routeMapC.set.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
		routeMapC.set.interface.addSC("Null", "Null interface");
			routeMapC.set.interface.Null.addSC("<0-0>", "Null interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routeMapC.set.interface.Null["<0-0>"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routeMapC.set.interface.Null["<0-0>"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routeMapC.set.interface.Null["<0-0>"].addSC("Loopback", "Loopback interface");
					routeMapC.set.interface.Null["<0-0>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
		routeMapC.set.interface.addSC("Vlan", "Catalyst Vlans");
			routeMapC.set.interface.Vlan.addSC("<1-1001>", "Vlan interface number");
				routeMapC.set.interface.Vlan["<1-1001>"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
					routeMapC.set.interface.Vlan["<1-1001>"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
				routeMapC.set.interface.Vlan["<1-1001>"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
					routeMapC.set.interface.Vlan["<1-1001>"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
				routeMapC.set.interface.Vlan["<1-1001>"].addSC("Loopback", "Loopback interface");
					routeMapC.set.interface.Vlan["<1-1001>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
				routeMapC.set.interface.Vlan["<1-1001>"].addSC("Null", "Null interface");
					routeMapC.set.interface.Vlan["<1-1001>"].Null.addSC("<0-0>", "Null interface number");
						routeMapC.set.interface.Vlan["<1-1001>"].Null["<0-0>"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
							routeMapC.set.interface.Vlan["<1-1001>"].Null["<0-0>"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
						routeMapC.set.interface.Vlan["<1-1001>"].Null["<0-0>"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
							routeMapC.set.interface.Vlan["<1-1001>"].Null["<0-0>"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
						routeMapC.set.interface.Vlan["<1-1001>"].Null["<0-0>"].addSC("Loopback", "Loopback interface");
							routeMapC.set.interface.Vlan["<1-1001>"].Null["<0-0>"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
	routeMapC.set.addSC("ip", "IP specific information");
		routeMapC.set.ip.addSC("df", "Set DF bit");
			routeMapC.set.ip.df.addSC("<0-1>", "DF bit");
		routeMapC.set.ip.addSC("next-hop", "Next hop address");
			routeMapC.set.ip["next-hop"].addSC("A.B.C.D", "IP address of next hop");
			routeMapC.set.ip["next-hop"].addSC("peer-address", "Use peer address (for BGP only)");
			routeMapC.set.ip["next-hop"].addSC("verify-availability", "Verify if nexthop is a CDP neighbor");
		routeMapC.set.ip.addSC("precedence", "Set precedence field");
			
		routeMapC.set.ip.addSC("qos-group", "Set QOS Group ID");
			routeMapC.set.ip["qos-group"].addSC("<0-99>", "QOS Group ID");
	routeMapC.set.addSC("level", "Where to import route");
		routeMapC.set.level.addSC("backbone", "Import into OSPF backbone area");
		routeMapC.set.level.addSC("level-1", "Import into a level-1 area");
		routeMapC.set.level.addSC("level-1-2", "Import into level-1 and level-2");
		routeMapC.set.level.addSC("level-2", "Import into level-2 sub-domain");
		routeMapC.set.level.addSC("stub-area", "Import into OSPF NSSA area");
	routeMapC.set.addSC("local-preference", "BGP local preference path attribute");
		routeMapC.set["local-preference"].addSC("<0-4294967295>", "Preference value");
	routeMapC.set.addSC("metric", "Metric value for destination routing protocol");
		routeMapC.set.metric.addSC("+/-<metric>", "Add or subtract metric");
		routeMapC.set.metric.addSC("<0-4294967295>", "Metric value or Bandwidth in Kbits per second");
			routeMapC.set.metric["<0-4294967295>"].addSC("+/-<delay>", "Add or subtract delay");
			routeMapC.set.metric["<0-4294967295>"].addSC("<1-4294967295>", "IGRP delay metric, in 10 microsecond units");
				routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"].addSC("<0-255>", "IGRP reliability metric where 255 is 100% reliable");
					routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"]["<0-255>"].addSC("<1-255>", "IGRP Effective bandwidth metric (Loading) where 255 is 100% loaded");
						routeMapC.set.metric["<0-4294967295>"]["<1-4294967295>"]["<0-255>"]["<1-255>"].addSC("<1-4294967295>", "IGRP MTU of the path");
	routeMapC.set.addSC("metric-type", "Type of metric for destination routing protocol");
		routeMapC.set["metric-type"].addSC("external", "IS-IS external metric");
		routeMapC.set["metric-type"].addSC("internal", "Use IGP metric as the MED for BGP");
		routeMapC.set["metric-type"].addSC("type-1", "OSPF external type 1 metric");
		routeMapC.set["metric-type"].addSC("type-2", "OSPF external type 2 metric");
	routeMapC.set.addSC("origin", "BGP origin code");
		routeMapC.set.origin.addSC("egp", "remote EGP");
			routeMapC.set.origin.egp.addSC("<0-65535>", "remote AS");
		routeMapC.set.origin.addSC("igp", "local IGP");
		routeMapC.set.origin.addSC("incomplete", "unknown heritage");
	routeMapC.set.addSC("tag", "Tag value for destination routing protocol");
		routeMapC.set.tag.addSC("<0-4294967295>", "Tag value");
	routeMapC.set.addSC("traffic-index", "BGP traffic classification number for accounting");
		routeMapC.set["traffic-index"].addSC("<1-8>", "Bucket number");
	routeMapC.set.addSC("weight", "BGP weight for routing table");
		routeMapC.set.weight.addSC("<0-4294967295>", "Weight value");
