Commands

Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | CS 1 | CS 2 | CS 3 | All |

Module 8: Route Optimization

8.1.2

Passive Interfaces

> Router(config)#router rip
> Router(config-router)#network network number
> Router(config-router)#passive-interface type number

8.1.3

Filtering Routing Updates with Distribute-List

> Router(config-router)#distribute-list access-list-number in [interface-name]
> Router(config-router)#distribute-list access-list-number out [interface-name | routing-process | as-number]
> RTZ(config-router)#distribute-list access-list-number out
> Configuring a Passive EIGRP Interface Using distribute-list Command
> RTA(config)#router eigrp access-list-number
> RTA(config-router)#network network number
> RTA(config-router)#distribute-list access-list-number out interface interface-name
> RTA(config-router)#exit
> RTA(config)#access-list access-list-number deny any

8.3.4

Modifying Administrative Distance by Using the Distance Command

> Router(config-router)#distance weight {source-ip-address source-mask [access-list-number | name]}

8.3.6

Configuring one-way redistribution

> Router(config-router)#redistribute protocol [process-id] {level-1 | level-1-2 | level-2} [metric metric-value][metric-type type-value] [match {internal | external 1 | external 2}][tag tag-value] [route-map map-tag][weight weight] [subnets]

| Close Window |

| All contents copyright © 2003 Cisco Systems, Inc. All rights reserved.