Output=Router%2DC%23show+ip+bgp+neighbors%0ABGP+neighbor+is+3%2E0%2E0%2E1%2C++remote+AS+300%2C+external+link%0A++BGP+version+4%2C+remote+router+ID+10%2E0%2E0%2E1%0A++BGP+state+%3D+Established%2C+up+for+02%3A21%3A39%0A++Last+read+00%3A00%3A40%2C+hold+time+is+180%2C+keepalive+interval+is+60+seconds%0A++Neighbor+capabilities%3A%0A++++Route+refresh%3A+advertised+and+received%0A++++Address+family+IPv4+Unicast%3A+advertised+and+received%0A++Received+179+messages%2C+0+notifications%2C+0+in+queue%0A++Sent+177+messages%2C+0+notifications%2C+0+in+queue%0A++Route+refresh+request%3A+received+0%2C+sent+0%0A++Minimum+time+between+advertisement+runs+is+30+seconds%0A%0A+For+address+family%3A+IPv4+Unicast%0A++BGP+table+version+6%2C+neighbor+version+6%0A++Index+1%2C+Offset+0%2C+Mask+0x2%0A++2+accepted+prefixes+consume+72+bytes%0A++Prefix+advertised+4%2C+suppressed+0%2C+withdrawn+0%0A%0A++Connections+established+4%3B+dropped+3%0A++Last+reset+02%3A22%3A00%2C+due+to+User+reset%0AConnection+state+is+ESTAB%2C+I%2FO+status%3A+1%2C+unread+input+bytes%3A+0%0ALocal+host%3A+3%2E0%2E0%2E2%2C+Local+port%3A+11005%0AForeign+host%3A+3%2E0%2E0%2E1%2C+Foreign+port%3A+179%0A%0AEnqueued+packets+for+retransmit%3A+0%2C+input%3A+0++mis%2Dordered%3A+0+%280+bytes%29%0A%0AEvent+Timers+%28current+time+is+0xD9AC60%29%3A%0ATimer++++++++++Starts++++Wakeups++++++++++++Next%0ARetrans+++++++++++146++++++++++0+++++++++++++0x0%0ATimeWait++++++++++++0++++++++++0+++++++++++++0x0%0AAckHold+++++++++++148++++++++101+++++++++++++0x0%0ASendWnd+++++++++++++0++++++++++0+++++++++++++0x0%0AKeepAlive+++++++++++0++++++++++0+++++++++++++0x0%0AGiveUp++++++++++++++0++++++++++0+++++++++++++0x0%0APmtuAger++++++++++++0++++++++++0+++++++++++++0x0%0ADeadWait++++++++++++0++++++++++0+++++++++++++0x0%0A%0Aiss%3A+2473456117++snduna%3A+2473458926++sndnxt%3A+2473458926+++++sndwnd%3A++15054%0Airs%3A+2496095970++rcvnxt%3A+2496098890++rcvwnd%3A++++++14929++delrcvwnd%3A+++1455%0A%0ASRTT%3A+300+ms%2C+RTTO%3A+607+ms%2C+RTV%3A+3+ms%2C+KRTT%3A+0+ms%0AminRTT%3A+16+ms%2C+maxRTT%3A+300+ms%2C+ACK+hold%3A+200+ms%0AFlags%3A+higher+precedence%2C+nagle%0A%0ADatagrams+%28max+data+segment+is+1460+bytes%29%3A%0ARcvd%3A+199+%28out+of+order%3A+0%29%2C+with+data%3A+148%2C+total+data+bytes%3A+2919%0ASent%3A+249+%28retransmit%3A+0%29%2C+with+data%3A+145%2C+total+data+bytes%3A+2808%0ARouter%2DC%23%0A