Output=Router+C%23show+running%2Dconfig%0ARouter+C+Configuration%0Ainterface+serial+0%0Aip+address+170%2E10%2E63%2E3+255%2E255%2E255%2E0%0A%0Ainterface+serial+1%0Aip+address+170%2E10%2E64%2E3+255%2E255%2E255%2E0%0A%0Ainterface+ethernet+0%0Aip+address+170%2E10%2E24%2E3+255%2E255%2E255%2E0%0A%0Arouter+rip%0Anetwork+170%2E10%2E0%2E0%0A%0ARouter+C%23%0A++