Router A#show running-config
interface serial 0 
ip address 130.10.62.1 255.255.255.0 
interface serial 1 
ip address 130.10.63.1 255.255.255.0 
interface ethernet 0 
ip address 130.10.8.1 255.255.255.0 
interface tokenring 0 
ip address 130.10.9.1 255.255.255.0 
! 
router rip 
default-metric 10 
network 130.10.0.0 
passive-interface serial 0 
passive-interface serial 1 
redistribute ospf 109 match internal external 1 external 2 
! 
router ospf 109 
network 130.10.62.0 0.0.0.255 area 0 
network 130.10.63.0 0.0.0.255 area 0 
redistribute rip subnets 
distribute-list 11 out rip 
! 
access-list 11 permit 130.10.8.0 0.0.7.255 
access-list 11 deny 0.0.0.0 255.255.255.255 
Router A#
