
lineauxC.addSC("absolute-timeout", "Set absolute timeout for line disconnection");
lineauxC.addSC("access-class", "Filter connections based on an IP access list");
lineauxC.addSC("activation-character", "Define the activation character");
lineauxC.addSC("arap", "Appletalk Remote Access Protocol");
lineauxC.addSC("autobaud", "Set line to autobaud");
lineauxC.addSC("autocommand", "Automatically execute an EXEC command");
lineauxC.addSC("autocommand-options", "Autocommand options");
lineauxC.addSC("autohangup", "");
lineauxC.addSC("autoselect", "Set line to autoselect");
lineauxC.addSC("callback", "Callback settings");
lineauxC.addSC("data-character-bits", "Size of characters being handled");
lineauxC.addSC("databits", "Set number of data bits per character");
lineauxC.addSC("default", "Set a command to its defaults");
lineauxC.addSC("disconnect-character", "Define the disconnect character");
lineauxC.addSC("dispatch-character", "Define the dispatch character");
lineauxC.addSC("dispatch-machine", "Reference a TCP dispatch state machine");
lineauxC.addSC("dispatch-timeout", "Set the dispatch timer");
lineauxC.addSC("domain-lookup", "Enable domain lookups in show commands");
lineauxC.addSC("editing", "Enable command line editing");
lineauxC.addSC("escape-character", "Change the current line's escape character");
lineauxC.addSC("exec", "Start an EXEC process");
lineauxC.addSC("exec-banner", "Enable the display of the EXEC banner");
lineauxC.addSC("exec-character-bits", "Size of characters to the command exec");
lineauxC.addSC("exec-timeout", "Set the EXEC timeout");
   lineauxC["exec-timeout"].addSC("<0-35791>", "Timeout in minutes");
      lineauxC["exec-timeout"]["<0-35791>"].addSC("<0-2147483>", "Timeout in seconds");
lineauxC.addSC("exit", "Exit from line configuration mode");
lineauxC.addSC("flowcontrol", "Set the flow control");
   lineauxC.flowcontrol.addSC("NONE", "Set no flow control");
   lineauxC.flowcontrol.addSC("hardware", "Set hardware flow control");
      lineauxC.flowcontrol.hardware.addSC("in", "Listen to flow control from the attached device");
      lineauxC.flowcontrol.hardware.addSC("out", "Send flow control information to the attached device");
   lineauxC.flowcontrol.addSC("software", "Set software flow control");
lineauxC.addSC("flush-at-activation", "Clear input stream at activation");
lineauxC.addSC("full-help", "Provide help to unprivileged user");
lineauxC.addSC("help", "Description of the interactive help system");
lineauxC.addSC("history", "Enable and control the command history function");
lineauxC.addSC("hold-character", "Define the hold character");
lineauxC.addSC("insecure", "Mark line as 'insecure' for LAT");
lineauxC.addSC("international", "Enable international 8-bit character support");
lineauxC.addSC("ip", "IP options");
lineauxC.addSC("keymap-type", "Specify a keymap entry to use");
lineauxC.addSC("lat", "DEC Local Area Transport (LAT) protocol-specific configuration");
//lineauxC.addSC("length", "Set number of lines on a screen");
lineauxC.addSC("location", "Enter terminal location description");
lineauxC.addSC("lockable", "Allow users to lock a line");
lineauxC.addSC("logging", "Modify message logging facilities");
lineauxC.addSC("login", "Enable password checking");
   lineauxC.login.addSC("local", "Local password checking");
   lineauxC.login.addSC("tacacs", "Use tacacs server for password checking");
lineauxC.addSC("logout-warning", "Set Warning countdown for absolute timeout of line");
lineauxC.addSC("modem", "Configure the Modem Control Lines");
   lineauxC.modem.addSC("CTS-Alarm", "Alarm device which only uses CTS for call control");
   lineauxC.modem.addSC("DTR-active", "Leave DTR low unless line has an active incoming connection or EXEC");
   lineauxC.modem.addSC("Dialin", "Configure line for a modern dial-in modem");
   lineauxC.modem.addSC("Host", "Devices that expect an incoming modem call");
   lineauxC.modem.addSC("InOut", "Configure line for incoming AND outgoing use of modem");
   lineauxC.modem.addSC("Printer", "Devices that require DSR/CD active");
   lineauxC.modem.addSC("answer-timeout", "Set interval between the time the server raises DTR in response to RING and the modem responds to CTS");
   lineauxC.modem.addSC("autoconfigure", "Automatically configure modem on line");
   lineauxC.modem.addSC("busyout", "Block calls to and from the modem");
lineauxC.addSC("monitor", "Copy debug output to the current terminal line");
lineauxC.addSC("motd-banner", "Enable the display of the MOTD banner");
lineauxC.addSC("no", "Negate a command or set its defaults");
lineauxC.addSC("notify", "Inform users of output from concurrent sessions");
lineauxC.addSC("ntp", "Configure NTP");
lineauxC.addSC("padding", "Set padding for a specified output character");
lineauxC.addSC("parity", "Set terminal parity");
lineauxC.addSC("password", "Set a password");
   lineauxC.password.addSC("0", "Specifies an UNENCRYPTED password will follow");
   lineauxC.password.addSC("7", "Specifies a HIDDEN password will follow");
   lineauxC.password.addSC("LINE", "The UNENCRYPTED (cleartext) line password");
lineauxC.addSC("private", "Configuration options that user can set will remain in effect between terminal sessions");
lineauxC.addSC("privilege", "Change privilege level for line");
lineauxC.addSC("refuse-message", "Define a refuse banner");
lineauxC.addSC("rotary", "Add line to a rotary group");
lineauxC.addSC("rxspeed", "Set the receive speed");
lineauxC.addSC("script", "specify event related chat scripts to run on the line");
lineauxC.addSC("session-disconnect-warning", "Set warning countdown for session-timeout");
lineauxC.addSC("session-limit", "Set maximum number of sessions");
lineauxC.addSC("session-timeout", "Set interval for closing connection when there is no input traffic");
lineauxC.addSC("special-character-bits", "Size of the escape (and other special) characters");
lineauxC.addSC("speed", "Set the transmit and receive speeds");
   lineauxC.speed.addSC("<0-4294967295>", "Transmit and receive speeds");
lineauxC.addSC("start-character", "Define the start character");
lineauxC.addSC("stop-character", "Define the stop character");
lineauxC.addSC("stopbits", "Set async line stop bits");
   lineauxC.stopbits.addSC("1", "One stop bit");
   lineauxC.stopbits.addSC("1.5", "One and one-half stop bits");
   lineauxC.stopbits.addSC("2", "Two stop bits");
lineauxC.addSC("telnet", "Telnet protocol-specific configuration");
lineauxC.addSC("terminal-type", "Set the terminal type");
lineauxC.addSC("timeout", "Timeouts for the line");
lineauxC.addSC("transport", "Define transport protocols for line");
   lineauxC.transport.addSC("input", "Define which protocols to use when connecting to the terminal server");
      lineauxC.transport.input.addSC("all", "All protocols");
      lineauxC.transport.input.addSC("lat", "DEC LAT protocol");
      lineauxC.transport.input.addSC("mop", "DEC MOP Remote Console Protocol");
      lineauxC.transport.input.addSC("nasi", "NASI protocol");
      lineauxC.transport.input.addSC("none", "No protocols");
      lineauxC.transport.input.addSC("pad", "X.3 PAD");
      lineauxC.transport.input.addSC("rlogin", "Unix rlogin protocol");
      lineauxC.transport.input.addSC("telnet", "TCP/IP Telnet protocol");
      lineauxC.transport.input.addSC("udptn", "UDPTN async via UDP protocol");
      lineauxC.transport.input.addSC("v120", "Async over ISDN");
   lineauxC.transport.addSC("output", "Define which protocols to use for outgoing connections");
   lineauxC.transport.addSC("preferred", "Specify the preferred protocol to use");
lineauxC.addSC("txspeed", "Set the transmit speeds");
lineauxC.addSC("vacant-message", "Define a vacant banner");
lineauxC.addSC("width", "Set width of the display terminal");
lineauxC.addSC("x25", "X25 protocol-specific configuration");
