
enableC.addSC("access-enable", "Create a temporary Access-List entry");
enableC.addSC("access-profile", "Apply user-profile to interface");
enableC.addSC("access-template", "Create a temporary Access-List entry");
enableC.addSC("alps", "ALPS exec commands");
enableC.addSC("archive", "manage archive files");
enableC.addSC("audio-prompt", "load ivr prompt");
enableC.addSC("bfe", "For manual emergency modes setting");
enableC.addSC("cd", "Change current directory");
enableC.addSC("clear", "Reset functions");
   enableC.clear.addSC("dlsw", "Data Link Switching (DLSw)");
   enableC.clear.addSC("h323", "Clear H.323 protocol related information");
   enableC.clear.addSC("host", "Delete host table entries");
   enableC.clear.addSC("interface", "Clear the hardware logic on an interface");
   enableC.clear.addSC("ip", "IP");
      enableC.clear.ip.addSC("access-list", "Clear access list statistical information");
      enableC.clear.ip.addSC("access-template", "Access-template");
      enableC.clear.ip.addSC("accounting", "Clear IP accounting database");
      enableC.clear.ip.addSC("bgp", "Clear BGP connections");
      enableC.clear.ip.addSC("cache", "Delete cache table entries");
      enableC.clear.ip.addSC("eigrp", "Clear IP-EIGRP");
      enableC.clear.ip.addSC("igmp", "IGMP clear commands");
       enableC.clear.ip.addSC("nat", "Clear NAT");
         enableC.clear.ip.nat.addSC("statistics", "Clear translation statistics");
         enableC.clear.ip.nat.addSC("translation", "Clear dynamic translation");
            enableC.clear.ip.nat.translation.addSC("*", "Delete all dynamic translations");
            enableC.clear.ip.nat.translation.addSC("inside", "Inside addresses (and ports)");
            enableC.clear.ip.nat.translation.addSC("outside", "Outside addresses (and ports)");
            enableC.clear.ip.nat.translation.addSC("tcp", "Transmission Control Protocol");
            enableC.clear.ip.nat.translation.addSC("udp", "User Datagram Protocol");
       enableC.clear.ip.addSC("ospf", "OSPF clear commands");
       enableC.clear.ip.addSC("redirect", "Redirect cache");
      enableC.clear.ip.addSC("route", "Delete route table entries");
         enableC.clear.ip.route.addSC("*", "Delete all routes");
         enableC.clear.ip.route.addSC("A.B.C.D", "Destination network route to delete");
         enableC.clear.ip.route.addSC("vrf", "Clear routes for a VPN Routing/Forwarding instance");
      enableC.clear.ip.addSC("rsvp", "RSVP");
      enableC.clear.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
      enableC.clear.ip.addSC("sdr", "Session Directory (SDPv2) cache");
      enableC.clear.ip.addSC("trigger-authentication", "Clear trigger-authentication host table");
      enableC.clear.ip.addSC("wccp", "Reset wccp information");
   enableC.clear.addSC("ipx", "Reset Novell/IPX information");
   enableC.clear.addSC("isis", "Clear IS-IS data structures");
   enableC.clear.addSC("kerberos", "Clear Kerberos Values");
   enableC.clear.addSC("line", "Reset a terminal line");
   enableC.clear.addSC("logging", "Clear logging buffer");
   enableC.clear.addSC("tcp", "Clear a TCP connection or statistics");
enableC.addSC("clock", "Manage the system clock");
enableC.addSC("configure", "Enter configuration mode");
	enableC.configure.addSC("memory", "Configure from NV memory");
	enableC.configure.addSC("network", "Configure from a TFTP network host");
	enableC.configure.addSC("overwrite-network", "Overwrite NV memory from TFTP network host");
	enableC.configure.addSC("terminal", "Configure from the terminal");
enableC.addSC("connect", "Open a terminal connection");
enableC.addSC("copy", "Copy from one file to another");
   enableC.copy.addSC("/erase", "Erase destination file system.");
   enableC.copy.addSC("rcp:", "Copy from rcp: file system");
   enableC.copy.addSC("running-config", "Copy from current system configuration");
      enableC.copy["running-config"].addSC("running-config", "Update (merge with) current system configuration");
      enableC.copy["running-config"].addSC("startup-config", "Copy to startup configuration");
   enableC.copy.addSC("startup-config", "Copy from startup configuration");
enableC.addSC("debug", "Debugging functions (see also 'undebug')");
   enableC.debug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
   enableC.debug.addSC("all", "Enable all debugging");
   enableC.debug.addSC("ethernet-interface", "Ethernet network interface events");
   enableC.debug.addSC("fastethernet", "Fast Ethernet interface information");
   enableC.debug.addSC("frame-relay", "Frame Relay");
   enableC.debug.addSC("interface", "interface");
   enableC.debug.addSC("ip", "IP information");
      enableC.debug.ip.addSC("bgp", "BGP information");
      enableC.debug.ip.addSC("nat", "NAT events");
      enableC.debug.ip.addSC("ospf", "OSPF information");
         enableC.debug.ip.ospf.addSC("adj", "OSPF adjacency events");
         enableC.debug.ip.ospf.addSC("database-timer", "OSPF database timer");
         enableC.debug.ip.ospf.addSC("events", "OSPF events");
         enableC.debug.ip.ospf.addSC("flood", "OSPF flooding");
         enableC.debug.ip.ospf.addSC("lsa-generation", "OSPF lsa generation");
         enableC.debug.ip.ospf.addSC("packet", "OSPF packets");
         enableC.debug.ip.ospf.addSC("retransmission", "OSPF retransmission events");
         enableC.debug.ip.ospf.addSC("spf", "OSPF spf");
         enableC.debug.ip.ospf.addSC("tree", "OSPF database tree");
      enableC.debug.ip.addSC("packet", "General IP debugging and IPSO security transactions");
      enableC.debug.ip.addSC("policy", "Policy routing");
      enableC.debug.ip.addSC("rip", "RIP protocol transactions");
         enableC.debug.ip.rip.addSC("database", "RIP database events");
         enableC.debug.ip.rip.addSC("events", "RIP protocol events");
         enableC.debug.ip.rip.addSC("trigger", "RIP trigger extension");
      enableC.debug.ip.addSC("routing", "Routing table events");
         enableC.debug.ip.routing.addSC("<1-199>", "Access list");
         enableC.debug.ip.routing.addSC("<1300-2699>", "Access list (expanded range)");
      enableC.debug.ip.addSC("socket", "Socket event");
      enableC.debug.ip.addSC("tcp", "TCP information");
      enableC.debug.ip.addSC("tempacl", "IP temporary ACL");
      enableC.debug.ip.addSC("trigger-authentication", "Trigger authentication");
      enableC.debug.ip.addSC("udp", "UDP based transactions");
   enableC.debug.addSC("ipx", "Novell/IPX information");
   enableC.debug.addSC("isis", "IS-IS Information");
      enableC.debug.isis.addSC("adj-packets", "IS-IS Adjacency related packets");
      enableC.debug.isis.addSC("checksum-errors", "IS-IS LSP checksum errors");
      enableC.debug.isis.addSC("local-updates", "IS-IS local update packets");
      enableC.debug.isis.addSC("protocol-errors", "IS-IS LSP protocol errors");
      enableC.debug.isis.addSC("snp-packets", "IS-IS CSNP/PSNP packets");
      enableC.debug.isis.addSC("spf-events", "IS-IS Shortest Path First Events");
      enableC.debug.isis.addSC("spf-statistics", "IS-IS SPF Timing and Statistic Data");
      enableC.debug.isis.addSC("spf-triggers", "IS-IS SPF triggering events");
      enableC.debug.isis.addSC("update-packets", "IS-IS Update related packets");
   enableC.debug.addSC("kerberos", "KERBEROS authentication and authorization");
   enableC.debug.addSC("serial", "Serial interface information");
   enableC.debug.addSC("telnet", "Incoming telnet connections");
   enableC.debug.addSC("tftp", "TFTP debugging");
   enableC.debug.addSC("translate", "Protocol translation events");
enableC.addSC("delete", "Delete a file");
enableC.addSC("dir", "List files on a filesystem");
enableC.addSC("disable", "Turn off privileged commands");
enableC.addSC("disconnect", "Disconnect an existing network connection");
enableC.addSC("enable", "Turn on privileged commands");
   enableC.enable.addSC("<0-15>", "Enable level");
enableC.addSC("erase", "Erase a filesystem");
enableC.addSC("exit", "Exit from the EXEC");
enableC.addSC("help", "Description of the interactive help system");
enableC.addSC("lock", "Lock the terminal");
enableC.addSC("name-connection", "Name an existing network connection");
enableC.addSC("no", "Disable debugging functions");
enableC.addSC("pad", "Open a X.29 PAD connection");
enableC.addSC("ping", "Send echo messages");
   enableC.ping.addSC("WORD", "Ping destination address or hostname");
   enableC.ping.addSC("apollo", "Apollo echo");
   enableC.ping.addSC("appletalk", "Appletalk echo");
   enableC.ping.addSC("clns", "CLNS echo");
   enableC.ping.addSC("decnet", "DECnet echo");
   enableC.ping.addSC("ip", "IP echo");
      enableC.ping.ip.addSC("WORD", "Ping destination address or hostname");
   enableC.ping.addSC("ipx", "Novell/IPX echo");
      enableC.ping.ipx.addSC("WORD", "Ping destination address or hostname");
   enableC.ping.addSC("srb", "srb echo");
      enableC.ping.srb.addSC("WORD", "Ping destination address or hostname");
   enableC.ping.addSC("tag", "Tag encapsulated IP echo");
      enableC.ping.tag.addSC("WORD", "Ping destination address or hostname");
   enableC.ping.addSC("vines", "Vines echo");
      enableC.ping.vines.addSC("WORD", "Ping destination address or hostname");
   enableC.ping.addSC("xns", "XNS echo");
enableC.addSC("ppp", "Start IETF Point-to-Point Protocol (PPP)");
enableC.addSC("pwd", "Display current working directory");
enableC.addSC("reload", "Halt and perform a cold restart");
enableC.addSC("resume", "Resume an active network connection");
enableC.addSC("rlogin", "Open an rlogin connection");
enableC.addSC("send", "Send a message to other tty lines");
enableC.addSC("set", "Set system parameter (not config)");
enableC.addSC("setup", "Run the SETUP command facility");
enableC.addSC("show", "Show running system information");
   enableC.show.addSC("access-expression", "List access expression");
   enableC.show.addSC("access-lists", "List access lists");
   enableC.show.addSC("accounting", "Accounting data for active sessions");
   enableC.show.addSC("aliases", "Display alias commands");
   enableC.show.addSC("arap", "Show Appletalk Remote Access statistics");
   enableC.show.addSC("arp", "ARP table");
   enableC.show.addSC("async", "Information on terminal lines used as router interfaces");
   enableC.show.addSC("backup", "Backup status");
   enableC.show.addSC("call", "Show Calls");
   enableC.show.addSC("cdp", "CDP information");
   enableC.show.addSC("class-map", "Show QoS Class Map");
   enableC.show.addSC("clns", "CLNS network information");
      enableC.show.clns.addSC("cache", "CLNS fast-switching route cache");
      enableC.show.clns.addSC("es-neighbors", "ES neighbor adjacencies");
      enableC.show.clns.addSC("filter-set", "CLNS filter sets");
      enableC.show.clns.addSC("interface", "CLNS interface status and configuration");
      enableC.show.clns.addSC("is-neighbors", "IS neighbor adjacencies");
      enableC.show.clns.addSC("neighbors", "CLNS neighbor adjacencies");
         enableC.show.clns.neighbors.addSC("Async", "Async interface");
            enableC.show.clns.neighbors.Async.addSC("<1-65>", "Async interface number");
         enableC.show.clns.neighbors.addSC("Dialer", "Dialer interface");
            enableC.show.clns.neighbors.Dialer.addSC("<0-255>", "Dialer interface number");
         enableC.show.clns.neighbors.addSC("FastEthernet", "FastEthernet IEEE 802.3");
            enableC.show.clns.neighbors.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
         enableC.show.clns.neighbors.addSC("Serial", "Serial");
            enableC.show.clns.neighbors.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show.clns.neighbors.addSC("areas", "CLNS multiarea adjacencies");
            enableC.show.clns.neighbors.areas.addSC("Async", "Async interface");
               enableC.show.clns.neighbors.areas.Async.addSC("<1-65>", "Async interface number");
            enableC.show.clns.neighbors.areas.addSC("Dialer", "Dialer interface");
               enableC.show.clns.neighbors.areas.Dialer.addSC("<0-255>", "Dialer interface number");
            enableC.show.clns.neighbors.areas.addSC("FastEthernet", "FastEthernet IEEE 802.3");
               enableC.show.clns.neighbors.areas.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            enableC.show.clns.neighbors.areas.addSC("Serial", "Serial");
               enableC.show.clns.neighbors.areas.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show.clns.neighbors.addSC("detail", "Show detailed information");
      enableC.show.clns.addSC("protocol", "CLNS routing protocol process information");
      enableC.show.clns.addSC("redirects", "CLNS redirect information");
      enableC.show.clns.addSC("route", "CLNS prefix routing table");
      enableC.show.clns.addSC("traffic", "CLNS protocol statistics");
   enableC.show.addSC("clock", "Display the system clock");
   enableC.show.addSC("compress", "Show compression statistics");
   enableC.show.addSC("configuration", "Contents of Non-Volatile memory");
   enableC.show.addSC("controllers", "Interface controller status");
   enableC.show.addSC("crypto", "Encryption module");
      enableC.show.crypto.addSC("dynamic-map", "Crypto map templates");
      enableC.show.crypto.addSC("ipsec", "Show IPSEC policy");
         enableC.show.crypto.ipsec.addSC("sa", "IPSEC SA table");
            enableC.show.crypto.ipsec.sa.addSC("address", "IPSEC SA table in (dest) address order");
            enableC.show.crypto.ipsec.sa.addSC("detail", "show counter detail");
            enableC.show.crypto.ipsec.sa.addSC("identity", "IPSEC SADB identity tree");
               enableC.show.crypto.ipsec.sa.identity.addSC("detail", "show counter detail");
               enableC.show.crypto.ipsec.sa.identity.addSC("interface", "show info for specific interface");
                  enableC.show.crypto.ipsec.sa.identity.interface.addSC("Async", "Async interface");
                  enableC.show.crypto.ipsec.sa.identity.interface.addSC("Dialer", "Dialer interface");
                  enableC.show.crypto.ipsec.sa.identity.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
                  enableC.show.crypto.ipsec.sa.identity.interface.addSC("Loopback", "Loopback interface");
                  enableC.show.crypto.ipsec.sa.identity.interface.addSC("Null", "Null interface");
                  enableC.show.crypto.ipsec.sa.identity.interface.addSC("Serial", "Serial");
            enableC.show.crypto.ipsec.sa.addSC("interface", "Show info for specific interface");
            enableC.show.crypto.ipsec.sa.addSC("map", "IPSEC SA table for a specific crypto map");
               enableC.show.crypto.ipsec.sa.map.addSC("WORD", "crypto map tag");
                  enableC.show.crypto.ipsec.sa.map.WORD.addSC("detail", "show counter detail");
         enableC.show.crypto.ipsec.addSC("transform-set", "Crypto transform sets");
      enableC.show.crypto.addSC("isakmp", "Show ISAKMP Security Associations");
         enableC.show.crypto.isakmp.addSC("policy", "Show ISAKMP protection suite policy");
         enableC.show.crypto.isakmp.addSC("sa", "Show ISAKMP Security Associations");
      enableC.show.crypto.addSC("key", "Show long term public keys");
      enableC.show.crypto.addSC("map", "Crypto maps");
         enableC.show.crypto.map.addSC("interface", "Crypto maps for an interface.");
            enableC.show.crypto.map.interface.addSC("Async", "Async interface");
               enableC.show.crypto.map.interface.Async.addSC("<1-65>", "Async interface number");
            enableC.show.crypto.map.interface.addSC("Dialer", "Dialer interface");
               enableC.show.crypto.map.interface.Dialer.addSC("<0-255>", "Dialer interface number");
            enableC.show.crypto.map.interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
               enableC.show.crypto.map.interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            enableC.show.crypto.map.interface.addSC("Loopback", "Loopback interface");
               enableC.show.crypto.map.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
            enableC.show.crypto.map.interface.addSC("Serial", "Serial");
               enableC.show.crypto.map.interface.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show.crypto.map.addSC("tag", "Crypto maps with a given tag.");
            enableC.show.crypto.map.tag.addSC("WORD", "Crypto map tag");
   enableC.show.addSC("debugging", "State of each debugging option");
   enableC.show.addSC("dhcp", "Dynamic Host Configuration Protocol status");
   enableC.show.addSC("dial-peer", "Dial Plan Mapping Table for, e.g. VoIP Peers");
   enableC.show.addSC("dialer", "Dialer parameters and statistics");
   enableC.show.addSC("frame-relay", "Frame-Relay information");
      enableC.show["frame-relay"].addSC("end-to-end", "Frame-relay end-to-end VC information");
      enableC.show["frame-relay"].addSC("fragment", "show frame relay fragmentation information");
      enableC.show["frame-relay"].addSC("ip", "show frame relay IP statistics");
      enableC.show["frame-relay"].addSC("map", "Frame-Relay map table");
      enableC.show["frame-relay"].addSC("pvc", "show frame relay pvc statistics");
         enableC.show["frame-relay"].pvc.addSC("interface", "");
            enableC.show["frame-relay"].pvc.interface.addSC("Dialer", "Dialer interface");
               enableC.show["frame-relay"].pvc.interface.Dialer.addSC("<0-255>", "Dialer interface number");
            enableC.show["frame-relay"].pvc.interface.addSC("Serial", "Serial");
               enableC.show["frame-relay"].pvc.interface.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show["frame-relay"].pvc.addSC("<16-1022>", "DLCI");
      enableC.show["frame-relay"].addSC("qos-autosense", "show frame relay qos-autosense information");
      enableC.show["frame-relay"].addSC("route", "show frame relay route");
      enableC.show["frame-relay"].addSC("traffic", "Frame-Relay protocol statistics");
      enableC.show["frame-relay"].addSC("vofr", "Show frame-relay VoFR statistics");
   enableC.show.addSC("gateway", "Show status of gateway");
   enableC.show.addSC("history", "Display the session command history");
   enableC.show.addSC("hosts", "IP domain-name, lookup style, nameservers, and host table");
   enableC.show.addSC("interfaces", "Interface status and configuration");
   enableC.show.addSC("ip", "IP information");
      enableC.show.ip.addSC("access-lists", "List IP access lists");
      enableC.show.ip.addSC("accounting", "The active IP accounting database");
      enableC.show.ip.addSC("aliases", "IP alias table");
      enableC.show.ip.addSC("arp", "IP ARP table");
      enableC.show.ip.addSC("bgp", "BGP information");
      enableC.show.ip.addSC("dhcp", "Show items in the DHCP database");
      enableC.show.ip.addSC("eigrp", "IP-EIGRP show commands");
         enableC.show.ip.eigrp.addSC("interfaces", "IP-EIGRP interfaces");
            enableC.show.ip.eigrp.interfaces.addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.interfaces.addSC("Async", "Async interface");
               enableC.show.ip.eigrp.interfaces.Async.addSC("<1-65>", "Async interface number");
            enableC.show.ip.eigrp.interfaces.addSC("Dialer", "Dialer interface");
               enableC.show.ip.eigrp.interfaces.Dialer.addSC("<0-255>", "Dialer interface number");
                  enableC.show.ip.eigrp.interfaces.Dialer["<0-255>"].addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.interfaces.addSC("FastEthernet", "FastEthernet IEEE 802.3");
               enableC.show.ip.eigrp.interfaces.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            enableC.show.ip.eigrp.interfaces.addSC("Loopback", "Loopback interface");
               enableC.show.ip.eigrp.interfaces.Loopback.addSC("<0-2147483647>", "Loopback interface number");
                  enableC.show.ip.eigrp.interfaces.Loopback["<0-2147483647>"].addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.interfaces.addSC("Null", "Null interface");
               enableC.show.ip.eigrp.interfaces.Null.addSC("<0-0>", "Null interface number");
                  enableC.show.ip.eigrp.interfaces.Null["<0-0>"].addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.interfaces.addSC("Serial", "Serial");
               enableC.show.ip.eigrp.interfaces.Serial.addSC("<0-1>", "Serial interface number");
            enableC.show.ip.eigrp.interfaces.addSC("detail", "Show detailed peer information");
               enableC.show.ip.eigrp.interfaces.detail.addSC("<1-65535>", "AS Number");
               enableC.show.ip.eigrp.interfaces.detail.addSC("Async", "Async interface");
                  enableC.show.ip.eigrp.interfaces.detail.Async.addSC("<1-65>", "Async interface number");
               enableC.show.ip.eigrp.interfaces.detail.addSC("Dialer", "Dialer interface");
                  enableC.show.ip.eigrp.interfaces.detail.Dialer.addSC("<0-255>", "Dialer interface number");
               enableC.show.ip.eigrp.interfaces.detail.addSC("FastEthernet", "FastEthernet IEEE 802.3");
                  enableC.show.ip.eigrp.interfaces.detail.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
               enableC.show.ip.eigrp.interfaces.detail.addSC("Loopback", "Loopback interface");
                  enableC.show.ip.eigrp.interfaces.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
               enableC.show.ip.eigrp.interfaces.detail.addSC("Null", "Null interface");
                  enableC.show.ip.eigrp.interfaces.detail.Null.addSC("<0-0>", "Null interface number");
               enableC.show.ip.eigrp.interfaces.detail.addSC("Serial", "Serial");
                  enableC.show.ip.eigrp.interfaces.detail.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show.ip.eigrp.addSC("neighbors", "IP-EIGRP neighbors");
            enableC.show.ip.eigrp.neighbors.addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.neighbors.addSC("Async", "Async interface");
               enableC.show.ip.eigrp.neighbors.Async.addSC("<1-65>", "Async interface number");
            enableC.show.ip.eigrp.neighbors.addSC("Dialer", "Dialer interface");
               enableC.show.ip.eigrp.neighbors.Dialer.addSC("<0-255>", "Dialer interface number");
                  enableC.show.ip.eigrp.neighbors.Dialer["<0-255>"].addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.neighbors.addSC("FastEthernet", "FastEthernet IEEE 802.3");
               enableC.show.ip.eigrp.neighbors.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            enableC.show.ip.eigrp.neighbors.addSC("Loopback", "Loopback interface");
               enableC.show.ip.eigrp.neighbors.Loopback.addSC("<0-2147483647>", "Loopback interface number");
                  enableC.show.ip.eigrp.neighbors.Loopback["<0-2147483647>"].addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.neighbors.addSC("Null", "Null interface");
               enableC.show.ip.eigrp.neighbors.Null.addSC("<0-0>", "Null interface number");
                  enableC.show.ip.eigrp.neighbors.Null["<0-0>"].addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.neighbors.addSC("Serial", "Serial");
               enableC.show.ip.eigrp.neighbors.Serial.addSC("<0-1>", "Serial interface number");
            enableC.show.ip.eigrp.neighbors.addSC("detail", "Show detailed peer information");
               enableC.show.ip.eigrp.neighbors.detail.addSC("<1-65535>", "AS Number");
               enableC.show.ip.eigrp.neighbors.detail.addSC("Async", "Async interface");
                  enableC.show.ip.eigrp.neighbors.detail.Async.addSC("<1-65>", "Async interface number");
               enableC.show.ip.eigrp.neighbors.detail.addSC("Dialer", "Dialer interface");
                  enableC.show.ip.eigrp.neighbors.detail.Dialer.addSC("<0-255>", "Dialer interface number");
               enableC.show.ip.eigrp.neighbors.detail.addSC("FastEthernet", "FastEthernet IEEE 802.3");
                  enableC.show.ip.eigrp.neighbors.detail.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
               enableC.show.ip.eigrp.neighbors.detail.addSC("Loopback", "Loopback interface");
                  enableC.show.ip.eigrp.neighbors.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
               enableC.show.ip.eigrp.neighbors.detail.addSC("Null", "Null interface");
                  enableC.show.ip.eigrp.neighbors.detail.Null.addSC("<0-0>", "Null interface number");
               enableC.show.ip.eigrp.neighbors.detail.addSC("Serial", "Serial");
                  enableC.show.ip.eigrp.neighbors.detail.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show.ip.eigrp.addSC("topology", "IP-EIGRP Topology Table");
            enableC.show.ip.eigrp.topology.addSC("<1-65535>", "AS Number");
            enableC.show.ip.eigrp.topology.addSC("A.B.C.D", "Network to display information about");
               enableC.show.ip.eigrp.topology["A.B.C.D"].addSC("A.B.C.D", "Network mask");
            enableC.show.ip.eigrp.topology.addSC("active", "Show only active entries");
            enableC.show.ip.eigrp.topology.addSC("all-links", "Show all links in topology table");
            enableC.show.ip.eigrp.topology.addSC("pending", "Show only entries pending transmission");
            enableC.show.ip.eigrp.topology.addSC("summary", "Show a summary of the topology table");
            enableC.show.ip.eigrp.topology.addSC("zero-successors", "Show only zero successor entries");
         enableC.show.ip.eigrp.addSC("traffic", "IP-EIGRP Traffic Statistics");
      enableC.show.ip.addSC("flow", "NetFlow switching");
      enableC.show.ip.addSC("interface", "IP interface status and configuration");
      enableC.show.ip.addSC("irdp", "ICMP Router Discovery Protocol");
      enableC.show.ip.addSC("local", "IP local options");
      enableC.show.ip.addSC("nat", "IP NAT information");
         enableC.show.ip.nat.addSC("statistics", "Translation statistics");
         enableC.show.ip.nat.addSC("translations", "Translation entries");
            enableC.show.ip.nat.translations.addSC("verbose", "Show extra information");
      enableC.show.ip.addSC("nhrp", "NHRP information");
      enableC.show.ip.addSC("ospf", "OSPF information");
         enableC.show.ip.ospf.addSC("<1-4294967295>", "Process ID number");
            enableC.show.ip.ospf["<1-4294967295>"].addSC("<0-4294967295>", "OSPF area ID as a decimal number");
            enableC.show.ip.ospf["<1-4294967295>"].addSC("A.B.C.D", "OSPF area ID in IP address format");
         enableC.show.ip.ospf.addSC("border-routers", "Border and Boundary Router Information");
         enableC.show.ip.ospf.addSC("database", "Database summary");
            enableC.show.ip.ospf.database.addSC("adv-router", "Advertising Router link states");
               enableC.show.ip.ospf.database["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
            enableC.show.ip.ospf.database.addSC("asbr-summary", "ASBR summary link states");
               enableC.show.ip.ospf.database["asbr-summary"].addSC("A.B.C.D", "Link state ID (as an IP address)");
               enableC.show.ip.ospf.database["asbr-summary"].addSC("adv-router", "Advertising Router link states");
                  enableC.show.ip.ospf.database["asbr-summary"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
               enableC.show.ip.ospf.database["asbr-summary"].addSC("internal", "Internal LSA information");
                  enableC.show.ip.ospf.database["asbr-summary"].internal.addSC("adv-router", "Advertising Router link states");
            enableC.show.ip.ospf.database.addSC("database-summary", "Summary of database");
            enableC.show.ip.ospf.database.addSC("external", "External link states");
               enableC.show.ip.ospf.database.external.addSC("A.B.C.D", "Link state ID (as an IP address)");
               enableC.show.ip.ospf.database.external.addSC("adv-router", "Advertising Router link states");
                  enableC.show.ip.ospf.database.external["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
               enableC.show.ip.ospf.database.external.addSC("internal", "Internal LSA information");
                  enableC.show.ip.ospf.database.external.internal.addSC("adv-router", "Advertising Router link states");
            enableC.show.ip.ospf.database.addSC("network", "Network link states");
               enableC.show.ip.ospf.database.network.addSC("A.B.C.D", "Link state ID (as an IP address)");
               enableC.show.ip.ospf.database.network.addSC("adv-router", "Advertising Router link states");
                  enableC.show.ip.ospf.database.network["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
               enableC.show.ip.ospf.database.network.addSC("internal", "Internal LSA information");
                  enableC.show.ip.ospf.database.network.internal.addSC("adv-router", "Advertising Router link states");
            enableC.show.ip.ospf.database.addSC("nssa-external", "NSSA External link states");
               enableC.show.ip.ospf.database["nssa-external"].addSC("A.B.C.D", "Link state ID (as an IP address)");
               enableC.show.ip.ospf.database["nssa-external"].addSC("adv-router", "Advertising Router link states");
                  enableC.show.ip.ospf.database["nssa-external"]["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
               enableC.show.ip.ospf.database["nssa-external"].addSC("internal", "Internal LSA information");
                  enableC.show.ip.ospf.database["nssa-external"].internal.addSC("adv-router", "Advertising Router link states");
            enableC.show.ip.ospf.database.addSC("router", "Router link states");
               enableC.show.ip.ospf.database.router.addSC("A.B.C.D", "Link state ID (as an IP address)");
               enableC.show.ip.ospf.database.router.addSC("adv-router", "Advertising Router link states");
                  enableC.show.ip.ospf.database.router["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
               enableC.show.ip.ospf.database.router.addSC("internal", "Internal LSA information");
                  enableC.show.ip.ospf.database.router.internal.addSC("adv-router", "Advertising Router link states");
            enableC.show.ip.ospf.database.addSC("self-originate", "Self-originated link states");
            enableC.show.ip.ospf.database.addSC("summary", "Network summary link states");
               enableC.show.ip.ospf.database.summary.addSC("A.B.C.D", "Link state ID (as an IP address)");
               enableC.show.ip.ospf.database.summary.addSC("adv-router", "Advertising Router link states");
                  enableC.show.ip.ospf.database.summary["adv-router"].addSC("A.B.C.D", "Advertising Router (as an IP address)");
               enableC.show.ip.ospf.database.summary.addSC("internal", "Internal LSA information");
                  enableC.show.ip.ospf.database.summary.internal.addSC("adv-router", "Advertising Router link states");
               enableC.show.ip.ospf.database.summary.addSC("self-originate", "Self-originated link states");
         enableC.show.ip.ospf.addSC("flood-list", "Link state flood list");
         enableC.show.ip.ospf.addSC("interface", "Interface information");
         enableC.show.ip.ospf.addSC("neighbor", "Neighbor list");
            enableC.show.ip.ospf.neighbor.addSC("Async", "Async interface");
            enableC.show.ip.ospf.neighbor.addSC("Dialer", "Dialer interface");
            enableC.show.ip.ospf.neighbor.addSC("FastEthernet", "FastEthernet IEEE 802.3");
               enableC.show.ip.ospf.neighbor.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
            enableC.show.ip.ospf.neighbor.addSC("Loopback", "Loopback interface");
            enableC.show.ip.ospf.neighbor.addSC("Null", "Null interface");
            enableC.show.ip.ospf.neighbor.addSC("Serial", "Serial");
            enableC.show.ip.ospf.neighbor.addSC("detail", "detail of all neighbors");
               enableC.show.ip.ospf.neighbor.detail.addSC("Async", "Async interface");
                  enableC.show.ip.ospf.neighbor.detail.Async.addSC("<1-65>", "Async interface number");
               enableC.show.ip.ospf.neighbor.detail.addSC("Dialer", "Dialer interface");
                  enableC.show.ip.ospf.neighbor.detail.Dialer.addSC("<0-255>", "Dialer interface number");
               enableC.show.ip.ospf.neighbor.detail.addSC("FastEthernet", "FastEthernet IEEE 802.3");
                  enableC.show.ip.ospf.neighbor.detail.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
               enableC.show.ip.ospf.neighbor.detail.addSC("Loopback", "Loopback interface");
                  enableC.show.ip.ospf.neighbor.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
               enableC.show.ip.ospf.neighbor.detail.addSC("Null", "Null interface");
                  enableC.show.ip.ospf.neighbor.detail.Null.addSC("<0-0>", "Null interface number");
               enableC.show.ip.ospf.neighbor.detail.addSC("Serial", "Serial");
                  enableC.show.ip.ospf.neighbor.detail.Serial.addSC("<0-1>", "Serial interface number");
         enableC.show.ip.ospf.addSC("request-list", "Link state request list");
         enableC.show.ip.ospf.addSC("retransmission-list", "Link state retransmission list");
         enableC.show.ip.ospf.addSC("summary-address", "Summary-address redistribution Information");
         enableC.show.ip.ospf.addSC("virtual-links", "Virtual link information");
      enableC.show.ip.addSC("pgm", "PGM Reliable Transport Protocol");
      enableC.show.ip.addSC("pim", "PIM information");
      enableC.show.ip.addSC("policy", "Policy routing");
      enableC.show.ip.addSC("port-map", "Port to Application Mapping (PAM) information");
      enableC.show.ip.addSC("prefix-list", "List IP prefix lists");
      enableC.show.ip.addSC("protocols", "IP routing protocol process parameters and statistics");
         enableC.show.ip.protocols.addSC("summary", "Short form answer");
         enableC.show.ip.protocols.addSC("vrf", "Display protocols for a VPN Routing/Forwarding instance");
      enableC.show.ip.addSC("redirects", "IP redirects");
      enableC.show.ip.addSC("rip", "IP RIP show commands");
      enableC.show.ip.addSC("route", "IP routing table");
         enableC.show.ip.route.addSC("bgp", "Border Gateway Protocol (BGP)");
            enableC.show.ip.route.bgp.addSC("<1-65535>", "Autonomous system number");
         enableC.show.ip.route.addSC("connected", "Connected");
         enableC.show.ip.route.addSC("egp", "Exterior Gateway Protocol (EGP)");
            enableC.show.ip.route.egp.addSC("<0-65535>", "Remote autonomous system number");
         enableC.show.ip.route.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
            enableC.show.ip.route.eigrp.addSC("<1-65535>", "Autonomous system number");
         enableC.show.ip.route.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
            enableC.show.ip.route.igrp.addSC("<1-65535>", "Autonomous system number");
         enableC.show.ip.route.addSC("isis", "ISO IS-IS");
            enableC.show.ip.route.isis.addSC("WORD", "ISO routing area tag");
         enableC.show.ip.route.addSC("list", "IP Access list");
            enableC.show.ip.route.list.addSC("<1-199>", "IP access list number");
         enableC.show.ip.route.addSC("mobile", "Mobile routes");
         enableC.show.ip.route.addSC("odr", "On Demand stub Routes");
         enableC.show.ip.route.addSC("ospf", "Open Shortest Path First (OSPF)");
            enableC.show.ip.route.ospf.addSC("<1-65535>", "Process ID");
         enableC.show.ip.route.addSC("profile", "IP routing table profile");
         enableC.show.ip.route.addSC("rip", "Routing Information Protocol (RIP)");
         enableC.show.ip.route.addSC("static", "Static routes");
         enableC.show.ip.route.addSC("summary", "Summary of all routes");
         enableC.show.ip.route.addSC("supernets-only", "Show supernet entries only");
         enableC.show.ip.route.addSC("traffic-engineering", "Traffic engineered routes");
         enableC.show.ip.route.addSC("vrf", "Display routes from a VPN Routing/Forwarding instance");
      enableC.show.ip.addSC("rpf", "Display RPF information for multicast source");
      enableC.show.ip.addSC("rsvp", "RSVP information");
      enableC.show.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
      enableC.show.ip.addSC("sdr", "Session Directory (SDPv2) cache");
      enableC.show.ip.addSC("sockets", "Open IP sockets");
      enableC.show.ip.addSC("tcp", "TCP/IP header-compression statistics");
      enableC.show.ip.addSC("traffic", "IP protocol statistics");
      enableC.show.ip.addSC("trigger-authentication", "Trigger-authentication host table");
      enableC.show.ip.addSC("vrf", "VPN Routing/Forwarding instance information");
      enableC.show.ip.addSC("wccp", "WCCP information");
   enableC.show.addSC("ipx", "Novell IPX information");
   enableC.show.addSC("isis", "IS-IS routing information");
      enableC.show.isis.addSC("database", "IS-IS link state database");
         enableC.show.isis.database.addSC("detail", "Detailed link state database information");
         enableC.show.isis.database.addSC("l1", "IS-IS Level-1 routing link state database");
         enableC.show.isis.database.addSC("l2", "IS-IS Level-2 routing link state database");
         enableC.show.isis.database.addSC("level-1", "IS-IS Level-1 routing link state database");
         enableC.show.isis.database.addSC("level-2", "IS-IS Level-2 routing link state database");
      enableC.show.isis.addSC("hostname", "IS-IS Dynamic hostname mapping");
      enableC.show.isis.addSC("lsp-log", "IS-IS LSP log");
      enableC.show.isis.addSC("mesh-groups", "IS-IS mesh groups");
      enableC.show.isis.addSC("route", "IS-IS level-1 routing table");
      enableC.show.isis.addSC("spf-log", "IS-IS SPF log");
      enableC.show.isis.addSC("topology", "IS-IS paths to Intermediate Systems");
   enableC.show.addSC("kerberos", "Show Kerberos Values");
   enableC.show.addSC("key", "Key information");
   enableC.show.addSC("keymap", "Terminal keyboard mappings");
   enableC.show.addSC("lat", "DEC LAT information");
   enableC.show.addSC("line", "TTY line information");
      enableC.show.line.addSC("<0-70>", "First Line range");
         enableC.show.line["<0-70>"].addSC("<1-70>", "Last Line range");
      enableC.show.line.addSC("aux", "Auxiliary line");
         enableC.show.line.aux.addSC("<0-0>", "First Line range");
      enableC.show.line.addSC("console", "Primary terminal line");
         enableC.show.line.console.addSC("<0-0>", "First Line range");
      enableC.show.line.addSC("summary", "Quick line status summary");
      enableC.show.line.addSC("tty", "Terminal controller");
         enableC.show.line.tty.addSC("<1-64>", "First Line range");
            enableC.show.line.tty["<1-64>"].addSC("<2-64>", "Last Line range");
            enableC.show.line.tty["<1-64>"].addSC("summary", "Quick line status summary");
      enableC.show.line.addSC("vty", "Virtual terminal");
         enableC.show.line.vty.addSC("<0-133>", "First Line range");
            enableC.show.line.vty["<0-133>"].addSC("<1-133>", "Last Line range");
            enableC.show.line.vty["<0-133>"].addSC("summary", "Quick line status summary");
   enableC.show.addSC("llc2", "IBM LLC2 circuit information");
   enableC.show.addSC("lnm", "IBM LAN manager");
   enableC.show.addSC("local-ack", "Local Acknowledgement virtual circuits");
   enableC.show.addSC("location", "Display the system location");
   enableC.show.addSC("logging", "Show the contents of logging buffers");
      enableC.show.logging.addSC("history", "Show the contents of syslog history table");
   enableC.show.addSC("memory", "Memory statistics");
   enableC.show.addSC("modemcap", "Show Modem Capabilities database");
   enableC.show.addSC("mpoa", "MPOA show commands");
   enableC.show.addSC("nbf", "NBF (NetBEUI) information");
   enableC.show.addSC("ncia", "Native Client Interface Architecture");
   enableC.show.addSC("netbios-cache", "NetBIOS name cache contents");
   enableC.show.addSC("node", "Show known LAT nodes");
   enableC.show.addSC("policy-map", "Show QoS Policy Map");
      enableC.show["policy-map"].addSC("WORD", "policy-map name");
         enableC.show["policy-map"].WORD.addSC("class", "Show Qos Policy actions for a indvidual class");
            enableC.show["policy-map"].WORD.class.addSC("WORD", "class-map name");
      enableC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
         enableC.show["policy-map"].interface.addSC("Async", "Async interface");
            enableC.show["policy-map"].interface.Async.addSC("<1-65>", "Async interface number");
         enableC.show["policy-map"].interface.addSC("Dialer", "Dialer interface");
            enableC.show["policy-map"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
         enableC.show["policy-map"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
            enableC.show["policy-map"].interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
         enableC.show["policy-map"].interface.addSC("Loopback", "Loopback interface");
            enableC.show["policy-map"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
         enableC.show["policy-map"].interface.addSC("Null", "Null interface");
            enableC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
         enableC.show["policy-map"].interface.addSC("Serial", "Serial");
            enableC.show["policy-map"].interface.Serial.addSC("<0-1>", "Serial interface number");
   enableC.show.addSC("ppp", "PPP parameters and statistics");
   enableC.show.addSC("printers", "Show LPD printer information");
   enableC.show.addSC("privilege", "Show current privilege level");
   enableC.show.addSC("processes", "Active process statistics");
   enableC.show.addSC("protocols", "Active network routing protocols");
   enableC.show.addSC("qllc", "Display qllc-llc2 and qllc-sdlc conversion information");
   enableC.show.addSC("queue", "Show queue contents");
   enableC.show.addSC("queueing", "Show queueing configuration");
   enableC.show.addSC("registry", "Function registry information");
   enableC.show.addSC("reload", "Scheduled reload information");
   enableC.show.addSC("rhosts", "Remote-host+user equivalences");
   enableC.show.addSC("route-map", "route-map information");
   enableC.show.addSC("rtr", "Response Time Reporter (RTR)");
   enableC.show.addSC("running-config", "Current operating configuration");
      enableC.show["running-config"].addSC("interface", "Show interface configuration");
         enableC.show["running-config"].interface.addSC("Async", "Async interface");
            enableC.show["running-config"].interface.Async.addSC("<1-65>", "Async interface number");
         enableC.show["running-config"].interface.addSC("Dialer", "Dialer interface");
            enableC.show["running-config"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
         enableC.show["running-config"].interface.addSC("FastEthernet", "FastEthernet IEEE 802.3");
            enableC.show["running-config"].interface.FastEthernet.addSC("<0-1>", "FastEthernet interface number");
         enableC.show["running-config"].interface.addSC("Loopback", "Loopback interface");
            enableC.show["running-config"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
         enableC.show["running-config"].interface.addSC("Null", "Null interface");
            enableC.show["running-config"].interface.Null.addSC("<0-0>", "Null interface number");
         enableC.show["running-config"].interface.addSC("Serial", "Serial");
            enableC.show["running-config"].interface.Serial.addSC("<0-1>", "Serial interface number");
   enableC.show.addSC("sdllc", "Display sdlc - llc2 conversion information");
   enableC.show.addSC("sessions", "Information about Telnet connections");
   enableC.show.addSC("standby", "Hot standby protocol information");
   enableC.show.addSC("startup-config", "Contents of startup configuration");
   enableC.show.addSC("stun", "STUN status and configuration");
   enableC.show.addSC("subscriber-policy", "Subscriber policy");
   enableC.show.addSC("tcp", "Status of TCP connections");
   enableC.show.addSC("terminal", "Display terminal configuration parameters");
   enableC.show.addSC("time-range", "Time range");
   enableC.show.addSC("tn3270", "TN3270 settings");
   enableC.show.addSC("traffic-shape", "traffic rate shaping configuration");
      enableC.show["traffic-shape"].addSC("Async", "Async interface");
      enableC.show["traffic-shape"].addSC("Dialer", "Dialer interface");
      enableC.show["traffic-shape"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
      enableC.show["traffic-shape"].addSC("Loopback", "Loopback interface");
      enableC.show["traffic-shape"].addSC("Null", "Null interface");
      enableC.show["traffic-shape"].addSC("Serial", "Serial");
         enableC.show["traffic-shape"].statistics.addSC("Async", "Async interface");
            enableC.show["traffic-shape"].statistics.Async.addSC("<1-65>", "Async interface number");
         enableC.show["traffic-shape"].statistics.addSC("Loopback", "Loopback interface");
            enableC.show["traffic-shape"].statistics.Loopback.addSC("<0-2147483647>", "Loopback interface number");
         enableC.show["traffic-shape"].statistics.addSC("Serial", "Serial");
            enableC.show["traffic-shape"].statistics.Serial.addSC("<0-1>", "Serial interface number");
   enableC.show.addSC("users", "Display information about terminal lines");
   enableC.show.addSC("version", "System hardware and software status");
enableC.addSC("slip", "Start Serial-line IP (SLIP)");
enableC.addSC("start-chat", "Start a chat-script on a line");
enableC.addSC("systat", "Display information about terminal lines");
enableC.addSC("telnet", "Open a telnet connection");
enableC.addSC("terminal", "Set terminal line parameters");
enableC.addSC("test", "Test subsystems, memory, and interfaces");
enableC.addSC("tn3270", "Open a tn3270 connection");
enableC.addSC("traceroute", "Trace route to destination");
   enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
   enableC.traceroute.addSC("clns", "ISO CLNS Trace");
      enableC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
   enableC.traceroute.addSC("ip", "IP Trace");
      enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
   enableC.traceroute.addSC("ipx", "IPX Trace");
      enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
enableC.addSC("verify", "Verify a file");
enableC.addSC("where", "List active connections");
enableC.addSC("which-route", "Do OSI route table lookup and display results");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
	enableC.write.addSC("erase", "Erase NV memory");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("network", "Write to network TFTP server");
	enableC.write.addSC("terminal", "Write to terminal");
