RTF#show running-config
ip subnet-zero
interface Ethernet1/1
ip address 172.16.1.2 255.255.255.
interface Serial2/1
ip address 192.68.5.1 255.255.255.0
router ospf 10
network 172.16.0.0 0.0.255.255 area 0
network 192.68.0.0 0.0.255.255 area 0
router bgp 3
no synchronization
neighbor 172.16.2.254 remote-as 3
neighbor 192.68.12.1 remote-as 2
neighbor 192.68.12.1 ebgp-multihop 2
no auto-summary
ip classless
RTF#
