
subintFC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	subintFC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	subintFC.arp.addSC("timeout", "Set ARP cache timeout");
		subintFC.arp.timeout.addSC("<0-2147483>", "Seconds");
subintFC.addSC("bandwidth", "Set bandwidth informational parameter");
	subintFC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
subintFC.addSC("carrier-delay", "Specify delay for interface transitions");
	subintFC["carrier-delay"].addSC("<0-60>", "Carrier Transitions delay seconds");
subintFC.addSC("cdp", "CDP interface subcommands");
	subintFC.cdp.addSC("enable", "Enable CDP on interface");
subintFC.addSC("default", "Set a command to its defaults");
	subintFC["default"].addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		subintFC["default"].arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		subintFC["default"].arp.addSC("timeout", "Set ARP cache timeout");
	subintFC["default"].addSC("bandwidth", "Set bandwidth informational parameter");
	subintFC["default"].addSC("carrier-delay", "Specify delay for interface transitions");
	subintFC["default"].addSC("cdp", "CDP interface subcommands");
		subintFC["default"].cdp.addSC("enable", "Enable CDP on interface");
subintFC.addSC("delay", "Specify interface throughput delay");
	subintFC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
subintFC.addSC("description", "Interface specific description");
	subintFC.description.addSC("LINE", "Up to 240 characters describing this interface");
subintFC.addSC("exit", "Exit from interface configuration mode");
subintFC.addSC("ip", "Interface Internet Protocol config commands");
	subintFC.ip.addSC("access-group", "Specify access control for packets");
		subintFC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			subintFC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
		subintFC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			subintFC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
		subintFC.ip["access-group"].addSC("WORD", "Access-list name");
			subintFC.ip["access-group"].WORD.addSC("in", "inbound packets");
subintFC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	subintFC.mtu.addSC("<1500-1530>", "MTU size in bytes");
subintFC.addSC("no", "Negate a command or set its defaults");
	subintFC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		subintFC.no.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		subintFC.no.arp.addSC("timeout", "Set ARP cache timeout");
	subintFC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	subintFC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	subintFC.no.addSC("cdp", "CDP interface subcommands");
		subintFC.no.cdp.addSC("enable", "Enable CDP on interface");
	subintFC.no.addSC("delay", "Specify interface throughput delay");
	subintFC.no.addSC("description", "Interface specific description");
	subintFC.no.addSC("ip", "Interface Internet Protocol config commands");
		subintFC.no.ip.addSC("access-group", "Specify access control for packets");
			subintFC.no.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			subintFC.no.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			subintFC.no.ip["access-group"].addSC("in", "inbound packets");
	subintFC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");

	subintFC.no.addSC("shutdown","Shutdown the selected interface");

subintFC.addSC("ntp", "Configure NTP");
	subintFC.ntp.addSC("broadcast", "Configure NTP broadcast service");
		subintFC.ntp.broadcast.addSC("client", "Listen to NTP broadcasts");
		subintFC.ntp.broadcast.addSC("destination", "Configure broadcast destination address");
			subintFC.ntp.broadcast.destination.addSC("Hostname or A.B.C.D", "Destination broadcast IP address");
		subintFC.ntp.broadcast.addSC("key", "Configure broadcast authentication key");
			subintFC.ntp.broadcast.key.addSC("<0-4294967295>", "Broadcast key number");
				subintFC.ntp.broadcast.key["<0-4294967295>"].addSC("destination", "Configure broadcast destination address");
		subintFC.ntp.broadcast.addSC("version", "Configure NTP version");
			subintFC.ntp.broadcast.version.addSC("<1-3>", "NTP version number");
				subintFC.ntp.broadcast.version["<1-3>"].addSC("destination", "Configure broadcast destination address");
				subintFC.ntp.broadcast.version["<1-3>"].addSC("key", "Configure broadcast authentication key");
	subintFC.ntp.addSC("disable", "Disable NTP");
subintFC.addSC("service-policy", "Configure QoS Service Policy");
	subintFC["service-policy"].addSC("input", "Assign policy-map to the input of an interface");
		subintFC["service-policy"].input.addSC("WORD", "policy-map name");
subintFC.addSC("shutdown", "Shutdown the selected interface");
subintFC.addSC("timeout", "Define timeout values for this interface");
	subintFC.timeout.addSC("absolute", "Define session timeout value for this interface");
		subintFC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
			subintFC.timeout.absolute["<0-35790>"].addSC("<0-59>", "Session lifetime (in seconds)");
