Output=RTD%23show+running%2Dconfig%0Aip+subnet%2Dzero%0Ainterface+Serial0%2F0%0Aip+address+192%2E68%2E12%2E1+255%2E255%2E255%2E0%0Arouter+ospf+10%0Anetwork+192%2E68%2E0%2E0+0%2E0%2E255%2E255+area+0%0Arouter+bgp+2%0Aneighbor+192%2E68%2E5%2E1+remote%2Das+3%0Aneighbor+192%2E68%2E5%2E1+ebgp%2Dmultihop+2%0Ano+auto%2Dsummary%0Aip+classless%0ARTD%23%0A