Output=Router+B%23show+running%2Dconfig%0Ainterface+serial+0%0Aip+address+130%2E10%2E62%2E2+255%2E255%2E255%2E0%0Ainterface+serial+1%0Aip+address+130%2E10%2E64%2E2+255%2E255%2E255%2E0%0Ainterface+ethernet+0%0Aip+address+130%2E10%2E17%2E2+255%2E255%2E255%2E0%0Ainterface+tokenring+0%0Aip+address+130%2E10%2E16%2E2+255%2E255%2E255%2E0%0A%21%0Arouter+rip%0Adefault%2Dmetric+10%0Anetwork+130%2E10%2E0%2E0%0Apassive%2Dinterface+serial+0%0Apassive%2Dinterface+serial+1%0Aredistribute+ospf+109+match+internal+external+1+external+2%0A%21%0Arouter+ospf+109%0Anetwork+130%2E10%2E62%2E0+0%2E0%2E0%2E255+area+0%0Anetwork+130%2E10%2E64%2E0+0%2E0%2E0%2E255+area+0%0Aredistribute+rip+subnets%0Adistribute%2Dlist+11+out+rip%0Aaccess%2Dlist+11+permit+130%2E10%2E16%2E0+0%2E0%2E7%2E255%0Aaccess%2Dlist+11+deny+0%2E0%2E0%2E0+255%2E255%2E255%2E255%0ARouter+B%23