Current configuration:
!
version 12.0
service timestamps debug uptime
service timestamps log uptime
no service password-encryption
!
hostname Router-A
!
enable secret 5 $1$fZNO$0NTNtxFEV6HMoU3sSKeIq.
!
ip subnet-zero
!
ip audit notify log
ip audit po max-events 100
!
process-max-time 200
!
interface FastEthernet0/0
 ip address 12.0.0.1 255.0.0.0
 no ip directed-broadcast
!
interface Serial0/0
 no ip address
 no ip directed-broadcast
 no ip mroute-cache
 shutdown
!
interface FastEthernet0/1
 no ip address
 no ip directed-broadcast
 shutdown
!
interface Serial0/1
 ip address 2.0.0.2 255.255.255.0
 no ip directed-broadcast
!
router eigrp 300
 network 2.0.0.0
 network 12.0.0.0
!
router bgp 300
 no synchronization
 network 12.0.0.0
 neighbor 2.0.0.1 remote-as 300
!
ip classless
no ip http server
!
line con 0
 transport input none
line aux 0
line vty 0 4
 password cisco
 login
!
no scheduler allocate
end
