Router-B#show ip bgp
BGP table version is 12, local router ID is 10.0.0.1
Status codes: s suppressed, d damped, h history, * valid, > best, i - internal
Origin codes: i - IGP, e - EGP, ? - incomplete

   Network          Next Hop            Metric LocPrf Weight Path
*> 10.0.0.0         0.0.0.0                  0         32768 i
*> 11.0.0.0         3.0.0.2                  0             0 200 i
*>i12.0.0.0         2.0.0.2                  0    100      0 i
Router-B#
