Router-A#show ip bgp
BGP table version is 12, local router ID is 12.0.0.1
Status codes: s suppressed, d damped, h history, * valid, > best, i - internal
Origin codes: i - IGP, e - EGP, ? - incomplete

   Network          Next Hop            Metric LocPrf Weight Path
*>i10.0.0.0         2.0.0.1                  0    100      0 i
*>i11.0.0.0         2.0.0.1                  0    100      0 200 i
*> 12.0.0.0         0.0.0.0                  0         32768 i
Router-A#
