Output=Router%2DC%23show+ip+bgp+summary%0ABGP+router+identifier+11%2E0%2E0%2E1%2C+local+AS+number+200%0ABGP+table+version+is+6%2C+main+routing+table+version+6%0A3+network+entries+and+3+paths+using+399+bytes+of+memory%0A3+BGP+path+attribute+entries+using+156+bytes+of+memory%0A1+BGP+AS%2DPATH+entries+using+24+bytes+of+memory%0A0+BGP+route%2Dmap+cache+entries+using+0+bytes+of+memory%0A0+BGP+filter%2Dlist+cache+entries+using+0+bytes+of+memory%0ABGP+activity+10%2F53+prefixes%2C+10%2F7+paths%0A%0ANeighbor++++++++V++++AS+MsgRcvd+MsgSent+++TblVer++InQ+OutQ+Up%2FDown++State%2FPfxRcd%0A%0A3%2E0%2E0%2E1+++++++++4+++300+++++178+++++176++++++++6++++0++++0+02%3A20%3A15++++++++2%0ARouter%2DC%23%0A