
enableC.addSC("access-enable", "Create a temporary Access-List entry");
enableC.addSC("access-profile", "Apply user-profile to interface");
enableC.addSC("access-template", "Create a temporary Access-List entry");
enableC.addSC("archive", "manage archive files");
enableC.addSC("cd", "Change current directory");
enableC.addSC("clear", "Reset functions");
	enableC.clear.addSC("access-list", "Clear access list statistical information");
	enableC.clear.addSC("access-template", "Access-template");
	enableC.clear.addSC("adjacency", "Adjacent nodes");
	enableC.clear.addSC("arp-cache", "Clear the entire ARP cache");
	enableC.clear.addSC("atm", "ATM information");
	enableC.clear.addSC("bridge", "Reset bridge forwarding cache");
	enableC.clear.addSC("cdp", "Reset cdp information");
	enableC.clear.addSC("counters", "Clear counters on one or all interfaces");
	enableC.clear.addSC("dialer", "Clear dialer statistics");
	enableC.clear.addSC("frame-relay", "Clear Frame Relay information");
	enableC.clear.addSC("host", "Delete host table entries");
	enableC.clear.addSC("interface", "Clear the hardware logic on an interface");
	enableC.clear.addSC("ip", "IP");
		enableC.clear.ip.addSC("access-list", "Clear access list statistical information");
		enableC.clear.ip.addSC("access-template", "Access-template");
		enableC.clear.ip.addSC("accounting", "Clear IP accounting database");
		enableC.clear.ip.addSC("cache", "Delete cache table entries");
		enableC.clear.ip.addSC("cef", "Cisco Express Forwarding info");
		enableC.clear.ip.addSC("cgmp", "Cisco Group Management Protocol (CGMP)");
		enableC.clear.ip.addSC("dhcp", "Delete items from the DHCP database");
		enableC.clear.ip.addSC("dvmrp", "DVMRP");
		enableC.clear.ip.addSC("eigrp", "Clear IP-EIGRP");
		enableC.clear.ip.addSC("flow", "Clear flow information");
		enableC.clear.ip.addSC("igmp", "IGMP clear commands");
		enableC.clear.ip.addSC("mroute", "Delete multicast route table entries");
		enableC.clear.ip.addSC("msdp", "Multicast Source Discovery Protocol (MSDP)");
		enableC.clear.ip.addSC("mtag", "Clear multicast TIB entries");
		enableC.clear.ip.addSC("nat", "Clear NAT");
			enableC.clear.ip.nat.addSC("statistics", "Clear translation statistics");
			enableC.clear.ip.nat.addSC("translation", "Clear dynamic translation");
				enableC.clear.ip.nat.translation.addSC("*", "Delete all dynamic translations");
				enableC.clear.ip.nat.translation.addSC("inside", "Inside addresses (and ports)");
				enableC.clear.ip.nat.translation.addSC("outside", "Outside addresses (and ports)");
				enableC.clear.ip.nat.translation.addSC("tcp", "Transmission Control Protocol");
				enableC.clear.ip.nat.translation.addSC("udp", "User Datagram Protocol");
		enableC.clear.ip.addSC("pim", "PIM");
		enableC.clear.ip.addSC("prefix-list", "Prefix-list");
		enableC.clear.ip.addSC("redirect", "Redirect cache");
		enableC.clear.ip.addSC("route", "Delete route table entries");
			enableC.clear.ip.route.addSC("*", "Delete all routes");
			enableC.clear.ip.route.addSC("A.B.C.D", "Destination network route to delete");
			enableC.clear.ip.route.addSC("vrf", "Clear routes for a VPN Routing/Forwarding instance");
		enableC.clear.ip.addSC("rsvp", "RSVP");
		enableC.clear.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
		enableC.clear.ip.addSC("sdr", "Session Directory (SDPv2) cache");
		enableC.clear.ip.addSC("tcp", "TCP/UDP/IP header-compression statistics");
	enableC.clear.addSC("ipx", "Reset Novell/IPX information");
	enableC.clear.addSC("line", "Reset a terminal line");
	enableC.clear.addSC("logging", "Clear logging buffer");
	enableC.clear.addSC("memory", "Memory counters");
	enableC.clear.addSC("mgcp", "clear Media Gateway Control Protocol");
	enableC.clear.addSC("parser", "Clear parser data");
	enableC.clear.addSC("snapshot", "Clear Snapshot timers");
	enableC.clear.addSC("tcp", "Clear a TCP connection or statistics");
	enableC.clear.addSC("vpdn", "Clear a VPDN entity");
enableC.addSC("clock", "Manage the system clock");
enableC.addSC("cns", "CNS subsystem");
enableC.addSC("configure", "Enter configuration mode");
	enableC.configure.addSC("memory", "Configure from NV memory");
	enableC.configure.addSC("network", "Configure from a TFTP network host");
	enableC.configure.addSC("overwrite-network", "Overwrite NV memory from TFTP network host");
	enableC.configure.addSC("terminal", "Configure from the terminal");
enableC.addSC("connect", "Open a terminal connection");
enableC.addSC("copy", "Copy from one file to another");
	enableC.copy.addSC("/erase", "Erase destination file system.");
	enableC.copy.addSC("flash:", "Copy from flash: file system");
	enableC.copy.addSC("ftp:", "Copy from ftp: file system");
	enableC.copy.addSC("null:", "Copy from null: file system");
	enableC.copy.addSC("nvram:", "Copy from nvram: file system");
	enableC.copy.addSC("rcp:", "Copy from rcp: file system");
	enableC.copy.addSC("running-config", "Copy from current system configuration");
		enableC.copy["running-config"].addSC("flash:", "Copy to flash: file system");
		enableC.copy["running-config"].addSC("ftp:", "Copy to ftp: file system");
		enableC.copy["running-config"].addSC("null:", "Copy to null: file system");
		enableC.copy["running-config"].addSC("nvram:", "Copy to nvram: file system");
		enableC.copy["running-config"].addSC("rcp:", "Copy to rcp: file system");
		enableC.copy["running-config"].addSC("rommon:", "Copy to rommon: file system");
		enableC.copy["running-config"].addSC("running-config", "Update (merge with) current system configuration");
		enableC.copy["running-config"].addSC("startup-config", "Copy to startup configuration");
		enableC.copy["running-config"].addSC("system:", "Copy to system: file system");
		enableC.copy["running-config"].addSC("tftp:", "Copy to tftp: file system");
		enableC.copy["running-config"].addSC("xmodem:", "Copy to xmodem: file system");
		enableC.copy["running-config"].addSC("ymodem:", "Copy to ymodem: file system");
	enableC.copy.addSC("startup-config", "Copy from startup configuration");
		enableC.copy["startup-config"].addSC("flash:", "Copy to flash: file system");
		enableC.copy["startup-config"].addSC("ftp:", "Copy to ftp: file system");
		enableC.copy["startup-config"].addSC("null:", "Copy to null: file system");
		enableC.copy["startup-config"].addSC("nvram:", "Copy to nvram: file system");
		enableC.copy["startup-config"].addSC("rcp:", "Copy to rcp: file system");
		enableC.copy["startup-config"].addSC("rommon:", "Copy to rommon: file system");
		enableC.copy["startup-config"].addSC("running-config", "Update (merge with) current system configuration");
		enableC.copy["startup-config"].addSC("startup-config", "Copy to startup configuration");
		enableC.copy["startup-config"].addSC("system:", "Copy to system: file system");
		enableC.copy["startup-config"].addSC("tftp:", "Copy to tftp: file system");
		enableC.copy["startup-config"].addSC("xmodem:", "Copy to xmodem: file system");
		enableC.copy["startup-config"].addSC("ymodem:", "Copy to ymodem: file system");
	enableC.copy.addSC("system:", "Copy from system: file system");
	enableC.copy.addSC("tftp:", "Copy from tftp: file system");
	enableC.copy.addSC("xmodem:", "Copy from xmodem: file system");
	enableC.copy.addSC("ymodem:", "Copy from ymodem: file system");
enableC.addSC("debug", "Debugging functions (see also 'undebug')");
	enableC.debug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
	enableC.debug.addSC("access-expression", "Boolean access expression");
	enableC.debug.addSC("adjacency", "adjacency");
	enableC.debug.addSC("all", "Enable all debugging");
	enableC.debug.addSC("arp", "IP ARP and HP Probe transactions");
	enableC.debug.addSC("async", "Async interface information");
	enableC.debug.addSC("atm", "ATM interface packets");
	enableC.debug.addSC("call", "Call Information");
	enableC.debug.addSC("callback", "Callback activity");
	enableC.debug.addSC("cca", "CCA activity");
	enableC.debug.addSC("cch323", "CCH323 information");
	enableC.debug.addSC("ccsip", "CCSIP information");
	enableC.debug.addSC("cdp", "CDP information");
	enableC.debug.addSC("chat", "Chat scripts activity");
	enableC.debug.addSC("cns", "CNS subsys debugs");
	enableC.debug.addSC("compress", "COMPRESS traffic");
	enableC.debug.addSC("condition", "Condition");
	enableC.debug.addSC("custom-queue", "Custom output queueing");
	enableC.debug.addSC("dhcp", "DHCP client activity");
	enableC.debug.addSC("dialer", "Dial on Demand");
	enableC.debug.addSC("dnsix", "Dnsix information");
	enableC.debug.addSC("domain", "Domain Name System");
	enableC.debug.addSC("dspapi", "Generic DSP API");
	enableC.debug.addSC("dxi", "atm-dxi information");
	enableC.debug.addSC("eigrp", "EIGRP Protocol information");
	enableC.debug.addSC("entry", "Incoming queue entries");
	enableC.debug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.debug.addSC("fax", "Fax");
	enableC.debug.addSC("frame-relay", "Frame Relay");
	enableC.debug.addSC("h225", "H.225 Library Debugging");
	enableC.debug.addSC("h245", "H.245 Library Debugging");
	enableC.debug.addSC("hpi", "HPI (54x) DSP messages");
	enableC.debug.addSC("interface", "interface");
	enableC.debug.addSC("ip", "IP information");
		enableC.debug.ip.addSC("cache", "IP cache operations");
		enableC.debug.ip.addSC("cef", "IP CEF operations");
		enableC.debug.ip.addSC("cgmp", "CGMP protocol activity");
		enableC.debug.ip.addSC("dhcp", "Dynamic Host Configuration Protocol");
		enableC.debug.ip.addSC("dvmrp", "DVMRP protocol activity");
		enableC.debug.ip.addSC("eigrp", "IP-EIGRP information");
		enableC.debug.ip.addSC("error", "IP error debugging");
		enableC.debug.ip.addSC("flow", "IP Flow switching operations");
		enableC.debug.ip.addSC("ftp", "FTP dialogue");
		enableC.debug.ip.addSC("html", "HTML connections");
		enableC.debug.ip.addSC("http", "HTTP connections");
		enableC.debug.ip.addSC("icmp", "ICMP transactions");
		enableC.debug.ip.addSC("igmp", "IGMP protocol activity");
		enableC.debug.ip.addSC("igrp", "IGRP information");
		enableC.debug.ip.addSC("interface", "IP interface configuration changes");
		enableC.debug.ip.addSC("mcache", "IP multicast cache operations");
		enableC.debug.ip.addSC("mhbeat", "IP multicast heartbeat monitoring");
		enableC.debug.ip.addSC("mpacket", "IP multicast packet debugging");
		enableC.debug.ip.addSC("mrouting", "IP multicast routing table activity");
		enableC.debug.ip.addSC("msdp", "Multicast Source Discovery Protocol (MSDP)");
		enableC.debug.ip.addSC("mtag", "IP multicast tagswitching activity");
		enableC.debug.ip.addSC("nat", "NAT events");
		enableC.debug.ip.addSC("packet", "General IP debugging and IPSO security transactions");
		enableC.debug.ip.addSC("peer", "IP peer address activity");
		enableC.debug.ip.addSC("pim", "PIM protocol activity");
		enableC.debug.ip.addSC("policy", "Policy routing");
		enableC.debug.ip.addSC("rgmp", "RGMP protocol activity");
		enableC.debug.ip.addSC("rip", "RIP protocol transactions");
			enableC.debug.ip.rip.addSC("database", "RIP database events");
			enableC.debug.ip.rip.addSC("events", "RIP protocol events");
			enableC.debug.ip.rip.addSC("trigger", "RIP trigger extension");
		enableC.debug.ip.addSC("routing", "Routing table events");
			enableC.debug.ip.routing.addSC("<1-199>", "Access list");
			enableC.debug.ip.routing.addSC("<1300-2699>", "Access list (expanded range)");
			enableC.debug.ip.routing.addSC("static", "IP Static routing");
				enableC.debug.ip.routing.static.addSC("detail", "IP Static routing detail");
				enableC.debug.ip.routing.static.addSC("route", "IP Static routing route");
					enableC.debug.ip.routing.static.route.addSC("A.B.C.D", "Destination prefix");
						enableC.debug.ip.routing.static.route["A.B.C.D"].addSC("A.B.C.D", "Destination prefix mask");
				enableC.debug.ip.routing.static.addSC("summary", "IP Static routing control summary");
				enableC.debug.ip.routing.static.addSC("time", "IP Static routing time spent");
		enableC.debug.ip.addSC("rsvp", "RSVP protocol activity");
		enableC.debug.ip.addSC("rtp", "RTP information");
		enableC.debug.ip.addSC("sd", "Session Directory (SD)");
		enableC.debug.ip.addSC("security", "IP security options");
		enableC.debug.ip.addSC("socket", "Socket event");
		enableC.debug.ip.addSC("tcp", "TCP information");
		enableC.debug.ip.addSC("tempacl", "IP temporary ACL");
		enableC.debug.ip.addSC("udp", "UDP based transactions");
		enableC.debug.ip.addSC("urd", "URL RenDezvous (URD)");
	enableC.debug.addSC("ipx", "Novell/IPX information");
	enableC.debug.addSC("lapb", "LAPB protocol transactions");
	enableC.debug.addSC("list", "Set interface or/and access list for the next debug command");
	enableC.debug.addSC("llc2", "LLC2 type II Information");
	enableC.debug.addSC("mgcp", "Media Gateway Control Protocol");
	enableC.debug.addSC("modem", "Modem control/process activation");
	enableC.debug.addSC("nvram", "Debug NVRAM behavior");
	enableC.debug.addSC("packet", "Log unknown packets");
	enableC.debug.addSC("pots", "POTS information");
	enableC.debug.addSC("ppp", "PPP (Point to Point Protocol) information");
	enableC.debug.addSC("priority", "Priority output queueing");
	enableC.debug.addSC("ras", "H.323 RAS Library");
	enableC.debug.addSC("rtpspi", "RTP Service Provider Interface.");
	enableC.debug.addSC("serial", "Serial interface information");
	enableC.debug.addSC("smf", "Software MAC filter");
	enableC.debug.addSC("snapshot", "Snapshot activity");
	enableC.debug.addSC("snmp", "SNMP information");
	enableC.debug.addSC("sntp", "SNTP information");
	enableC.debug.addSC("spanning-tree", "Spanning tree debugging");
	enableC.debug.addSC("srcp", "Simple Resource Coordination Protocol");
	enableC.debug.addSC("sscop", "SSCOP");
	enableC.debug.addSC("standby", "Hot standby protocol");
	enableC.debug.addSC("tacacs", "TACACS authentication and authorization");
	enableC.debug.addSC("tbridge", "Transparent Bridging");
	enableC.debug.addSC("telnet", "Incoming telnet connections");
	enableC.debug.addSC("template", "Template activity");
	enableC.debug.addSC("tftp", "TFTP debugging");
	enableC.debug.addSC("translation", "translation rule information");
	enableC.debug.addSC("tunnel", "Generic Tunnel Interface");
	enableC.debug.addSC("voice", "VOICE information");
	enableC.debug.addSC("voip", "VOIP information");
	enableC.debug.addSC("vpdn", "VPDN information");
	enableC.debug.addSC("vpm", "Voice Port Module SPI information");
	enableC.debug.addSC("vtemplate", "Virtual Template information");
	enableC.debug.addSC("vtsp", "Voice Telephony Call Control information");
enableC.addSC("delete", "Delete a file");
enableC.addSC("dir", "List files on a filesystem");
enableC.addSC("disable", "Turn off privileged commands");
enableC.addSC("disconnect", "Disconnect an existing network connection");
enableC.addSC("elog", "Event-logging control commands");
enableC.addSC("enable", "Turn on privileged commands");
	enableC.enable.addSC("<0-15>", "Enable level");
enableC.addSC("erase", "Erase a filesystem");
enableC.addSC("exit", "Exit from the EXEC");
enableC.addSC("help", "Description of the interactive help system");
enableC.addSC("lock", "Lock the terminal");
enableC.addSC("login", "Log in as a particular user");
enableC.addSC("logout", "Exit from the EXEC");
enableC.addSC("more", "Display the contents of a file");
enableC.addSC("mrinfo", "Request neighbor and version information from a multicast router");
enableC.addSC("mstat", "Show statistics after multiple multicast traceroutes");
enableC.addSC("mtrace", "Trace reverse multicast path from destination to source");
enableC.addSC("name-connection", "Name an existing network connection");
enableC.addSC("no", "Disable debugging functions");
enableC.addSC("ping", "Send echo messages");
	enableC.ping.addSC("WORD", "Ping destination address or hostname");
	enableC.ping.addSC("ip", "IP echo");
		enableC.ping.ip.addSC("WORD", "Ping destination address or hostname");
	enableC.ping.addSC("ipx", "Novell/IPX echo");
		enableC.ping.ipx.addSC("WORD", "Ping destination address or hostname");
	enableC.ping.addSC("tag", "Tag encapsulated IP echo");
		enableC.ping.tag.addSC("WORD", "Ping destination address or hostname");
enableC.addSC("ppp", "Start IETF Point-to-Point Protocol (PPP)");
enableC.addSC("pwd", "Display current working directory");
enableC.addSC("reload", "Halt and perform a cold restart");
enableC.addSC("resume", "Resume an active network connection");
enableC.addSC("rlogin", "Open an rlogin connection");
enableC.addSC("rsh", "Execute a remote command");
enableC.addSC("send", "Send a message to other tty lines");
enableC.addSC("setup", "Run the SETUP command facility");
enableC.addSC("show", "Show running system information");
	enableC.show.addSC("access-expression", "List access expression");
	enableC.show.addSC("access-lists", "List access lists");
	enableC.show.addSC("accounting", "Accounting data for active sessions");
	enableC.show.addSC("adjacency", "Adjacent nodes");
	enableC.show.addSC("aliases", "Display alias commands");
	enableC.show.addSC("arp", "ARP table");
	enableC.show.addSC("async", "Information on terminal lines used as router interfaces");
	enableC.show.addSC("atm", "ATM information");
	enableC.show.addSC("bridge", "Bridge Forwarding/Filtering Database [verbose]");
	enableC.show.addSC("buffers", "Buffer pool statistics");
	enableC.show.addSC("call", "Show call");
	enableC.show.addSC("cca", "CCA information");
	enableC.show.addSC("cdp", "CDP information");
	enableC.show.addSC("cef", "Cisco Express Forwarding");
	enableC.show.addSC("class-map", "Show QoS Class Map");
	enableC.show.addSC("clock", "Display the system clock");
	enableC.show.addSC("cns", "CNS subsystem");
	enableC.show.addSC("compress", "Show compression statistics");
	enableC.show.addSC("configuration", "Contents of Non-Volatile memory");
	enableC.show.addSC("controllers", "Interface controller status");
	enableC.show.addSC("debugging", "State of each debugging option");
	enableC.show.addSC("derived-config", "Derived operating configuration");
	enableC.show.addSC("dhcp", "Dynamic Host Configuration Protocol status");
	enableC.show.addSC("dial-peer", "Dial Plan Mapping Table for, e.g. VoIP Peers");
	enableC.show.addSC("dialer", "Dialer parameters and statistics");
	enableC.show.addSC("dialplan", "Voice telephony dial plan");
	enableC.show.addSC("dnsix", "Shows Dnsix/DMDP information");
	enableC.show.addSC("dsl", "DSL Show Commands");
	enableC.show.addSC("dxi", "atm-dxi information");
	enableC.show.addSC("entry", "Queued terminal entries");
	enableC.show.addSC("exception", "exception informations");
	enableC.show.addSC("file", "Show filesystem information");
	enableC.show.addSC("flash:", "display information about flash: file system");
	enableC.show.addSC("frame-relay", "Frame-Relay information");
		enableC.show["frame-relay"].addSC("ip", "show frame relay IP statistics");
		enableC.show["frame-relay"].addSC("lmi", "show frame relay lmi statistics");
		enableC.show["frame-relay"].addSC("map", "Frame-Relay map table");
		enableC.show["frame-relay"].addSC("pvc", "show frame relay pvc statistics");
			enableC.show["frame-relay"].pvc.addSC("interface", "");
				enableC.show["frame-relay"].pvc.interface.addSC("Dialer", "Dialer interface");
					enableC.show["frame-relay"].pvc.interface.Dialer.addSC("<0-255>", "Dialer interface number");
				enableC.show["frame-relay"].pvc.interface.addSC("Tunnel", "Tunnel interface");
					enableC.show["frame-relay"].pvc.interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			enableC.show["frame-relay"].pvc.addSC("<16-1022>", "DLCI");
		enableC.show["frame-relay"].addSC("qos-autosense", "show frame relay qos-autosense information");
		enableC.show["frame-relay"].addSC("route", "show frame relay route");
		enableC.show["frame-relay"].addSC("traffic", "Frame-Relay protocol statistics");
		enableC.show["frame-relay"].addSC("vofr", "Show frame-relay VoFR statistics");
	enableC.show.addSC("gateway", "Show status of gateway");
	enableC.show.addSC("history", "Display the session command history");
	enableC.show.addSC("hosts", "IP domain-name, lookup style, nameservers, and host table");
	enableC.show.addSC("html", "HTML helper commands");
	enableC.show.addSC("idb", "List of Hardware Interface Descriptor Blocks");
	enableC.show.addSC("interfaces", "Interface status and configuration");
	enableC.show.addSC("ip", "IP information");
		enableC.show.ip.addSC("access-lists", "List IP access lists");
		enableC.show.ip.addSC("accounting", "The active IP accounting database");
		enableC.show.ip.addSC("aliases", "IP alias table");
		enableC.show.ip.addSC("arp", "IP ARP table");
		enableC.show.ip.addSC("cache", "IP fast-switching route cache");
		enableC.show.ip.addSC("cef", "Cisco Express Forwarding");
		enableC.show.ip.addSC("dhcp", "Show items in the DHCP database");
		enableC.show.ip.addSC("dvmrp", "DVMRP information");
		enableC.show.ip.addSC("eigrp", "IP-EIGRP show commands");
			enableC.show.ip.eigrp.addSC("interfaces", "IP-EIGRP interfaces");
				enableC.show.ip.eigrp.interfaces.addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.interfaces.addSC("ATM", "ATM interface");
					enableC.show.ip.eigrp.interfaces.ATM.addSC("<0-0>", "ATM interface number");
						enableC.show.ip.eigrp.interfaces.ATM["<0-0>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.interfaces.addSC("Async", "Async interface");
					enableC.show.ip.eigrp.interfaces.Async.addSC("<1-0>", "Async interface number");
				enableC.show.ip.eigrp.interfaces.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.eigrp.interfaces.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.eigrp.interfaces.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.eigrp.interfaces.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.eigrp.interfaces.addSC("Dialer", "Dialer interface");
					enableC.show.ip.eigrp.interfaces.Dialer.addSC("<0-255>", "Dialer interface number");
						enableC.show.ip.eigrp.interfaces.Dialer["<0-255>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.interfaces.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.eigrp.interfaces.Ethernet.addSC("<0-0>", "Ethernet interface number");
						enableC.show.ip.eigrp.interfaces.Ethernet["<0-0>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.interfaces.addSC("Lex", "Lex interface");
					enableC.show.ip.eigrp.interfaces.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.eigrp.interfaces.addSC("Loopback", "Loopback interface");
					enableC.show.ip.eigrp.interfaces.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.eigrp.interfaces.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.eigrp.interfaces.Multilink.addSC("<0-2147483647>", "Multilink interface number");
				enableC.show.ip.eigrp.interfaces.addSC("Null", "Null interface");
					enableC.show.ip.eigrp.interfaces.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.eigrp.interfaces.Null["<0-0>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.interfaces.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.eigrp.interfaces.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.eigrp.interfaces.addSC("Vif", "PGM Multicast Host interface");
				enableC.show.ip.eigrp.interfaces.addSC("Virtual-Template", "Virtual Template interface");
				enableC.show.ip.eigrp.interfaces.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show.ip.eigrp.interfaces.addSC("detail", "Show detailed peer information");
					enableC.show.ip.eigrp.interfaces.detail.addSC("<1-65535>", "AS Number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("ATM", "ATM interface");
						enableC.show.ip.eigrp.interfaces.detail.ATM.addSC("<0-0>", "ATM interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Async", "Async interface");
						enableC.show.ip.eigrp.interfaces.detail.Async.addSC("<1-0>", "Async interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.eigrp.interfaces.detail.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.eigrp.interfaces.detail.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Dialer", "Dialer interface");
						enableC.show.ip.eigrp.interfaces.detail.Dialer.addSC("<0-255>", "Dialer interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.eigrp.interfaces.detail.Ethernet.addSC("<0-0>", "Ethernet interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Lex", "Lex interface");
						enableC.show.ip.eigrp.interfaces.detail.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Loopback", "Loopback interface");
						enableC.show.ip.eigrp.interfaces.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.eigrp.interfaces.detail.Multilink.addSC("<0-2147483647>", "Multilink interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Null", "Null interface");
						enableC.show.ip.eigrp.interfaces.detail.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.eigrp.interfaces.detail.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.eigrp.interfaces.detail.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show.ip.eigrp.interfaces.addSC("static", "Show static peer information");
					enableC.show.ip.eigrp.interfaces.static.addSC("<1-65535>", "AS Number");
					enableC.show.ip.eigrp.interfaces.static.addSC("ATM", "ATM interface");
						enableC.show.ip.eigrp.interfaces.static.ATM.addSC("<0-0>", "ATM interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Async", "Async interface");
						enableC.show.ip.eigrp.interfaces.static.Async.addSC("<1-0>", "Async interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.eigrp.interfaces.static.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.eigrp.interfaces.static.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Dialer", "Dialer interface");
						enableC.show.ip.eigrp.interfaces.static.Dialer.addSC("<0-255>", "Dialer interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.eigrp.interfaces.static.Ethernet.addSC("<0-0>", "Ethernet interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Lex", "Lex interface");
						enableC.show.ip.eigrp.interfaces.static.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Loopback", "Loopback interface");
						enableC.show.ip.eigrp.interfaces.static.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.eigrp.interfaces.static.Multilink.addSC("<0-2147483647>", "Multilink interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Null", "Null interface");
						enableC.show.ip.eigrp.interfaces.static.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.eigrp.interfaces.static.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.eigrp.interfaces.static.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.eigrp.interfaces.static.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.eigrp.interfaces.static.addSC("Virtual-TokenRing", "Virtual TokenRing");
			enableC.show.ip.eigrp.addSC("neighbors", "IP-EIGRP neighbors");
				enableC.show.ip.eigrp.neighbors.addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.neighbors.addSC("ATM", "ATM interface");
					enableC.show.ip.eigrp.neighbors.ATM.addSC("<0-0>", "ATM interface number");
						enableC.show.ip.eigrp.neighbors.ATM["<0-0>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.neighbors.addSC("Async", "Async interface");
					enableC.show.ip.eigrp.neighbors.Async.addSC("<1-0>", "Async interface number");
				enableC.show.ip.eigrp.neighbors.addSC("BVI", "Bridge-Group Virtual Interface");
					enableC.show.ip.eigrp.neighbors.BVI.addSC("<1-255>", "BVI interface number");
				enableC.show.ip.eigrp.neighbors.addSC("CTunnel", "CTunnel interface");
					enableC.show.ip.eigrp.neighbors.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
				enableC.show.ip.eigrp.neighbors.addSC("Dialer", "Dialer interface");
					enableC.show.ip.eigrp.neighbors.Dialer.addSC("<0-255>", "Dialer interface number");
						enableC.show.ip.eigrp.neighbors.Dialer["<0-255>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.neighbors.addSC("Ethernet", "IEEE 802.3");
					enableC.show.ip.eigrp.neighbors.Ethernet.addSC("<0-0>", "Ethernet interface number");
						enableC.show.ip.eigrp.neighbors.Ethernet["<0-0>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.neighbors.addSC("Lex", "Lex interface");
					enableC.show.ip.eigrp.neighbors.Lex.addSC("<0-2147483647>", "Lex interface number");
				enableC.show.ip.eigrp.neighbors.addSC("Loopback", "Loopback interface");
					enableC.show.ip.eigrp.neighbors.Loopback.addSC("<0-2147483647>", "Loopback interface number");
				enableC.show.ip.eigrp.neighbors.addSC("Multilink", "Multilink-group interface");
					enableC.show.ip.eigrp.neighbors.Multilink.addSC("<0-2147483647>", "Multilink interface number");
				enableC.show.ip.eigrp.neighbors.addSC("Null", "Null interface");
					enableC.show.ip.eigrp.neighbors.Null.addSC("<0-0>", "Null interface number");
						enableC.show.ip.eigrp.neighbors.Null["<0-0>"].addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.neighbors.addSC("Tunnel", "Tunnel interface");
					enableC.show.ip.eigrp.neighbors.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
				enableC.show.ip.eigrp.neighbors.addSC("Vif", "PGM Multicast Host interface");
				enableC.show.ip.eigrp.neighbors.addSC("Virtual-Template", "Virtual Template interface");
				enableC.show.ip.eigrp.neighbors.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show.ip.eigrp.neighbors.addSC("detail", "Show detailed peer information");
					enableC.show.ip.eigrp.neighbors.detail.addSC("<1-65535>", "AS Number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("ATM", "ATM interface");
						enableC.show.ip.eigrp.neighbors.detail.ATM.addSC("<0-0>", "ATM interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Async", "Async interface");
						enableC.show.ip.eigrp.neighbors.detail.Async.addSC("<1-0>", "Async interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.eigrp.neighbors.detail.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.eigrp.neighbors.detail.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Dialer", "Dialer interface");
						enableC.show.ip.eigrp.neighbors.detail.Dialer.addSC("<0-255>", "Dialer interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.eigrp.neighbors.detail.Ethernet.addSC("<0-0>", "Ethernet interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Lex", "Lex interface");
						enableC.show.ip.eigrp.neighbors.detail.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Loopback", "Loopback interface");
						enableC.show.ip.eigrp.neighbors.detail.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.eigrp.neighbors.detail.Multilink.addSC("<0-2147483647>", "Multilink interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Null", "Null interface");
						enableC.show.ip.eigrp.neighbors.detail.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.eigrp.neighbors.detail.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.eigrp.neighbors.detail.addSC("Virtual-TokenRing", "Virtual TokenRing");
				enableC.show.ip.eigrp.neighbors.addSC("static", "Show static peer information");
					enableC.show.ip.eigrp.neighbors.static.addSC("<1-65535>", "AS Number");
					enableC.show.ip.eigrp.neighbors.static.addSC("ATM", "ATM interface");
						enableC.show.ip.eigrp.neighbors.static.ATM.addSC("<0-0>", "ATM interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Async", "Async interface");
						enableC.show.ip.eigrp.neighbors.static.Async.addSC("<1-0>", "Async interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("BVI", "Bridge-Group Virtual Interface");
						enableC.show.ip.eigrp.neighbors.static.BVI.addSC("<1-255>", "BVI interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("CTunnel", "CTunnel interface");
						enableC.show.ip.eigrp.neighbors.static.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Dialer", "Dialer interface");
						enableC.show.ip.eigrp.neighbors.static.Dialer.addSC("<0-255>", "Dialer interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Ethernet", "IEEE 802.3");
						enableC.show.ip.eigrp.neighbors.static.Ethernet.addSC("<0-0>", "Ethernet interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Lex", "Lex interface");
						enableC.show.ip.eigrp.neighbors.static.Lex.addSC("<0-2147483647>", "Lex interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Loopback", "Loopback interface");
						enableC.show.ip.eigrp.neighbors.static.Loopback.addSC("<0-2147483647>", "Loopback interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Multilink", "Multilink-group interface");
						enableC.show.ip.eigrp.neighbors.static.Multilink.addSC("<0-2147483647>", "Multilink interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Null", "Null interface");
						enableC.show.ip.eigrp.neighbors.static.Null.addSC("<0-0>", "Null interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Tunnel", "Tunnel interface");
						enableC.show.ip.eigrp.neighbors.static.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
					enableC.show.ip.eigrp.neighbors.static.addSC("Vif", "PGM Multicast Host interface");
					enableC.show.ip.eigrp.neighbors.static.addSC("Virtual-Template", "Virtual Template interface");
					enableC.show.ip.eigrp.neighbors.static.addSC("Virtual-TokenRing", "Virtual TokenRing");
			enableC.show.ip.eigrp.addSC("topology", "IP-EIGRP Topology Table");
				enableC.show.ip.eigrp.topology.addSC("<1-65535>", "AS Number");
				enableC.show.ip.eigrp.topology.addSC("A.B.C.D", "Network to display information about");
					enableC.show.ip.eigrp.topology["A.B.C.D"].addSC("A.B.C.D", "Network mask");
				enableC.show.ip.eigrp.topology.addSC("active", "Show only active entries");
				enableC.show.ip.eigrp.topology.addSC("all-links", "Show all links in topology table");
				enableC.show.ip.eigrp.topology.addSC("detail-links", "Show all links in topology table");
				enableC.show.ip.eigrp.topology.addSC("pending", "Show only entries pending transmission");
				enableC.show.ip.eigrp.topology.addSC("summary", "Show a summary of the topology table");
				enableC.show.ip.eigrp.topology.addSC("zero-successors", "Show only zero successor entries");
			enableC.show.ip.eigrp.addSC("traffic", "IP-EIGRP Traffic Statistics");
		enableC.show.ip.addSC("flow", "NetFlow switching");
		enableC.show.ip.addSC("igmp", "IGMP information");
		enableC.show.ip.addSC("interface", "IP interface status and configuration");
		enableC.show.ip.addSC("irdp", "ICMP Router Discovery Protocol");
		enableC.show.ip.addSC("local", "IP local options");
		enableC.show.ip.addSC("masks", "Masks associated with a network");
		enableC.show.ip.addSC("mcache", "IP multicast fast-switching cache");
		enableC.show.ip.addSC("mpacket", "Display possible duplicate multicast packets");
		enableC.show.ip.addSC("mroute", "IP multicast routing table");
		enableC.show.ip.addSC("msdp", "Multicast Source Discovery Protool (MSDP)");
		enableC.show.ip.addSC("mtag", "IP Multicast Tagswitching TIB");
		enableC.show.ip.addSC("nat", "IP NAT information");
			enableC.show.ip.nat.addSC("statistics", "Translation statistics");
			enableC.show.ip.nat.addSC("translations", "Translation entries");
				enableC.show.ip.nat.translations.addSC("icmp", "Show ICMP entries");
				enableC.show.ip.nat.translations.addSC("pptp", "Show PPTP entries");
				enableC.show.ip.nat.translations.addSC("tcp", "Show TCP entries");
				enableC.show.ip.nat.translations.addSC("udp", "Show UDP entries");
				enableC.show.ip.nat.translations.addSC("verbose", "Show extra information");
		enableC.show.ip.addSC("pim", "PIM information");
		enableC.show.ip.addSC("policy", "Policy routing");
		enableC.show.ip.addSC("prefix-list", "List IP prefix lists");
		enableC.show.ip.addSC("protocols", "IP routing protocol process parameters and statistics");
			enableC.show.ip.protocols.addSC("summary", "Short form answer");
			enableC.show.ip.protocols.addSC("vrf", "Display protocols for a VPN Routing/Forwarding instance");
		enableC.show.ip.addSC("redirects", "IP redirects");
		enableC.show.ip.addSC("rip", "IP RIP show commands");
		enableC.show.ip.addSC("route", "IP routing table");
			enableC.show.ip.route.addSC("bgp", "Border Gateway Protocol (BGP)");
				enableC.show.ip.route.bgp.addSC("<1-65535>", "Autonomous system number");
			enableC.show.ip.route.addSC("connected", "Connected");
			enableC.show.ip.route.addSC("egp", "Exterior Gateway Protocol (EGP)");
				enableC.show.ip.route.egp.addSC("<0-65535>", "Remote autonomous system number");
			enableC.show.ip.route.addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				enableC.show.ip.route.eigrp.addSC("<1-65535>", "Autonomous system number");
			enableC.show.ip.route.addSC("igrp", "Interior Gateway Routing Protocol (IGRP)");
				enableC.show.ip.route.igrp.addSC("<1-65535>", "Autonomous system number");
			enableC.show.ip.route.addSC("isis", "ISO IS-IS");
				enableC.show.ip.route.isis.addSC("WORD", "ISO routing area tag");
			enableC.show.ip.route.addSC("list", "IP Access list");
				enableC.show.ip.route.list.addSC("<1-199>", "IP access list number");
			enableC.show.ip.route.addSC("mobile", "Mobile routes");
			enableC.show.ip.route.addSC("odr", "On Demand stub Routes");
			enableC.show.ip.route.addSC("ospf", "Open Shortest Path First (OSPF)");
				enableC.show.ip.route.ospf.addSC("<1-65535>", "Process ID");
					enableC.show.ip.route.ospf["<1-65535>"].addSC("vrf", "VPN Routing/Forwarding Instance");
			enableC.show.ip.route.addSC("profile", "IP routing table profile");
			enableC.show.ip.route.addSC("rip", "Routing Information Protocol (RIP)");
			enableC.show.ip.route.addSC("static", "Static routes");
			enableC.show.ip.route.addSC("summary", "Summary of all routes");
			enableC.show.ip.route.addSC("supernets-only", "Show supernet entries only");
			enableC.show.ip.route.addSC("vrf", "Display routes from a VPN Routing/Forwarding instance");
		enableC.show.ip.addSC("rpf", "Display RPF information for multicast source");
		enableC.show.ip.addSC("rsvp", "RSVP information");
		enableC.show.ip.addSC("rsvp", "RSVP information");
		enableC.show.ip.addSC("rtp", "RTP/UDP/IP header-compression statistics");
		enableC.show.ip.addSC("sdr", "Session Directory (SDPv2) cache");
		enableC.show.ip.addSC("sockets", "Open IP sockets");
		enableC.show.ip.addSC("tcp", "TCP/IP header-compression statistics");
		enableC.show.ip.addSC("traffic", "IP protocol statistics");
		enableC.show.ip.addSC("vrf", "VPN Routing/Forwarding instance information");
	enableC.show.addSC("ipx", "Novell IPX information");
	enableC.show.addSC("key", "Key information");
	enableC.show.addSC("line", "TTY line information");
		enableC.show.line.addSC("<0-5>", "First Line range");
			enableC.show.line["<0-5>"].addSC("<1-5>", "Last Line range");
		enableC.show.line.addSC("async-queue", "Show async-queue");
			enableC.show.line["async-queue"].addSC("<1-99>", "rotary group number");
		enableC.show.line.addSC("console", "Primary terminal line");
			enableC.show.line.console.addSC("<0-0>", "First Line range");
		enableC.show.line.addSC("summary", "Quick line status summary");
		enableC.show.line.addSC("vty", "Virtual terminal");
			enableC.show.line.vty.addSC("<0-4>", "First Line range");
				enableC.show.line.vty["<0-4>"].addSC("<1-4>", "Last Line range");
				enableC.show.line.vty["<0-4>"].addSC("summary", "Quick line status summary");
	enableC.show.addSC("llc2", "IBM LLC2 circuit information");
	enableC.show.addSC("location", "Display the system location");
	enableC.show.addSC("logging", "Show the contents of logging buffers");
		enableC.show.logging.addSC("history", "Show the contents of syslog history table");
	enableC.show.addSC("memory", "Memory statistics");
	enableC.show.addSC("mgcp", "Display Media Gateway Control Protocol information");
	enableC.show.addSC("num-exp", "Number Expansion (Speed Dial) information");
	enableC.show.addSC("parser", "Display parser information");
	enableC.show.addSC("policy-map", "Show QoS Policy Map");
		enableC.show["policy-map"].addSC("interface", "Show Qos Policy Interface");
			enableC.show["policy-map"].interface.addSC("ATM", "ATM interface");
				enableC.show["policy-map"].interface.ATM.addSC("<0-0>", "ATM interface number");
					enableC.show["policy-map"].interface.ATM["<0-0>"].addSC("vc", "VC Service-Policy");
						enableC.show["policy-map"].interface.ATM["<0-0>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						enableC.show["policy-map"].interface.ATM["<0-0>"].vc.addSC("<1-65535>", "Enter VCI value");
			enableC.show["policy-map"].interface.addSC("Async", "Async interface");
				enableC.show["policy-map"].interface.Async.addSC("<1-0>", "Async interface number");
			enableC.show["policy-map"].interface.addSC("BVI", "Bridge-Group Virtual Interface");
				enableC.show["policy-map"].interface.BVI.addSC("<1-255>", "BVI interface number");
			enableC.show["policy-map"].interface.addSC("CTunnel", "CTunnel interface");
				enableC.show["policy-map"].interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			enableC.show["policy-map"].interface.addSC("Dialer", "Dialer interface");
				enableC.show["policy-map"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
					enableC.show["policy-map"].interface.Dialer["<0-255>"].addSC("vc", "VC Service-Policy");
						enableC.show["policy-map"].interface.Dialer["<0-255>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						enableC.show["policy-map"].interface.Dialer["<0-255>"].vc.addSC("<1-65535>", "Enter VCI value");
			enableC.show["policy-map"].interface.addSC("Ethernet", "IEEE 802.3");
				enableC.show["policy-map"].interface.Ethernet.addSC("<0-0>", "Ethernet interface number");
					enableC.show["policy-map"].interface.Ethernet["<0-0>"].addSC("vc", "VC Service-Policy");
						enableC.show["policy-map"].interface.Ethernet["<0-0>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						enableC.show["policy-map"].interface.Ethernet["<0-0>"].vc.addSC("<1-65535>", "Enter VCI value");
			enableC.show["policy-map"].interface.addSC("Group-Async", "Async Group interface");
				enableC.show["policy-map"].interface["Group-Async"].addSC("<0-0>", "Group-Async interface number");
			enableC.show["policy-map"].interface.addSC("Lex", "Lex interface");
				enableC.show["policy-map"].interface.Lex.addSC("<0-2147483647>", "Lex interface number");
			enableC.show["policy-map"].interface.addSC("Loopback", "Loopback interface");
				enableC.show["policy-map"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			enableC.show["policy-map"].interface.addSC("Multilink", "Multilink-group interface");
				enableC.show["policy-map"].interface.Multilink.addSC("<0-2147483647>", "Multilink interface number");
			enableC.show["policy-map"].interface.addSC("Null", "Null interface");
				enableC.show["policy-map"].interface.Null.addSC("<0-0>", "Null interface number");
					enableC.show["policy-map"].interface.Null["<0-0>"].addSC("vc", "VC Service-Policy");
						enableC.show["policy-map"].interface.Null["<0-0>"].vc.addSC("<0-255>", "Enter VPI/VCI value(slash required)");
						enableC.show["policy-map"].interface.Null["<0-0>"].vc.addSC("<1-65535>", "Enter VCI value");
			enableC.show["policy-map"].interface.addSC("Tunnel", "Tunnel interface");
				enableC.show["policy-map"].interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			enableC.show["policy-map"].interface.addSC("Vif", "PGM Multicast Host interface");
			enableC.show["policy-map"].interface.addSC("Virtual-Template", "Virtual Template interface");
			enableC.show["policy-map"].interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
			enableC.show["policy-map"].interface.addSC("input", "Input policy");
				enableC.show["policy-map"].interface.input.addSC("class", "Show statistics for a indvidual class");
					enableC.show["policy-map"].interface.input.class.addSC("WORD", "class-map name");
			enableC.show["policy-map"].interface.addSC("output", "Output policy");
				enableC.show["policy-map"].interface.output.addSC("class", "Show statistics for a indvidual class");
					enableC.show["policy-map"].interface.output.class.addSC("WORD", "class-map name");
	enableC.show.addSC("pots", "POTS information");
	enableC.show.addSC("ppp", "PPP parameters and statistics");
	enableC.show.addSC("privilege", "Show current privilege level");
	enableC.show.addSC("processes", "Active process statistics");
	enableC.show.addSC("protocols", "Active network routing protocols");
	enableC.show.addSC("queue", "Show queue contents");
	enableC.show.addSC("queueing", "Show queueing configuration");
	enableC.show.addSC("random-detect-group", "display random-detetct group");
	enableC.show.addSC("rawmsg", "Raw Message");
	enableC.show.addSC("registry", "Function registry information");
	enableC.show.addSC("reload", "Scheduled reload information");
	enableC.show.addSC("rhosts", "Remote-host+user equivalences");
	enableC.show.addSC("route-map", "route-map information");
	enableC.show.addSC("rtpspi", "RTP Service Provider Interface");
	enableC.show.addSC("running-config", "Current operating configuration");
		enableC.show["running-config"].addSC("interface", "Show interface configuration");
			enableC.show["running-config"].interface.addSC("ATM", "ATM interface");
				enableC.show["running-config"].interface.ATM.addSC("<0-0>", "ATM interface number");
			enableC.show["running-config"].interface.addSC("Async", "Async interface");
				enableC.show["running-config"].interface.Async.addSC("<1-0>", "Async interface number");
			enableC.show["running-config"].interface.addSC("BVI", "Bridge-Group Virtual Interface");
				enableC.show["running-config"].interface.BVI.addSC("<1-255>", "BVI interface number");
			enableC.show["running-config"].interface.addSC("CTunnel", "CTunnel interface");
				enableC.show["running-config"].interface.CTunnel.addSC("<0-2147483647>", "CTunnel interface number");
			enableC.show["running-config"].interface.addSC("Dialer", "Dialer interface");
				enableC.show["running-config"].interface.Dialer.addSC("<0-255>", "Dialer interface number");
			enableC.show["running-config"].interface.addSC("Ethernet", "IEEE 802.3");
				enableC.show["running-config"].interface.Ethernet.addSC("<0-0>", "Ethernet interface number");
			enableC.show["running-config"].interface.addSC("Group-Async", "Async Group interface");
				enableC.show["running-config"].interface["Group-Async"].addSC("<0-0>", "Group-Async interface number");
			enableC.show["running-config"].interface.addSC("Lex", "Lex interface");
				enableC.show["running-config"].interface.Lex.addSC("<0-2147483647>", "Lex interface number");
			enableC.show["running-config"].interface.addSC("Loopback", "Loopback interface");
				enableC.show["running-config"].interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
			enableC.show["running-config"].interface.addSC("Multilink", "Multilink-group interface");
				enableC.show["running-config"].interface.Multilink.addSC("<0-2147483647>", "Multilink interface number");
			enableC.show["running-config"].interface.addSC("Null", "Null interface");
				enableC.show["running-config"].interface.Null.addSC("<0-0>", "Null interface number");
			enableC.show["running-config"].interface.addSC("Tunnel", "Tunnel interface");
				enableC.show["running-config"].interface.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
			enableC.show["running-config"].interface.addSC("Vif", "PGM Multicast Host interface");
			enableC.show["running-config"].interface.addSC("Virtual-Template", "Virtual Template interface");
			enableC.show["running-config"].interface.addSC("Virtual-TokenRing", "Virtual TokenRing");
		enableC.show["running-config"].addSC("map-class", "Show map class information");
			enableC.show["running-config"]["map-class"].addSC("atm", "ATM map class information");
				enableC.show["running-config"]["map-class"].atm.addSC("WORD", "map class name");
			enableC.show["running-config"]["map-class"].addSC("dialer", "Dialer map class information");
				enableC.show["running-config"]["map-class"].dialer.addSC("WORD", "map class name");
			enableC.show["running-config"]["map-class"].addSC("frame-relay", "Frame Relay map class information");
				enableC.show["running-config"]["map-class"]["frame-relay"].addSC("WORD", "map class name");
	enableC.show.addSC("sessions", "Information about Telnet connections");
	enableC.show.addSC("sip-ua", "Show SIP User Agent");
	enableC.show.addSC("smf", "Software MAC filter");
	enableC.show.addSC("snapshot", "Snapshot parameters and statistics");
	enableC.show.addSC("snmp", "snmp statistics");
	enableC.show.addSC("sntp", "Simple network time protocol");
	enableC.show.addSC("spanning-tree", "Spanning tree topology");
	enableC.show.addSC("srcp", "Display SRCP Protocol information");
	enableC.show.addSC("sscop", "SSCOP");
	enableC.show.addSC("stacks", "Process stack utilization");
	enableC.show.addSC("standby", "Hot standby protocol information");
	enableC.show.addSC("startup-config", "Contents of startup configuration");
	enableC.show.addSC("subscriber-policy", "Subscriber policy");
	enableC.show.addSC("subsys", "Show subsystem information");
	enableC.show.addSC("tacacs", "Shows tacacs+ server statistics");
	enableC.show.addSC("tcp", "Status of TCP connections");
	enableC.show.addSC("tech-support", "Show system information for Tech-Support");
	enableC.show.addSC("template", "Template information");
	enableC.show.addSC("terminal", "Display terminal configuration parameters");
	enableC.show.addSC("time-range", "Time range");
	enableC.show.addSC("translation-rule", "Show translation rule table");
	enableC.show.addSC("users", "Display information about terminal lines");
	enableC.show.addSC("version", "System hardware and software status");
	enableC.show.addSC("voice", "Voice port configuration & stats");
	enableC.show.addSC("vpdn", "VPDN information");
	enableC.show.addSC("vtemplate", "Virtual Template interface information");
	enableC.show.addSC("whoami", "Info on current tty line");
enableC.addSC("slip", "Start Serial-line IP (SLIP)");
enableC.addSC("start-chat", "Start a chat-script on a line");
enableC.addSC("systat", "Display information about terminal lines");
enableC.addSC("telnet", "Open a telnet connection");
enableC.addSC("terminal", "Set terminal line parameters");
enableC.addSC("test", "Test subsystems, memory, and interfaces");
enableC.addSC("traceroute", "Trace route to destination");
	enableC.traceroute.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("appletalk", "AppleTalk Trace");
		enableC.traceroute.appletalk.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("clns", "ISO CLNS Trace");
		enableC.traceroute.clns.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ip", "IP Trace");
		enableC.traceroute.ip.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipv6", "IPv6 Trace");
		enableC.traceroute.ipv6.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("ipx", "IPX Trace");
		enableC.traceroute.ipx.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("oldvines", "Vines Trace (Cisco)");
		enableC.traceroute.oldvines.addSC("WORD", "Trace route to destination address or hostname");
	enableC.traceroute.addSC("vines", "Vines Trace (Banyan)");
		enableC.traceroute.vines.addSC("WORD", "Trace route to destination address or hostname");
enableC.addSC("tunnel", "Open a tunnel connection");
enableC.addSC("undebug", "Disable debugging functions (see also 'debug')");
	enableC.undebug.addSC("aaa", "AAA Authentication, Authorization and Accounting");
	enableC.undebug.addSC("access-expression", "Boolean access expression");
	enableC.undebug.addSC("adjacency", "adjacency");
	enableC.undebug.addSC("all", "Enable all debugging");
	enableC.undebug.addSC("arp", "IP ARP and HP Probe transactions");
	enableC.undebug.addSC("async", "Async interface information");
	enableC.undebug.addSC("atm", "ATM interface packets");
	enableC.undebug.addSC("call", "Call Information");
	enableC.undebug.addSC("callback", "Callback activity");
	enableC.undebug.addSC("cca", "CCA activity");
	enableC.undebug.addSC("cch323", "CCH323 information");
	enableC.undebug.addSC("ccsip", "CCSIP information");
	enableC.undebug.addSC("cdp", "CDP information");
	enableC.undebug.addSC("chat", "Chat scripts activity");
	enableC.undebug.addSC("cns", "CNS subsys debugs");
	enableC.undebug.addSC("compress", "COMPRESS traffic");
	enableC.undebug.addSC("condition", "Condition");
	enableC.undebug.addSC("custom-queue", "Custom output queueing");
	enableC.undebug.addSC("dhcp", "DHCP client activity");
	enableC.undebug.addSC("dialer", "Dial on Demand");
	enableC.undebug.addSC("dnsix", "Dnsix information");
	enableC.undebug.addSC("domain", "Domain Name System");
	enableC.undebug.addSC("dspapi", "Generic DSP API");
	enableC.undebug.addSC("dxi", "atm-dxi information");
	enableC.undebug.addSC("eigrp", "EIGRP Protocol information");
	enableC.undebug.addSC("entry", "Incoming queue entries");
	enableC.undebug.addSC("ethernet-interface", "Ethernet network interface events");
	enableC.undebug.addSC("fax", "Fax");
	enableC.undebug.addSC("frame-relay", "Frame Relay");
	enableC.undebug.addSC("h225", "H.225 Library Debugging");
	enableC.undebug.addSC("h245", "H.245 Library Debugging");
	enableC.undebug.addSC("hpi", "HPI (54x) DSP messages");
	enableC.undebug.addSC("interface", "interface");
	enableC.undebug.addSC("ip", "IP information");
	enableC.undebug.addSC("ipx", "Novell/IPX information");
	enableC.undebug.addSC("lapb", "LAPB protocol transactions");
	enableC.undebug.addSC("list", "Set interface or/and access list for the next debug command");
	enableC.undebug.addSC("llc2", "LLC2 type II Information");
	enableC.undebug.addSC("mgcp", "Media Gateway Control Protocol");
	enableC.undebug.addSC("modem", "Modem control/process activation");
	enableC.undebug.addSC("nvram", "Debug NVRAM behavior");
	enableC.undebug.addSC("packet", "Log unknown packets");
	enableC.undebug.addSC("pots", "POTS information");
	enableC.undebug.addSC("ppp", "PPP (Point to Point Protocol) information");
	enableC.undebug.addSC("priority", "Priority output queueing");
	enableC.undebug.addSC("ras", "H.323 RAS Library");
	enableC.undebug.addSC("rtpspi", "RTP Service Provider Interface.");
	enableC.undebug.addSC("serial", "Serial interface information");
	enableC.undebug.addSC("smf", "Software MAC filter");
	enableC.undebug.addSC("snapshot", "Snapshot activity");
	enableC.undebug.addSC("snmp", "SNMP information");
	enableC.undebug.addSC("sntp", "SNTP information");
	enableC.undebug.addSC("spanning-tree", "Spanning tree debugging");
	enableC.undebug.addSC("srcp", "Simple Resource Coordination Protocol");
	enableC.undebug.addSC("sscop", "SSCOP");
	enableC.undebug.addSC("standby", "Hot standby protocol");
	enableC.undebug.addSC("tacacs", "TACACS authentication and authorization");
	enableC.undebug.addSC("tbridge", "Transparent Bridging");
	enableC.undebug.addSC("telnet", "Incoming telnet connections");
	enableC.undebug.addSC("template", "Template activity");
	enableC.undebug.addSC("tftp", "TFTP debugging");
	enableC.undebug.addSC("translation", "translation rule information");
	enableC.undebug.addSC("tunnel", "Generic Tunnel Interface");
	enableC.undebug.addSC("voice", "VOICE information");
	enableC.undebug.addSC("voip", "VOIP information");
	enableC.undebug.addSC("vpdn", "VPDN information");
	enableC.undebug.addSC("vpm", "Voice Port Module SPI information");
	enableC.undebug.addSC("vtemplate", "Virtual Template information");
	enableC.undebug.addSC("vtsp", "Voice Telephony Call Control information");
enableC.addSC("verify", "Verify a file");
enableC.addSC("where", "List active connections");
enableC.addSC("write", "Write running configuration to memory, network, or terminal");
	enableC.write.addSC("erase", "Erase NV memory");
	enableC.write.addSC("memory", "Write to NV memory");
	enableC.write.addSC("network", "Write to network TFTP server");
	enableC.write.addSC("terminal", "Write to terminal");