Output=RTF%23show+running%2Dconfig%0Ahostname+RTF%0A%0Aip+subnet%2Dzero%0A%0Ainterface+Ethernet0%0A+ip+address+203%2E250%2E14%2E2+255%2E255%2E255%2E0%0A%0Ainterface+Serial1%0A+ip+address+203%2E250%2E15%2E1+255%2E255%2E255%2E252%0A%0Arouter+ospf+10%0A+network+203%2E250%2E0%2E0+0%2E0%2E255%2E255+area+0%0A%0Aip+classless%0A%0ARTF%23%0A