Content

| 5.7 |  | EIGRP Configuration Lab Exercises |
| 5.7.2 |  | Configuring EIGRP fault tolerance |

| Lab Activity Lab Exercise: Configuring EIGRP Fault Tolerance In this lab, EIGRP is configured over a full-mesh topology in order to test and observe DUAL replace a successor with a feasible successor after a link failure.

| Lab Activity e-Lab Activity: Configuring EIGRP Fault Tolerance This lab is to configure over a full mesh topology among three routers.