
intAsyncC.addSC("access-expression", "Build a bridge boolean access expression");
intAsyncC.addSC("apollo", "Apollo interface subcommands");
intAsyncC.addSC("appletalk", "Appletalk interface subcommands");
intAsyncC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
intAsyncC.addSC("asp", "ASP interface subcommands");
intAsyncC.addSC("async", "Async interface parameters");
intAsyncC.addSC("autodetect", "Autodetect Encapsulations on Serial interface");
intAsyncC.addSC("backup", "Modify backup");
intAsyncC.addSC("bandwidth", "Set bandwidth informational parameter");
	intAsyncC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intAsyncC.addSC("bridge-group", "Transparent bridging interface parameters");
intAsyncC.addSC("bsc", "BSC interface subcommands");
intAsyncC.addSC("bstun", "BSTUN interface subcommands");
intAsyncC.addSC("carrier-delay", "Specify delay for interface transitions");
intAsyncC.addSC("cdp", "CDP interface subcommands");
intAsyncC.addSC("clns", "CLNS interface subcommands");
intAsyncC.addSC("clock", "Configure serial interface clock");
	intAsyncC.clock.addSC("rate", "Configure serial interface clock speed");
		intAsyncC.clock.rate.addSC("<300-4000000>", "Choose clockrate from list above");
intAsyncC.addSC("crypto", "Encryption/Decryption commands");
	intAsyncC.crypto.addSC("map", "Assign a Crypto Map");
		intAsyncC.crypto.map.addSC("WORD", "Crypto Map tag");
intAsyncC.addSC("custom-queue-list", "Assign a custom queue list to an interface");
intAsyncC.addSC("decnet", "Interface DECnet config commands");
intAsyncC.addSC("default", "Set a command to its defaults");
intAsyncC.addSC("delay", "Specify interface throughput delay");
intAsyncC.addSC("description", "Interface specific description");
intAsyncC.addSC("dialer", "Dial-on-demand routing (DDR) commands");
intAsyncC.addSC("dialer-group", "Assign interface to dialer-list");
intAsyncC.addSC("down-when-looped", "Force looped serial interface down");
intAsyncC.addSC("dspu", "Down Stream PU");
intAsyncC.addSC("dxi", "ATM-DXI configuration commands");
intAsyncC.addSC("encapsulation", "Set encapsulation type for an interface");
	intAsyncC.encapsulation.addSC("bstun", "Block Serial tunneling (BSTUN)");
	intAsyncC.encapsulation.addSC("ppp", "Point-to-Point protocol");
	intAsyncC.encapsulation.addSC("slip", "Serial Line IP");
intAsyncC.addSC("exit", "Exit from interface configuration mode");
intAsyncC.addSC("fair-queue", "Enable Fair Queuing on an Interface");
intAsyncC.addSC("fras", "DLC Switch Interface Command");
intAsyncC.addSC("full-duplex", "Configure full-duplex operational mode");
intAsyncC.addSC("h323-gateway", "Configure H323 Gateway");
intAsyncC.addSC("half-duplex", "Configure half-duplex and related commands");
intAsyncC.addSC("help", "Description of the interactive help system");
intAsyncC.addSC("hold-queue", "Set hold queue depth");
intAsyncC.addSC("ip", "Interface Internet Protocol config commands");
	intAsyncC.ip.addSC("access-group", "Specify access control for packets");
	intAsyncC.ip.addSC("accounting", "Enable IP accounting on this interface");
	intAsyncC.ip.addSC("address", "Set the IP address of an interface");
		intAsyncC.ip.address.addSC("A.B.C.D", "IP address");
			intAsyncC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intAsyncC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		intAsyncC.ip.address.addSC("negotiated", "IP Address negotiated over PPP or via DHCP");
	intAsyncC.ip.addSC("audit", "Apply IDS audit name");
	intAsyncC.ip.addSC("auth-proxy", "Apply authenticaton proxy");
	intAsyncC.ip.addSC("authentication", "authentication subcommands");
	intAsyncC.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
			intAsyncC.ip["bandwidth-percent"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
				intAsyncC.ip["bandwidth-percent"].eigrp.addSC("<1-65535>",  "Autonomous system number");
					intAsyncC.ip["bandwidth-percent"].eigrp["<1-65535>"].addSC("<1-999999>",  "Maximum bandwidth percentage that EIGRP may use");

	intAsyncC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
	intAsyncC.ip.addSC("cgmp", "Enable/disable CGMP");
	intAsyncC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
	intAsyncC.ip.addSC("dvmrp", "DVMRP interface commands");
	intAsyncC.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
	intAsyncC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		   intAsyncC.ip["helper-address"].addSC("A.B.C.D",  "IP destination address");
	intAsyncC.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
	intAsyncC.ip.addSC("igmp", "IGMP interface commands");
	intAsyncC.ip.addSC("inspect", "Apply inspect name");
	intAsyncC.ip.addSC("irdp", "ICMP Router Discovery Protocol");
	intAsyncC.ip.addSC("load-sharing", "Style of load sharing");
	intAsyncC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	intAsyncC.ip.addSC("mobile", "Mobile IP support");
	intAsyncC.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
	intAsyncC.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
	intAsyncC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
	intAsyncC.ip.addSC("multicast", "IP multicast interface commands");
	intAsyncC.ip.addSC("nat", "NAT interface commands");
		intAsyncC.ip.nat.addSC("inside", "Inside interface for address translation");
		intAsyncC.ip.nat.addSC("outside", "Outside interface for address translation");
	intAsyncC.ip.addSC("nhrp", "NHRP interface subcommands");
	intAsyncC.ip.addSC("ospf", "OSPF interface commands");
		intAsyncC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
		intAsyncC.ip.ospf.addSC("cost", "Interface cost");
		intAsyncC.ip.ospf.cost.addSC("<1-65535>",  "Cost");
		intAsyncC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
		intAsyncC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			intAsyncC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		intAsyncC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		intAsyncC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			intAsyncC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		intAsyncC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
		intAsyncC.ip.ospf.addSC("network", "Network type");
		intAsyncC.ip.ospf.addSC("priority", "Router priority");
		intAsyncC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
		intAsyncC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
	intAsyncC.ip.addSC("pgm", "PGM Reliable Transport Protocol");
	intAsyncC.ip.addSC("pim", "PIM interface commands");
	intAsyncC.ip.addSC("policy", "Enable policy routing");
	intAsyncC.ip.addSC("probe", "Enable HP Probe support");
	intAsyncC.ip.addSC("proxy-arp", "Enable proxy ARP");
	intAsyncC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
	intAsyncC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	intAsyncC.ip.addSC("rip", "Router Information Protocol");
	intAsyncC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
	intAsyncC.ip.addSC("router", "IP router interface commands");
	intAsyncC.ip.addSC("rsvp", "RSVP interface commands");
	intAsyncC.ip.addSC("rtp", "RTP parameters");
	intAsyncC.ip.addSC("sap", "Session Advertisement Protocol interface commands");
	intAsyncC.ip.addSC("sdr", "Session Directory Protocol interface commands");
	intAsyncC.ip.addSC("security", "DDN IP Security Option");
	intAsyncC.ip.addSC("split-horizon", "Perform split horizon");
	intAsyncC.ip.addSC("summary-address", "Perform address summarization");
      intAsyncC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
         intAsyncC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
            intAsyncC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
               intAsyncC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
                  intAsyncC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");
      intAsyncC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
         intAsyncC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
            intAsyncC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
	intAsyncC.ip.addSC("tcp", "TCP header compression parameters");
	intAsyncC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
	intAsyncC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	intAsyncC.ip.addSC("verify", "Enable per packet validation");
	intAsyncC.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
	intAsyncC.ip.addSC("wccp", "WCCP interface commands");
intAsyncC.addSC("ipx", "Novell/IPX interface subcommands");
intAsyncC.addSC("isis", "IS-IS commands");
intAsyncC.addSC("iso-igrp", "ISO-IGRP interface subcommands");
intAsyncC.addSC("keepalive", "Enable keepalive");
intAsyncC.addSC("lan-name", "LAN Name command");
intAsyncC.addSC("lat", "LAT commands");
intAsyncC.addSC("llc2", "LLC2 Interface Subcommands");
intAsyncC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intAsyncC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intAsyncC.addSC("locaddr-priority", "Assign a priority group");
intAsyncC.addSC("logging", "Configure logging for interface");
intAsyncC.addSC("loopback", "Configure internal loopback on an interface");
intAsyncC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
intAsyncC.addSC("mop", "DEC MOP server commands");
intAsyncC.addSC("mpoa", "MPOA interface configuration commands");
intAsyncC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
intAsyncC.addSC("multilink-group", "Put interface in a multilink bundle");
intAsyncC.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
intAsyncC.addSC("no", "Negate a command or set its defaults");
	intAsyncC.no.addSC("access-expression", "Build a bridge boolean access expression");
	intAsyncC.no.addSC("apollo", "Apollo interface subcommands");
	intAsyncC.no.addSC("appletalk", "Appletalk interface subcommands");
	intAsyncC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intAsyncC.no.addSC("asp", "ASP interface subcommands");
	intAsyncC.no.addSC("async", "Async interface parameters");
	intAsyncC.no.addSC("autodetect", "Autodetect Encapsulations on Serial interface");
	intAsyncC.no.addSC("backup", "Modify backup parameters");
	intAsyncC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intAsyncC.no.addSC("bridge-group", "Transparent bridging interface parameters");
	intAsyncC.no.addSC("bsc", "BSC interface subcommands");
	intAsyncC.no.addSC("bstun", "BSTUN interface subcommands");
	intAsyncC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intAsyncC.no.addSC("cdp", "CDP interface subcommands");
	intAsyncC.no.addSC("clns", "CLNS interface subcommands");
	intAsyncC.no.addSC("clock", "Configure serial interface clock");
	intAsyncC.no.addSC("crypto", "Encryption/Decryption commands");
	intAsyncC.no.addSC("custom-queue-list", "Assign a custom queue list to an interface");
	intAsyncC.no.addSC("decnet", "Interface DECnet config commands");
	intAsyncC.no.addSC("delay", "Specify interface throughput delay");
	intAsyncC.no.addSC("description", "Interface specific description");
	intAsyncC.no.addSC("dialer", "Dial-on-demand routing (DDR) commands");
	intAsyncC.no.addSC("down-when-looped", "Force looped serial interface down");
	intAsyncC.no.addSC("dspu", "Down Stream PU");
	intAsyncC.no.addSC("dxi", "ATM-DXI configuration commands");
	intAsyncC.no.addSC("encapsulation", "Set encapsulation type for an interface");
	intAsyncC.no.addSC("fair-queue", "Enable Fair Queuing on an Interface");
	intAsyncC.no.addSC("fras", "DLC Switch Interface Command");
	intAsyncC.no.addSC("full-duplex", "Configure full-duplex operational mode");
	intAsyncC.no.addSC("h323-gateway", "Configure H323 Gateway");
	intAsyncC.no.addSC("half-duplex", "Configure half-duplex and related commands");
	intAsyncC.no.addSC("hold-queue", "Set hold queue depth");
	intAsyncC.no.addSC("ip", "Interface Internet Protocol config commands");
		intAsyncC.no.ip.addSC("access-group", "Specify access control for packets");
		intAsyncC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
		intAsyncC.no.ip.addSC("address", "Set the IP address of an interface");
			intAsyncC.no.ip.address.addSC("A.B.C.D", "IP address");
				intAsyncC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					intAsyncC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
			intAsyncC.no.ip.address.addSC("negotiated", "IP Address negotiated over PPP or via DHCP");
		intAsyncC.no.ip.addSC("audit", "Apply IDS audit name");
		intAsyncC.no.ip.addSC("auth-proxy", "Apply authenticaton proxy");
		intAsyncC.no.ip.addSC("authentication", "authentication subcommands");
		intAsyncC.no.ip.addSC("bandwidth-percent", "Set EIGRP bandwidth limit");
		intAsyncC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intAsyncC.no.ip.addSC("cgmp", "Enable/disable CGMP");
		intAsyncC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intAsyncC.no.ip.addSC("dvmrp", "DVMRP interface commands");
		intAsyncC.no.ip.addSC("hello-interval", "Configures IP-EIGRP hello interval");
		intAsyncC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		intAsyncC.no.ip.addSC("hold-time", "Configures IP-EIGRP hold time");
		intAsyncC.no.ip.addSC("igmp", "IGMP interface commands");
		intAsyncC.no.ip.addSC("inspect", "Apply inspect name");
		intAsyncC.no.ip.addSC("irdp", "ICMP Router Discovery Protocol");
		intAsyncC.no.ip.addSC("load-sharing", "Style of load sharing");
		intAsyncC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		intAsyncC.no.ip.addSC("mobile", "Mobile IP support");
		intAsyncC.no.ip.addSC("mrm", "Configure IP Multicast Routing Monitor tester");
		intAsyncC.no.ip.addSC("mroute-cache", "Enable switching cache for incoming multicast packets");
		intAsyncC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intAsyncC.no.ip.addSC("multicast", "IP multicast interface commands");
		intAsyncC.no.ip.addSC("nat", "NAT interface commands");
		intAsyncC.no.ip.addSC("nhrp", "NHRP interface subcommands");
		intAsyncC.no.ip.addSC("ospf", "OSPF interface commands");
		intAsyncC.no.ip.addSC("pgm", "PGM Reliable Transport Protocol");
		intAsyncC.no.ip.addSC("pim", "PIM interface commands");
		intAsyncC.no.ip.addSC("policy", "Enable policy routing");
		intAsyncC.no.ip.addSC("probe", "Enable HP Probe support");
		intAsyncC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		intAsyncC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intAsyncC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		intAsyncC.no.ip.addSC("rip", "Router Information Protocol");
		intAsyncC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		intAsyncC.no.ip.addSC("router", "IP router interface commands");
		intAsyncC.no.ip.addSC("rsvp", "RSVP interface commands");
		intAsyncC.no.ip.addSC("rtp", "RTP parameters");
		intAsyncC.no.ip.addSC("sap", "Session Advertisement Protocol interface commands");
		intAsyncC.no.ip.addSC("sdr", "Session Directory Protocol interface commands");
		intAsyncC.no.ip.addSC("security", "DDN IP Security Option");
		intAsyncC.no.ip.addSC("split-horizon", "Perform split horizon");
		intAsyncC.no.ip.addSC("summary-address", "Perform address summarization");
		intAsyncC.no.ip.addSC("tcp", "TCP header compression parameters");
		intAsyncC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intAsyncC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		intAsyncC.no.ip.addSC("verify", "Enable per packet validation");
		intAsyncC.no.ip.addSC("vrf", "VPN Routing/Forwarding parameters on the interface");
		intAsyncC.no.ip.addSC("wccp", "WCCP interface commands");
	intAsyncC.no.addSC("ipx", "Novell/IPX interface subcommands");
	intAsyncC.no.addSC("isis", "IS-IS commands");
	intAsyncC.no.addSC("iso-igrp", "ISO-IGRP interface subcommands");
	intAsyncC.no.addSC("keepalive", "Enable keepalive");
	intAsyncC.no.addSC("lan-name", "LAN Name command");
	intAsyncC.no.addSC("lat", "LAT commands");
	intAsyncC.no.addSC("llc2", "LLC2 Interface Subcommands");
	intAsyncC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intAsyncC.no.addSC("locaddr-priority", "Assign a priority group");
	intAsyncC.no.addSC("logging", "Configure logging for interface");
	intAsyncC.no.addSC("loopback", "Configure internal loopback on an interface");
	intAsyncC.no.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intAsyncC.no.addSC("mop", "DEC MOP server commands");
	intAsyncC.no.addSC("mpoa", "MPOA interface configuration commands");
	intAsyncC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intAsyncC.no.addSC("netbios", "Use a defined NETBIOS access list or enable name-caching");
	intAsyncC.no.addSC("shutdown","Shutdown the selected interface");

intAsyncC.addSC("ntp", "Configure NTP");
intAsyncC.addSC("peer", "Peer parameters for point to point interfaces");
intAsyncC.addSC("ppp", "Point-to-Point Protocol");
	intAsyncC.ppp.addSC("authentication", "Set PPP link authentication method");
		intAsyncC.ppp.authentication.addSC("chap", "Challenge Handshake Authentication Protocol (CHAP)");
			intAsyncC.ppp.authentication.chap.addSC("callin", "Authenticate remote on incoming call only");
			intAsyncC.ppp.authentication.chap.addSC("if-needed", "Do not negotiate PAP or CHAP if user has already authenticated");
		intAsyncC.ppp.authentication.addSC("ms-chap", "Microsoft Challenge Handshake Authentication Protocol (MS-CHAP)");
		intAsyncC.ppp.authentication.addSC("pap", "Password Authentication Protocol (PAP)");
			intAsyncC.ppp.authentication.pap.addSC("callin", "Authenticate remote on incoming call only");
			intAsyncC.ppp.authentication.pap.addSC("chap", "Challenge Handshake Authentication Protocol (CHAP)");
				intAsyncC.ppp.authentication.pap.chap.addSC("callin", "Authenticate remote on incoming call only");
			intAsyncC.ppp.authentication.pap.addSC("if-needed", "Do not negotiate PAP or CHAP if user has already authenticated");
			intAsyncC.ppp.authentication.pap.addSC("ms-chap", "Microsoft Challenge Handshake Authentication Protocol (MS-CHAP)");
				intAsyncC.ppp.authentication.pap["ms-chap"].addSC("callin", "Authenticate remote on incoming call only");
				intAsyncC.ppp.authentication.pap["ms-chap"].addSC("chap", "Challenge Handshake Authentication Protocol (CHAP)");
					intAsyncC.ppp.authentication.pap["ms-chap"].chap.addSC("callin", "Authenticate remote on incoming call only");
				intAsyncC.ppp.authentication.pap["ms-chap"].addSC("if-needed", "Do not negotiate PAP or CHAP if user has already authenticated");
	intAsyncC.ppp.addSC("bridge", "Enable PPP bridge translation");
	intAsyncC.ppp.addSC("callback", "Set PPP link callback option");
	intAsyncC.ppp.addSC("chap", "Set CHAP authentication parameters");
	intAsyncC.ppp.addSC("compression", "Enable PPP Compression control negotiation");
	intAsyncC.ppp.addSC("ipcp", "Set IPCP negotiation options");
	intAsyncC.ppp.addSC("lcp", "PPP LCP configuration");
	intAsyncC.ppp.addSC("max-bad-auth", "Allow multiple authentication failures");
	intAsyncC.ppp.addSC("multilink", "Make interface multilink capable");
	intAsyncC.ppp.addSC("pap", "Set PAP authentication parameters");
		intAsyncC.ppp.pap.addSC("refuse", "Refuse to authenticate using PAP");
		intAsyncC.ppp.pap.addSC("sent-username", "Set outbound PAP username");
			intAsyncC.ppp.pap["sent-username"].addSC("WORD", "Outbound PAP username");
				intAsyncC.ppp.pap["sent-username"].WORD.addSC("password", "Set outbound PAP password");
					intAsyncC.ppp.pap["sent-username"].WORD.password.addSC("<0-7>", "Encryption type (0=not yet encrypted)");
						intAsyncC.ppp.pap["sent-username"].WORD.password["<0-7>"].addSC("LINE", "Outbound PAP password");
	intAsyncC.ppp.addSC("quality", "Set minimum Link Quality before link is down");
	intAsyncC.ppp.addSC("reliable-link", "Use LAPB with PPP to provide a reliable link");
	intAsyncC.ppp.addSC("timeout", "Set PPP timeout parameters");
	intAsyncC.ppp.addSC("use-tacacs", "Use TACACS to verify PPP authentications");
intAsyncC.addSC("priority-group", "Assign a priority group to an interface");
intAsyncC.addSC("pulse-time", "Enables pulsing of DTR during resets");
intAsyncC.addSC("random-detect", "Enable Weighted Random Early Detection (WRED) on an Interface");
intAsyncC.addSC("rate-limit", "Rate Limit");
intAsyncC.addSC("sap-priority", "Assign a priority group");
intAsyncC.addSC("sdllc", "Configure SDLC to LLC2 translation");
intAsyncC.addSC("serial", "serial interface commands");
intAsyncC.addSC("service-policy", "Configure QoS Service Policy");
intAsyncC.addSC("shutdown", "Shutdown the selected interface");
intAsyncC.addSC("smds", "Modify SMDS parameters");
intAsyncC.addSC("smrp", "Simple Multicast Routing Protocol interface subcommands");
intAsyncC.addSC("sna", "SNA pu configuration");
intAsyncC.addSC("snapshot", "Configure snapshot support on the interface");
intAsyncC.addSC("snmp", "Modify SNMP interface parameters");
intAsyncC.addSC("stun", "STUN interface subcommands");
intAsyncC.addSC("tarp", "TARP interface subcommands");
intAsyncC.addSC("timeout", "Define timeout values for this interface");
intAsyncC.addSC("traffic-shape", "Enable Traffic Shaping on an Interface or Sub-Interface");
intAsyncC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
intAsyncC.addSC("tx-queue-limit", "Configure card level transmit queue limit");
intAsyncC.addSC("vines", "VINES interface subcommands");
intAsyncC.addSC("xns", "XNS interface subcommands");
