RTD#show running-config
ip subnet-zero
interface Serial0/0
ip address 192.68.12.1 255.255.255.0
router ospf 10
network 192.68.0.0 0.0.255.255 area 0
router bgp 2
neighbor 192.68.5.1 remote-as 3
neighbor 192.68.5.1 ebgp-multihop 2
no auto-summary
ip classless
RTD#
