Router-C#show ip bgp neighbors
BGP neighbor is 3.0.0.1,  remote AS 300, external link
  BGP version 4, remote router ID 10.0.0.1
  BGP state = Established, up for 02:21:39
  Last read 00:00:40, hold time is 180, keepalive interval is 60 seconds
  Neighbor capabilities:
    Route refresh: advertised and received
    Address family IPv4 Unicast: advertised and received
  Received 179 messages, 0 notifications, 0 in queue
  Sent 177 messages, 0 notifications, 0 in queue
  Route refresh request: received 0, sent 0
  Minimum time between advertisement runs is 30 seconds

 For address family: IPv4 Unicast
  BGP table version 6, neighbor version 6
  Index 1, Offset 0, Mask 0x2
  2 accepted prefixes consume 72 bytes
  Prefix advertised 4, suppressed 0, withdrawn 0

  Connections established 4; dropped 3
  Last reset 02:22:00, due to User reset
Connection state is ESTAB, I/O status: 1, unread input bytes: 0
Local host: 3.0.0.2, Local port: 11005
Foreign host: 3.0.0.1, Foreign port: 179

Enqueued packets for retransmit: 0, input: 0  mis-ordered: 0 (0 bytes)

Event Timers (current time is 0xD9AC60):
Timer          Starts    Wakeups            Next
Retrans           146          0             0x0
TimeWait            0          0             0x0
AckHold           148        101             0x0
SendWnd             0          0             0x0
KeepAlive           0          0             0x0
GiveUp              0          0             0x0
PmtuAger            0          0             0x0
DeadWait            0          0             0x0

iss: 2473456117  snduna: 2473458926  sndnxt: 2473458926     sndwnd:  15054
irs: 2496095970  rcvnxt: 2496098890  rcvwnd:      14929  delrcvwnd:   1455

SRTT: 300 ms, RTTO: 607 ms, RTV: 3 ms, KRTT: 0 ms
minRTT: 16 ms, maxRTT: 300 ms, ACK hold: 200 ms
Flags: higher precedence, nagle

Datagrams (max data segment is 1460 bytes):
Rcvd: 199 (out of order: 0), with data: 148, total data bytes: 2919
Sent: 249 (retransmit: 0), with data: 145, total data bytes: 2808
Router-C#
