Output=Current+configuration%3A%0A%21%0Aversion+12%2E0%0Aservice+timestamps+debug+uptime%0Aservice+timestamps+log+uptime%0Ano+service+password%2Dencryption%0A%21%0Ahostname+Router%2DA%0A%21%0Aenable+secret+5+%241%24fZNO%240NTNtxFEV6HMoU3sSKeIq%2E%0A%21%0Aip+subnet%2Dzero%0A%21%0Aip+audit+notify+log%0Aip+audit+po+max%2Devents+100%0A%21%0Aprocess%2Dmax%2Dtime+200%0A%21%0Ainterface+FastEthernet0%2F0%0A+ip+address+12%2E0%2E0%2E1+255%2E0%2E0%2E0%0A+no+ip+directed%2Dbroadcast%0A%21%0Ainterface+Serial0%2F0%0A+no+ip+address%0A+no+ip+directed%2Dbroadcast%0A+no+ip+mroute%2Dcache%0A+shutdown%0A%21%0Ainterface+FastEthernet0%2F1%0A+no+ip+address%0A+no+ip+directed%2Dbroadcast%0A+shutdown%0A%21%0Ainterface+Serial0%2F1%0A+ip+address+2%2E0%2E0%2E2+255%2E255%2E255%2E0%0A+no+ip+directed%2Dbroadcast%0A%21%0Arouter+eigrp+300%0A+network+2%2E0%2E0%2E0%0A+network+12%2E0%2E0%2E0%0A%21%0Arouter+bgp+300%0A+no+synchronization%0A+network+12%2E0%2E0%2E0%0A+neighbor+2%2E0%2E0%2E1+remote%2Das+300%0A%21%0Aip+classless%0Ano+ip+http+server%0A%21%0Aline+con+0%0A+transport+input+none%0Aline+aux+0%0Aline+vty+0+4%0A+password+cisco%0A+login%0A%21%0Ano+scheduler+allocate%0Aend%0A