
intLoopBackC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intLoopBackC.arp.addSC("arpa", "Standard arp protocol");
	intLoopBackC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	intLoopBackC.arp.addSC("probe", "HP style arp protocol");
	intLoopBackC.arp.addSC("snap", "IEEE 802.3 style arp");
	intLoopBackC.arp.addSC("timeout", "Set ARP cache timeout");
		intLoopBackC.arp.timeout.addSC("<0-2147483>", "Seconds");
intLoopBackC.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intLoopBackC.addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC["carrier-delay"].addSC("<0-60>", "Carrier Transitions delay seconds");
	intLoopBackC["carrier-delay"].addSC("msec", "delay specified in milliseconds");
		intLoopBackC["carrier-delay"].msec.addSC("<0-1000>", "Carrier Transitions delay milliseconds");
intLoopBackC.addSC("cdp", "CDP interface subcommands");
	intLoopBackC.cdp.addSC("enable", "Enable CDP on interface");
intLoopBackC.addSC("default", "Set a command to its defaults");
	intLoopBackC["default"].addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intLoopBackC["default"].arp.addSC("arpa", "Standard arp protocol");
		intLoopBackC["default"].arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		intLoopBackC["default"].arp.addSC("probe", "HP style arp protocol");
		intLoopBackC["default"].arp.addSC("snap", "IEEE 802.3 style arp");
		intLoopBackC["default"].arp.addSC("timeout", "Set ARP cache timeout");
	intLoopBackC["default"].addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC["default"].addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC["default"].addSC("cdp", "CDP interface subcommands");
		intLoopBackC["default"].cdp.addSC("enable", "Enable CDP on interface");
intLoopBackC.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
intLoopBackC.addSC("description", "Interface specific description");
	intLoopBackC.description.addSC("LINE", "Up to 240 characters describing this interface");
intLoopBackC.addSC("dot1x", "IEEE 802.1X subsystem");
	intLoopBackC.dot1x.addSC("multiple-hosts", "Open port to multiple hosts when authenticated");
	intLoopBackC.dot1x.addSC("port-control", "Control port authentication");
		intLoopBackC.dot1x["port-control"].addSC("auto", "Authenticate automatically");
		intLoopBackC.dot1x["port-control"].addSC("force-authorized", "Force port to authorized state");
		intLoopBackC.dot1x["port-control"].addSC("force-unauthorized", "Force port to unauthorized state");
intLoopBackC.addSC("exit", "Exit from interface configuration mode");
intLoopBackC.addSC("help", "Description of the interactive help system");
intLoopBackC.addSC("hold-queue", "Set hold queue depth");
	intLoopBackC["hold-queue"].addSC("<0-4096>", "Queue length");
		intLoopBackC["hold-queue"]["<0-4096>"].addSC("in", "Input queue");
		intLoopBackC["hold-queue"]["<0-4096>"].addSC("out", "Output queue");
intLoopBackC.addSC("ip", "Interface Internet Protocol config commands");
	intLoopBackC.ip.addSC("access-group", "Specify access control for packets");
		intLoopBackC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
		intLoopBackC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
		intLoopBackC.ip["access-group"].addSC("WORD", "Access-list name");
			intLoopBackC.ip["access-group"].WORD.addSC("in", "inbound packets");
	intLoopBackC.ip.addSC("accounting", "Enable IP accounting on this interface");
		intLoopBackC.ip.accounting.addSC("access-violations", "Account for IP packets violating access lists on this interface");
		intLoopBackC.ip.accounting.addSC("output-packets", "Account for IP packets output on this interface");
		intLoopBackC.ip.accounting.addSC("precedence", "Count packets by IP precedence on this interface");
			intLoopBackC.ip.accounting.precedence.addSC("input", "received packets");
			intLoopBackC.ip.accounting.precedence.addSC("output", "transmitted packets");
	intLoopBackC.ip.addSC("address", "Set the IP address of an interface");
		intLoopBackC.ip.address.addSC("A.B.C.D", "IP address");
			intLoopBackC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intLoopBackC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	intLoopBackC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intLoopBackC.ip["broadcast-address"].addSC("A.B.C.D", "IP broadcast address");
	intLoopBackC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intLoopBackC.ip["directed-broadcast"].addSC("<1-199>", "A standard IP access list number");
		intLoopBackC.ip["directed-broadcast"].addSC("<1300-2699>", "A standard IP expanded access list number");
	intLoopBackC.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
		intLoopBackC.ip["helper-address"].addSC("A.B.C.D", "IP destination address");
	intLoopBackC.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
	intLoopBackC.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
	intLoopBackC.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intLoopBackC.ip.mtu.addSC("<68-1000000>", "MTU (bytes)");
	intLoopBackC.ip.addSC("probe", "Enable HP Probe support");
		intLoopBackC.ip.probe.addSC("proxy", "Proxy support");
	intLoopBackC.ip.addSC("proxy-arp", "Enable proxy ARP");
	intLoopBackC.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intLoopBackC.ip["rarp-server"].addSC("A.B.C.D", "IP server address");
	intLoopBackC.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
	intLoopBackC.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
		intLoopBackC.ip["route-cache"].addSC("same-interface", "Enable fast-switching on the same interface");
	intLoopBackC.ip.addSC("security", "DDN IP Security Option");
		intLoopBackC.ip.security.addSC("add", "Ensure all outgoing packets have a basic security option");
		intLoopBackC.ip.security.addSC("aeso", "Specify AESO sources");
			intLoopBackC.ip.security.aeso.addSC("<0-255>", "ESO source");
				intLoopBackC.ip.security.aeso["<0-255>"].addSC("Hex-data", "Compartment bits in hex");
		intLoopBackC.ip.security.addSC("dedicated", "Set interface to specified level and authorities");
			intLoopBackC.ip.security.dedicated.addSC("Unclassified", "");
				intLoopBackC.ip.security.dedicated.Unclassified.addSC("doe", "");
				intLoopBackC.ip.security.dedicated.Unclassified.addSC("genser", "");
				intLoopBackC.ip.security.dedicated.Unclassified.addSC("nsa", "");
				intLoopBackC.ip.security.dedicated.Unclassified.addSC("sci", "");
				intLoopBackC.ip.security.dedicated.Unclassified.addSC("siop-esi", "");
			intLoopBackC.ip.security.dedicated.addSC("Confidential", "");
				intLoopBackC.ip.security.dedicated.Confidential.addSC("doe", "");
				intLoopBackC.ip.security.dedicated.Confidential.addSC("genser", "");
				intLoopBackC.ip.security.dedicated.Confidential.addSC("nsa", "");
				intLoopBackC.ip.security.dedicated.Confidential.addSC("sci", "");
				intLoopBackC.ip.security.dedicated.Confidential.addSC("siop-esi", "");
			intLoopBackC.ip.security.dedicated.addSC("Secret", "");
				intLoopBackC.ip.security.dedicated.Secret.addSC("doe", "");
				intLoopBackC.ip.security.dedicated.Secret.addSC("genser", "");
				intLoopBackC.ip.security.dedicated.Secret.addSC("nsa", "");
				intLoopBackC.ip.security.dedicated.Secret.addSC("sci", "");
				intLoopBackC.ip.security.dedicated.Secret.addSC("siop-esi", "");
			intLoopBackC.ip.security.dedicated.addSC("TopSecret", "");
				intLoopBackC.ip.security.dedicated.TopSecret.addSC("doe", "");
				intLoopBackC.ip.security.dedicated.TopSecret.addSC("genser", "");
				intLoopBackC.ip.security.dedicated.TopSecret.addSC("nsa", "");
				intLoopBackC.ip.security.dedicated.TopSecret.addSC("sci", "");
				intLoopBackC.ip.security.dedicated.TopSecret.addSC("siop-esi", "");
		intLoopBackC.ip.security.addSC("eso-max", "Specify maximum sensitivity level");
			intLoopBackC.ip.security["eso-max"].addSC("<0-255>", "ESO source");
				intLoopBackC.ip.security["eso-max"]["<0-255>"].addSC("Hex-data", "Compartment bits in hex");
		intLoopBackC.ip.security.addSC("eso-min", "Specify minimum sensitivity level");
			intLoopBackC.ip.security["eso-min"].addSC("<0-255>", "ESO source");
				intLoopBackC.ip.security["eso-min"]["<0-255>"].addSC("Hex-data", "Compartment bits in hex");
		intLoopBackC.ip.security.addSC("extended-allowed", "Process packets with an extended security option");
		intLoopBackC.ip.security.addSC("extended-ignored", "Ignore extended security options on incoming packets");
		intLoopBackC.ip.security.addSC("first", "Ensure security option always first on outgoing packets");
		intLoopBackC.ip.security.addSC("ignore-authorities", "Ignore all incoming authorities fields");
		intLoopBackC.ip.security.addSC("ignore-cipso", "Ignore all incoming CIPSO fields");
		intLoopBackC.ip.security.addSC("implicit-labelling", "Accept datagrams without a security option");
			intLoopBackC.ip.security["implicit-labelling"].addSC("Unclassified", "");
				intLoopBackC.ip.security["implicit-labelling"].Unclassified.addSC("doe", "");
				intLoopBackC.ip.security["implicit-labelling"].Unclassified.addSC("genser", "");
				intLoopBackC.ip.security["implicit-labelling"].Unclassified.addSC("nsa", "");
				intLoopBackC.ip.security["implicit-labelling"].Unclassified.addSC("sci", "");
				intLoopBackC.ip.security["implicit-labelling"].Unclassified.addSC("siop-esi", "");
			intLoopBackC.ip.security["implicit-labelling"].addSC("Confidential", "");
				intLoopBackC.ip.security["implicit-labelling"].Confidential.addSC("doe", "");
				intLoopBackC.ip.security["implicit-labelling"].Confidential.addSC("genser", "");
				intLoopBackC.ip.security["implicit-labelling"].Confidential.addSC("nsa", "");
				intLoopBackC.ip.security["implicit-labelling"].Confidential.addSC("sci", "");
				intLoopBackC.ip.security["implicit-labelling"].Confidential.addSC("siop-esi", "");
			intLoopBackC.ip.security["implicit-labelling"].addSC("Secret", "");
				intLoopBackC.ip.security["implicit-labelling"].Secret.addSC("doe", "");
				intLoopBackC.ip.security["implicit-labelling"].Secret.addSC("genser", "");
				intLoopBackC.ip.security["implicit-labelling"].Secret.addSC("nsa", "");
				intLoopBackC.ip.security["implicit-labelling"].Secret.addSC("sci", "");
				intLoopBackC.ip.security["implicit-labelling"].Secret.addSC("siop-esi", "");
			intLoopBackC.ip.security["implicit-labelling"].addSC("TopSecret", "");
				intLoopBackC.ip.security["implicit-labelling"].TopSecret.addSC("doe", "");
				intLoopBackC.ip.security["implicit-labelling"].TopSecret.addSC("genser", "");
				intLoopBackC.ip.security["implicit-labelling"].TopSecret.addSC("nsa", "");
				intLoopBackC.ip.security["implicit-labelling"].TopSecret.addSC("sci", "");
				intLoopBackC.ip.security["implicit-labelling"].TopSecret.addSC("siop-esi", "");
		intLoopBackC.ip.security.addSC("multilevel", "Set interface to range of levels and authorities");
			intLoopBackC.ip.security.multilevel.addSC("Unclassified", "");
				intLoopBackC.ip.security.multilevel.Unclassified.addSC("doe", "");
				intLoopBackC.ip.security.multilevel.Unclassified.addSC("genser", "");
				intLoopBackC.ip.security.multilevel.Unclassified.addSC("nsa", "");
				intLoopBackC.ip.security.multilevel.Unclassified.addSC("sci", "");
				intLoopBackC.ip.security.multilevel.Unclassified.addSC("siop-esi", "");
				intLoopBackC.ip.security.multilevel.Unclassified.addSC("to", "Begin second part of security specification");
			intLoopBackC.ip.security.multilevel.addSC("Confidential", "");
				intLoopBackC.ip.security.multilevel.Confidential.addSC("doe", "");
				intLoopBackC.ip.security.multilevel.Confidential.addSC("genser", "");
				intLoopBackC.ip.security.multilevel.Confidential.addSC("nsa", "");
				intLoopBackC.ip.security.multilevel.Confidential.addSC("sci", "");
				intLoopBackC.ip.security.multilevel.Confidential.addSC("siop-esi", "");
				intLoopBackC.ip.security.multilevel.Confidential.addSC("to", "Begin second part of security specification");
			intLoopBackC.ip.security.multilevel.addSC("Secret", "");
				intLoopBackC.ip.security.multilevel.Secret.addSC("doe", "");
				intLoopBackC.ip.security.multilevel.Secret.addSC("genser", "");
				intLoopBackC.ip.security.multilevel.Secret.addSC("nsa", "");
				intLoopBackC.ip.security.multilevel.Secret.addSC("sci", "");
				intLoopBackC.ip.security.multilevel.Secret.addSC("siop-esi", "");
				intLoopBackC.ip.security.multilevel.Secret.addSC("to", "Begin second part of security specification");
			intLoopBackC.ip.security.multilevel.addSC("TopSecret", "");
				intLoopBackC.ip.security.multilevel.TopSecret.addSC("doe", "");
				intLoopBackC.ip.security.multilevel.TopSecret.addSC("genser", "");
				intLoopBackC.ip.security.multilevel.TopSecret.addSC("nsa", "");
				intLoopBackC.ip.security.multilevel.TopSecret.addSC("sci", "");
				intLoopBackC.ip.security.multilevel.TopSecret.addSC("siop-esi", "");
				intLoopBackC.ip.security.multilevel.TopSecret.addSC("to", "Begin second part of security specification");
		intLoopBackC.ip.security.addSC("reserved-allowed", "Admit packets with security levels currently reserved");
		intLoopBackC.ip.security.addSC("strip", "Remove any basic security options on outgoing packets");
	intLoopBackC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intLoopBackC.ip.unnumbered.addSC("Async", "Async interface");
			intLoopBackC.ip.unnumbered.Async.addSC("<1-0>", "Async interface number");
		intLoopBackC.ip.unnumbered.addSC("BVI", "Bridge-Group Virtual Interface");
			intLoopBackC.ip.unnumbered.BVI.addSC("<1-255>", "BVI interface number");
		intLoopBackC.ip.unnumbered.addSC("Dialer", "Dialer interface");
			intLoopBackC.ip.unnumbered.Dialer.addSC("<0-255>", "Dialer interface number");
		intLoopBackC.ip.unnumbered.addSC("FastEthernet", "FastEthernet IEEE 802.3");
			intLoopBackC.ip.unnumbered.FastEthernet.addSC("<0-2>", "FastEthernet interface number");
		intLoopBackC.ip.unnumbered.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
			intLoopBackC.ip.unnumbered.GigabitEthernet.addSC("<0-2>", "GigabitEthernet interface number");
		intLoopBackC.ip.unnumbered.addSC("Lex", "Lex interface");
			intLoopBackC.ip.unnumbered.Lex.addSC("<0-2147483647>", "Lex interface number");
		intLoopBackC.ip.unnumbered.addSC("Loopback", "Loopback interface");
			intLoopBackC.ip.unnumbered.Loopback.addSC("<0-2147483647>", "Loopback interface number");
		intLoopBackC.ip.unnumbered.addSC("Multilink", "Multilink-group interface");
			intLoopBackC.ip.unnumbered.Multilink.addSC("<0-2147483647>", "Multilink interface number");
		intLoopBackC.ip.unnumbered.addSC("Null", "Null interface");
			intLoopBackC.ip.unnumbered.Null.addSC("<0-0>", "Null interface number");
		intLoopBackC.ip.unnumbered.addSC("Port-channel", "Ethernet Channel of interfaces");
			intLoopBackC.ip.unnumbered["Port-channel"].addSC("<1-6>", "Port-channel interface number");
		intLoopBackC.ip.unnumbered.addSC("Tunnel", "Tunnel interface");
			intLoopBackC.ip.unnumbered.Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
		intLoopBackC.ip.unnumbered.addSC("Virtual-Template", "Virtual Template interface");
			intLoopBackC.ip.unnumbered["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
		intLoopBackC.ip.unnumbered.addSC("Virtual-TokenRing", "Virtual TokenRing");
			intLoopBackC.ip.unnumbered["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
		intLoopBackC.ip.unnumbered.addSC("Vlan", "Catalyst Vlans");
			intLoopBackC.ip.unnumbered.Vlan.addSC("<1-1001>", "Vlan interface number");
	intLoopBackC.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
	intLoopBackC.ip.addSC("verify", "Enable per packet validation");
		intLoopBackC.ip.verify.addSC("unicast", "Enable per packet validation for unicast");
			intLoopBackC.ip.verify.unicast.addSC("reverse-path", "Reverse path validation of source address");
				intLoopBackC.ip.verify.unicast["reverse-path"].addSC("<1-199>", "A standard IP access list number");
				intLoopBackC.ip.verify.unicast["reverse-path"].addSC("<1300-2699>", "A standard IP expanded access list number");
intLoopBackC.addSC("keepalive", "Enable keepalive");
	intLoopBackC.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");
intLoopBackC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intLoopBackC.addSC("logging", "Configure logging for interface");
	intLoopBackC.logging.addSC("event", "Interface events");
		intLoopBackC.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
intLoopBackC.addSC("mls", "mls interface commands");
intLoopBackC.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");
	intLoopBackC.mtu.addSC("<64-1530>", "MTU size in bytes");
intLoopBackC.addSC("no", "Negate a command or set its defaults");
	intLoopBackC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intLoopBackC.no.arp.addSC("arpa", "Standard arp protocol");
		intLoopBackC.no.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		intLoopBackC.no.arp.addSC("probe", "HP style arp protocol");
		intLoopBackC.no.arp.addSC("snap", "IEEE 802.3 style arp");
		intLoopBackC.no.arp.addSC("timeout", "Set ARP cache timeout");
	intLoopBackC.no.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.no.addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC.no.addSC("cdp", "CDP interface subcommands");
		intLoopBackC.no.cdp.addSC("enable", "Enable CDP on interface");
	intLoopBackC.no.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.no.addSC("description", "Interface specific description");
	intLoopBackC.no.addSC("dot1x", "IEEE 802.1X subsystem");
		intLoopBackC.no.dot1x.addSC("multiple-hosts", "Open port to multiple hosts when authenticated");
		intLoopBackC.no.dot1x.addSC("port-control", "Control port authentication");
	intLoopBackC.no.addSC("hold-queue", "Set hold queue depth");
		intLoopBackC.no["hold-queue"].addSC("<0-4096>", "Queue length");
		intLoopBackC.no["hold-queue"].addSC("in", "Input queue");
		intLoopBackC.no["hold-queue"].addSC("out", "Output queue");
	intLoopBackC.no.addSC("ip", "Interface Internet Protocol config commands");
		intLoopBackC.no.ip.addSC("access-group", "Specify access control for packets");
			intLoopBackC.no.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intLoopBackC.no.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			intLoopBackC.no.ip["access-group"].addSC("in", "inbound packets");
		intLoopBackC.no.ip.addSC("accounting", "Enable IP accounting on this interface");
			intLoopBackC.no.ip.accounting.addSC("access-violations", "Account for IP packets violating access lists on this interface");
			intLoopBackC.no.ip.accounting.addSC("output-packets", "Account for IP packets output on this interface");
			intLoopBackC.no.ip.accounting.addSC("precedence", "Count packets by IP precedence on this interface");
				intLoopBackC.no.ip.accounting.precedence.addSC("input", "received packets");
				intLoopBackC.no.ip.accounting.precedence.addSC("output", "transmitted packets");
		intLoopBackC.no.ip.addSC("address", "Set the IP address of an interface");
			intLoopBackC.no.ip.address.addSC("A.B.C.D", "IP address");
				intLoopBackC.no.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
					intLoopBackC.no.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
		intLoopBackC.no.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intLoopBackC.no.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intLoopBackC.no.ip.addSC("helper-address", "Specify a destination address for UDP broadcasts");
			intLoopBackC.no.ip["helper-address"].addSC("A.B.C.D", "IP destination address");
		intLoopBackC.no.ip.addSC("local-proxy-arp", "Enable local-proxy ARP");
		intLoopBackC.no.ip.addSC("mask-reply", "Enable sending ICMP Mask Reply messages");
		intLoopBackC.no.ip.addSC("mtu", "Set IP Maximum Transmission Unit");
		intLoopBackC.no.ip.addSC("probe", "Enable HP Probe support");
			intLoopBackC.no.ip.probe.addSC("proxy", "Proxy support");
		intLoopBackC.no.ip.addSC("proxy-arp", "Enable proxy ARP");
		intLoopBackC.no.ip.addSC("rarp-server", "Enable RARP server for static arp entries");
		intLoopBackC.no.ip.addSC("redirects", "Enable sending ICMP Redirect messages");
		intLoopBackC.no.ip.addSC("route-cache", "Enable fast-switching cache for outgoing packets");
			intLoopBackC.no.ip["route-cache"].addSC("same-interface", "Enable fast-switching on the same interface");
		intLoopBackC.no.ip.addSC("security", "DDN IP Security Option");
			intLoopBackC.no.ip.security.addSC("add", "Ensure all outgoing packets have a basic security option");
			intLoopBackC.no.ip.security.addSC("aeso", "Specify AESO sources");
				intLoopBackC.no.ip.security.aeso.addSC("<0-255>", "ESO source");
			intLoopBackC.no.ip.security.addSC("eso-max", "Specify maximum sensitivity level");
				intLoopBackC.no.ip.security["eso-max"].addSC("<0-255>", "ESO source");
			intLoopBackC.no.ip.security.addSC("eso-min", "Specify minimum sensitivity level");
				intLoopBackC.no.ip.security["eso-min"].addSC("<0-255>", "ESO source");
			intLoopBackC.no.ip.security.addSC("extended-allowed", "Process packets with an extended security option");
			intLoopBackC.no.ip.security.addSC("extended-ignored", "Ignore extended security options on incoming packets");
			intLoopBackC.no.ip.security.addSC("first", "Ensure security option always first on outgoing packets");
			intLoopBackC.no.ip.security.addSC("ignore-authorities", "Ignore all incoming authorities fields");
			intLoopBackC.no.ip.security.addSC("ignore-cipso", "Ignore all incoming CIPSO fields");
			intLoopBackC.no.ip.security.addSC("implicit-labelling", "Accept datagrams without a security option");
				intLoopBackC.no.ip.security["implicit-labelling"].addSC("Unclassified", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Unclassified.addSC("doe", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Unclassified.addSC("genser", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Unclassified.addSC("nsa", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Unclassified.addSC("sci", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Unclassified.addSC("siop-esi", "");
				intLoopBackC.no.ip.security["implicit-labelling"].addSC("Confidential", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Confidential.addSC("doe", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Confidential.addSC("genser", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Confidential.addSC("nsa", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Confidential.addSC("sci", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Confidential.addSC("siop-esi", "");
				intLoopBackC.no.ip.security["implicit-labelling"].addSC("Secret", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Secret.addSC("doe", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Secret.addSC("genser", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Secret.addSC("nsa", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Secret.addSC("sci", "");
					intLoopBackC.no.ip.security["implicit-labelling"].Secret.addSC("siop-esi", "");
				intLoopBackC.no.ip.security["implicit-labelling"].addSC("TopSecret", "");
					intLoopBackC.no.ip.security["implicit-labelling"].TopSecret.addSC("doe", "");
					intLoopBackC.no.ip.security["implicit-labelling"].TopSecret.addSC("genser", "");
					intLoopBackC.no.ip.security["implicit-labelling"].TopSecret.addSC("nsa", "");
					intLoopBackC.no.ip.security["implicit-labelling"].TopSecret.addSC("sci", "");
					intLoopBackC.no.ip.security["implicit-labelling"].TopSecret.addSC("siop-esi", "");
			intLoopBackC.no.ip.security.addSC("reserved-allowed", "Admit packets with security levels currently reserved");
			intLoopBackC.no.ip.security.addSC("strip", "Remove any basic security options on outgoing packets");
		intLoopBackC.no.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
		intLoopBackC.no.ip.addSC("unreachables", "Enable sending ICMP Unreachable messages");
		intLoopBackC.no.ip.addSC("verify", "Enable per packet validation");
			intLoopBackC.no.ip.verify.addSC("unicast", "Enable per packet validation for unicast");
				intLoopBackC.no.ip.verify.unicast.addSC("reverse-path", "Reverse path validation of source address");
	intLoopBackC.no.addSC("keepalive", "Enable keepalive");
		intLoopBackC.no.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");
	intLoopBackC.no.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC.no.addSC("logging", "Configure logging for interface");
		intLoopBackC.no.logging.addSC("event", "Interface events");
			intLoopBackC.no.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
	intLoopBackC.no.addSC("mls", "mls interface commands");
	intLoopBackC.no.addSC("mtu", "Set the interface Maximum Transmission Unit (MTU)");

	intLoopBackC.no.addSC("shutdown","Shutdown the selected interface");

intLoopBackC.addSC("ntp", "Configure NTP");
	intLoopBackC.ntp.addSC("broadcast", "Configure NTP broadcast service");
		intLoopBackC.ntp.broadcast.addSC("client", "Listen to NTP broadcasts");
		intLoopBackC.ntp.broadcast.addSC("destination", "Configure broadcast destination address");
			intLoopBackC.ntp.broadcast.destination.addSC("Hostname or A.B.C.D", "Destination broadcast IP address");
		intLoopBackC.ntp.broadcast.addSC("key", "Configure broadcast authentication key");
			intLoopBackC.ntp.broadcast.key.addSC("<0-4294967295>", "Broadcast key number");
				intLoopBackC.ntp.broadcast.key["<0-4294967295>"].addSC("destination", "Configure broadcast destination address");
		intLoopBackC.ntp.broadcast.addSC("version", "Configure NTP version");
			intLoopBackC.ntp.broadcast.version.addSC("<1-3>", "NTP version number");
				intLoopBackC.ntp.broadcast.version["<1-3>"].addSC("destination", "Configure broadcast destination address");
				intLoopBackC.ntp.broadcast.version["<1-3>"].addSC("key", "Configure broadcast authentication key");
	intLoopBackC.ntp.addSC("disable", "Disable NTP");
intLoopBackC.addSC("rmon", "Configure Remote Monitoring on an interface");
	intLoopBackC.rmon.addSC("collection", "Configure Remote Monitoring Collection on an interface");
		intLoopBackC.rmon.collection.addSC("history", "Configure history");
			intLoopBackC.rmon.collection.history.addSC("<1-65535>", "Set RMON collection control index");
				intLoopBackC.rmon.collection.history["<1-65535>"].addSC("buckets", "Requested buckets of intervals. Default is 50 buckets");
				intLoopBackC.rmon.collection.history["<1-65535>"].addSC("interval", "Interval to sample data for each bucket. Default is 1800 seconds");
				intLoopBackC.rmon.collection.history["<1-65535>"].addSC("owner", "Set the owner of this RMON collection");
		intLoopBackC.rmon.collection.addSC("stats", "Configure statistics");
			intLoopBackC.rmon.collection.stats.addSC("<1-65535>", "Set RMON collection control index");
				intLoopBackC.rmon.collection.stats["<1-65535>"].addSC("owner", "Configure the owner of this RMON collection");
	intLoopBackC.rmon.addSC("native", "Monitor the interface in native mode");
	intLoopBackC.rmon.addSC("promiscuous", "Monitor the interface in promiscuous mode");
intLoopBackC.addSC("service-policy", "Configure QoS Service Policy");
	intLoopBackC["service-policy"].addSC("input", "Assign policy-map to the input of an interface");
		intLoopBackC["service-policy"].input.addSC("WORD", "policy-map name");
intLoopBackC.addSC("shutdown", "Shutdown the selected interface");
intLoopBackC.addSC("snmp", "Modify SNMP interface parameters");
	intLoopBackC.snmp.addSC("trap", "Allow a specific SNMP trap");
		intLoopBackC.snmp.trap.addSC("link-status", "Allow SNMP LINKUP and LINKDOWN traps");
intLoopBackC.addSC("spanning-tree", "Spanning Tree Subsystem");
	intLoopBackC["spanning-tree"].addSC("cost", "Change an interface's spanning tree port path cost");
		intLoopBackC["spanning-tree"].cost.addSC("<1-200000000>", "port path cost");
	intLoopBackC["spanning-tree"].addSC("guard", "Change an interface's spanning tree guard mode");
		intLoopBackC["spanning-tree"].guard.addSC("none", "Set guard mode to none");
		intLoopBackC["spanning-tree"].guard.addSC("root", "Set guard mode to root guard on interface");
	intLoopBackC["spanning-tree"].addSC("port-priority", "Change an interface's spanning tree port priority");
		intLoopBackC["spanning-tree"]["port-priority"].addSC("<0-255>", "port priority");
	intLoopBackC["spanning-tree"].addSC("portfast", "Enable an interface to move directly to forwarding on link up");
	intLoopBackC["spanning-tree"].addSC("stack-port", "Enable stack port");
intLoopBackC.addSC("timeout", "Define timeout values for this interface");
	intLoopBackC.timeout.addSC("absolute", "Define session timeout value for this interface");
		intLoopBackC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
			intLoopBackC.timeout.absolute["<0-35790>"].addSC("<0-59>", "Session lifetime (in seconds)");
intLoopBackC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
	intLoopBackC["transmit-interface"].addSC("Async", "Async interface");
		intLoopBackC["transmit-interface"].Async.addSC("<1-0>", "Async interface number");
	intLoopBackC["transmit-interface"].addSC("Dialer", "Dialer interface");
		intLoopBackC["transmit-interface"].Dialer.addSC("<0-255>", "Dialer interface number");
	intLoopBackC["transmit-interface"].addSC("FastEthernet", "FastEthernet IEEE 802.3");
		intLoopBackC["transmit-interface"].FastEthernet.addSC("<0-2>", "FastEthernet interface number");
	intLoopBackC["transmit-interface"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
		intLoopBackC["transmit-interface"].GigabitEthernet.addSC("<0-2>", "GigabitEthernet interface number");
	intLoopBackC["transmit-interface"].addSC("Group-Async", "Async Group interface");
		intLoopBackC["transmit-interface"]["Group-Async"].addSC("<0-0>", "Group-Async interface number");
	intLoopBackC["transmit-interface"].addSC("Lex", "Lex interface");
		intLoopBackC["transmit-interface"].Lex.addSC("<0-2147483647>", "Lex interface number");
	intLoopBackC["transmit-interface"].addSC("Loopback", "Loopback interface");
		intLoopBackC["transmit-interface"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
	intLoopBackC["transmit-interface"].addSC("Multilink", "Multilink-group interface");
		intLoopBackC["transmit-interface"].Multilink.addSC("<0-2147483647>", "Multilink interface number");
	intLoopBackC["transmit-interface"].addSC("Null", "Null interface");
		intLoopBackC["transmit-interface"].Null.addSC("<0-0>", "Null interface number");
	intLoopBackC["transmit-interface"].addSC("Port-channel", "Ethernet Channel of interfaces");
		intLoopBackC["transmit-interface"]["Port-channel"].addSC("<1-6>", "Port-channel interface number");
	intLoopBackC["transmit-interface"].addSC("Tunnel", "Tunnel interface");
		intLoopBackC["transmit-interface"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
	intLoopBackC["transmit-interface"].addSC("Virtual-Template", "Virtual Template interface");
		intLoopBackC["transmit-interface"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
	intLoopBackC["transmit-interface"].addSC("Virtual-TokenRing", "Virtual TokenRing");
		intLoopBackC["transmit-interface"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
	intLoopBackC["transmit-interface"].addSC("Vlan", "Catalyst Vlans");
		intLoopBackC["transmit-interface"].Vlan.addSC("<1-1001>", "Vlan interface number");
intLoopBackC.addSC("tx-ring-limit", "Configure PA level transmit ring limit");
	intLoopBackC["tx-ring-limit"].addSC("<1-32767>", "Number (ring limit)");
