Output=Router+C%23show+running%2Dconfig%0Ainterface+serial+0%0Aip+address+130%2E10%2E63%2E3+255%2E255%2E255%2E0%0Ainterface+serial+1%0Aip+address+130%2E10%2E64%2E3+255%2E255%2E255%2E0%0Ainterface+ethernet+0%0Aip+address+130%2E10%2E24%2E3+255%2E255%2E255%2E0%0A%21%0Arouter+rip%0Adefault%2Dmetric+10%0A%21%0Anetwork+130%2E10%2E0%2E0%0Apassive%2Dinterface+serial+0%0Apassive%2Dinterface+serial+1%0Aredistribute+ospf+109+match+internal+external+1+external+2%0A%21%0Arouter+ospf+109%0Anetwork+130%2E10%2E63%2E0+0%2E0%2E0%2E255+area+0%0Anetwork+130%2E10%2E64%2E0+0%2E0%2E0%2E255+area+0%0Aredistribute+rip+subnets%0Adistribute%2Dlist+11+out+rip%0Aaccess%2Dlist+11+permit+130%2E10%2E24%2E0+0%2E0%2E7%2E255%0Aaccess%2Dlist+11+deny+0%2E0%2E0%2E0+255%2E255%2E255%2E255%0ARouter+C%23%0A