Output=RTG%23show+running%2Dconfig%0Ahostname+RTG%0A%0Aip+subnet%2Dzero%0A%0Ainterface+Loopback0%0A+ip+address+195%2E211%2E10%2E174+255%2E255%2E255%2E192%0A%0Ainterface+Serial0%0A+ip+address+192%2E208%2E10%2E1+255%2E255%2E255%2E252%0A%0Ainterface+Serial1%0A+ip+address+195%2E211%2E10%2E1+255%2E255%2E255%2E252%0A%0Arouter+bgp+500%0A+network+195%2E211%2E10%2E0%0A+aggregate%2Daddress+195%2E211%2E0%2E0+255%2E255%2E0%2E0+summary%2Donly%0A+neighbor+192%2E208%2E10%2E2+remote%2Das+300%0A+neighbor+192%2E208%2E10%2E2+send%2Dcommunity%0A+neighbor+192%2E208%2E10%2E2+route%2Dmap+setcommunity+out%0A+neighbor+195%2E211%2E10%2E2+remote%2Das+400%0A%21%0Aip+classless%0Aaccess%2Dlist+1+permit+195%2E211%2E0%2E0+0%2E0%2E255%2E255%0Aaccess%2Dlist+2+permit+any%0Aaccess%2Dlist+101+permit+ip+195%2E211%2E0%2E0+0%2E0%2E255%2E255+host+255%2E255%2E0%2E0%0Aroute%2Dmap+setcommunity+permit+20%0A+match+ip+address+2%0A%21%0Aroute%2Dmap+setcommunity+permit+10%0A+match+ip+address+1%0A+set+community+no%2Dexport%0A%0ARTG%23%0A