intLoopBackC.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
	intLoopBackC.arp.addSC("arpa", "Standard arp protocol");
	intLoopBackC.arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
	intLoopBackC.arp.addSC("probe", "HP style arp protocol");
	intLoopBackC.arp.addSC("snap", "IEEE 802.3 style arp");
	intLoopBackC.arp.addSC("timeout", "Set ARP cache timeout");
		intLoopBackC.arp.timeout.addSC("<0-2147483>", "Seconds");
intLoopBackC.addSC("backup", "Modify backup parameters");
	intLoopBackC.backup.addSC("delay", "Delays before backup line up or down transitions");
		intLoopBackC.backup.delay.addSC("<0-4294967294>", "Seconds");
			intLoopBackC.backup.delay["<0-4294967294>"].addSC("never", "Never deactivate the backup line");
		intLoopBackC.backup.delay.addSC("never", "Never activate the backup line");
			intLoopBackC.backup.delay.never.addSC("<0-4294967294>", "Seconds");
			intLoopBackC.backup.delay.never.addSC("never", "Never deactivate the backup line");
	intLoopBackC.backup.addSC("interface", "Configure an interface as a backup");
		intLoopBackC.backup.interface.addSC("Async", "Async interface");
			intLoopBackC.backup.interface.Async.addSC("<1-0>", "Async interface number");
		intLoopBackC.backup.interface.addSC("BVI", "Bridge-Group Virtual Interface");
			intLoopBackC.backup.interface.BVI.addSC("<1-255>", "BVI interface number");
		intLoopBackC.backup.interface.addSC("Dialer", "Dialer interface");
			intLoopBackC.backup.interface.Dialer.addSC("<0-255>", "Dialer interface number");
		intLoopBackC.backup.interface.addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
			intLoopBackC.backup.interface["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
		intLoopBackC.backup.interface.addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
			intLoopBackC.backup.interface.GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
		intLoopBackC.backup.interface.addSC("Group-Async", "Async Group interface");
			intLoopBackC.backup.interface["Group-Async"].addSC("<0-0>", "Group-Async interface number");
		intLoopBackC.backup.interface.addSC("Lex", "Lex interface");
			intLoopBackC.backup.interface.Lex.addSC("<0-2147483647>", "Lex interface number");
		intLoopBackC.backup.interface.addSC("Loopback", "Loopback interface");
			intLoopBackC.backup.interface.Loopback.addSC("<0-2147483647>", "Loopback interface number");
		intLoopBackC.backup.interface.addSC("Multilink", "Multilink-group interface");
			intLoopBackC.backup.interface.Multilink.addSC("<0-2147483647>", "Multilink interface number");

intLoopBackC.addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC.bandwidth.addSC("<1-10000000>", "Bandwidth in kilobits");
intLoopBackC.addSC("bgp-policy", "Apply policy propogated by bgp community string");
	intLoopBackC["bgp-policy"].addSC("accounting", "bgp based policy accounting of traffic");
	intLoopBackC["bgp-policy"].addSC("destination", "use destination IP address for route lookup");
		intLoopBackC["bgp-policy"].destination.addSC("ip-prec-map", "map ip precedence bits");
		intLoopBackC["bgp-policy"].destination.addSC("ip-qos-map", "set qos-group");
	intLoopBackC["bgp-policy"].addSC("source", "use source IP address for route lookup");
		intLoopBackC["bgp-policy"].source.addSC("ip-prec-map", "map ip precedence bits");
		intLoopBackC["bgp-policy"].source.addSC("ip-qos-map", "set qos-group");
intLoopBackC.addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC["carrier-delay"].addSC("<0-60>", "Carrier Transitions delay seconds");
	intLoopBackC["carrier-delay"].addSC("msec", "delay specified in milliseconds");
		intLoopBackC["carrier-delay"].msec.addSC("<0-1000>", "Carrier Transitions delay milliseconds");
intLoopBackC.addSC("cdp", "CDP interface subcommands");
	intLoopBackC.cdp.addSC("enable", "Enable CDP on interface");

intLoopBackC.addSC("default", "Set a command to its defaults");
	intLoopBackC["default"].addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intLoopBackC["default"].arp.addSC("arpa", "Standard arp protocol");
		intLoopBackC["default"].arp.addSC("frame-relay", "Enable ARP for a frame relay interface");
		intLoopBackC["default"].arp.addSC("probe", "HP style arp protocol");
		intLoopBackC["default"].arp.addSC("snap", "IEEE 802.3 style arp");
		intLoopBackC["default"].arp.addSC("timeout", "Set ARP cache timeout");
	intLoopBackC["default"].addSC("backup", "Modify backup parameters");
		intLoopBackC["default"].backup.addSC("delay", "Delays before backup line up or down transitions");
		intLoopBackC["default"].backup.addSC("interface", "Configure an interface as a backup");
		intLoopBackC["default"].backup.addSC("load", "Load thresholds for line up or down transitions");
	intLoopBackC["default"].addSC("bandwidth", "Set bandwidth informational parameter");
	intLoopBackC["default"].addSC("bgp-policy", "Apply policy propogated by bgp community string");
		intLoopBackC["default"]["bgp-policy"].addSC("accounting", "bgp based policy accounting of traffic");
		intLoopBackC["default"]["bgp-policy"].addSC("destination", "use destination IP address for route lookup");
		intLoopBackC["default"]["bgp-policy"].addSC("source", "use source IP address for route lookup");
	intLoopBackC["default"].addSC("carrier-delay", "Specify delay for interface transitions");
	intLoopBackC["default"].addSC("cdp", "CDP interface subcommands");
		intLoopBackC["default"].cdp.addSC("enable", "Enable CDP on interface");
intLoopBackC.addSC("delay", "Specify interface throughput delay");
	intLoopBackC.delay.addSC("<1-16777215>", "Throughput delay (tens of microseconds)");
intLoopBackC.addSC("description", "Interface specific description");
	intLoopBackC.description.addSC("LINE", "Up to 240 characters describing this interface");
intLoopBackC.addSC("exit", "Exit from interface configuration mode");
intLoopBackC.addSC("help", "Description of the interactive help system");
intLoopBackC.addSC("hold-queue", "Set hold queue depth");

intLoopBackC.addSC("ip", "Interface Internet Protocol config commands");
	intLoopBackC.ip.addSC("access-group", "Specify access control for packets");
		intLoopBackC.ip["access-group"].addSC("<1-199>", "IP access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"]["<1-199>"].addSC("out", "outbound packets");
		intLoopBackC.ip["access-group"].addSC("<1300-2699>", "IP expanded access list (standard or extended)");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"]["<1300-2699>"].addSC("out", "outbound packets");
		intLoopBackC.ip["access-group"].addSC("WORD", "Access-list name");
			intLoopBackC.ip["access-group"].WORD.addSC("in", "inbound packets");
			intLoopBackC.ip["access-group"].WORD.addSC("out", "outbound packets");
	intLoopBackC.ip.addSC("address", "Set the IP address of an interface");
		intLoopBackC.ip.address.addSC("A.B.C.D", "IP address");
			intLoopBackC.ip.address["A.B.C.D"].addSC("A.B.C.D", "IP subnet mask");
				intLoopBackC.ip.address["A.B.C.D"]["A.B.C.D"].addSC("secondary", "Make this IP address a secondary address");
	intLoopBackC.ip.addSC("bgp", "BGP interface commands");
		intLoopBackC.ip.bgp.addSC("fast-external-fallover", "Over-ride bgp global fast-failover whenexternal peer goes down");
			intLoopBackC.ip.bgp["fast-external-fallover"].addSC("deny", "dis-allow fast fallover");
			intLoopBackC.ip.bgp["fast-external-fallover"].addSC("permit", "allow fast fallover");
	intLoopBackC.ip.addSC("broadcast-address", "Set the broadcast address of an interface");
		intLoopBackC.ip["broadcast-address"].addSC("A.B.C.D", "IP broadcast address");
	intLoopBackC.ip.addSC("cgmp", "Enable/disable CGMP");
		intLoopBackC.ip.cgmp.addSC("proxy", "CGMP for hosts and proxy for multicast routers");
		intLoopBackC.ip.cgmp.addSC("router-only", "CGMP proxy for multicast routers only");
	intLoopBackC.ip.addSC("directed-broadcast", "Enable forwarding of directed broadcasts");
		intLoopBackC.ip["directed-broadcast"].addSC("<1-199>", "A standard IP access list number");
		intLoopBackC.ip["directed-broadcast"].addSC("<1300-2699>", "A standard IP expanded access list number");

	intLoopBackC.ip.addSC("igmp", "IGMP interface commands");
		intLoopBackC.ip.igmp.addSC("access-group", "IGMP group access group");
			intLoopBackC.ip.igmp["access-group"].addSC("<1-99>", "Access list number");
			intLoopBackC.ip.igmp["access-group"].addSC("WORD", "IP Named Standard Access list");
		intLoopBackC.ip.igmp.addSC("helper-address", "IGMP helper address");
			intLoopBackC.ip.igmp["helper-address"].addSC("A.B.C.D", "IGMP helper address");
			intLoopBackC.ip.igmp["helper-address"].addSC("udl", "Unidirectional link to forward the report");

	intLoopBackC.ip.addSC("multicast", "IP multicast interface commands");
		intLoopBackC.ip.multicast.addSC("helper-map", "Broadcast to Multicast map OR Multicast to Broadcast map");
			intLoopBackC.ip.multicast["helper-map"].addSC("A.B.C.D", "IP multicast address");
				intLoopBackC.ip.multicast["helper-map"]["A.B.C.D"].addSC("A.B.C.D", "IP multicast address or IP broadcast address");
					intLoopBackC.ip.multicast["helper-map"]["A.B.C.D"]["A.B.C.D"].addSC("<100-199>", "access-list");
					intLoopBackC.ip.multicast["helper-map"]["A.B.C.D"]["A.B.C.D"].addSC("<2000-2699>", "access-list (expanded range)");
					intLoopBackC.ip.multicast["helper-map"]["A.B.C.D"]["A.B.C.D"].addSC("WORD", "IP Named Extended Access list");
			intLoopBackC.ip.multicast["helper-map"].addSC("broadcast", "Broadcast address");
				intLoopBackC.ip.multicast["helper-map"].broadcast.addSC("A.B.C.D", "IP multicast address or IP broadcast address");
					intLoopBackC.ip.multicast["helper-map"].broadcast["A.B.C.D"].addSC("<100-199>", "access-list");
					intLoopBackC.ip.multicast["helper-map"].broadcast["A.B.C.D"].addSC("<2000-2699>", "access-list (expanded range)");
					intLoopBackC.ip.multicast["helper-map"].broadcast["A.B.C.D"].addSC("WORD", "IP Named Extended Access list");
	intLoopBackC.ip.addSC("ospf", "OSPF interface commands");
		intLoopBackC.ip.ospf.addSC("authentication", "Enable authentication");
			intLoopBackC.ip.ospf.authentication.addSC("message-digest", "Use message-digest authentication");
			intLoopBackC.ip.ospf.authentication.addSC("null", "Use no authentication");
		intLoopBackC.ip.ospf.addSC("authentication-key", "Authentication password (key)");
			intLoopBackC.ip.ospf["authentication-key"].addSC("<0-7>", "Encryption type (0 for not yet encrypted, 7 for proprietary)");
			intLoopBackC.ip.ospf["authentication-key"].addSC("LINE", "The OSPF password (key)");
		intLoopBackC.ip.ospf.addSC("cost", "Interface cost");
			intLoopBackC.ip.ospf.cost.addSC("<1-65535>", "Cost");
		intLoopBackC.ip.ospf.addSC("database-filter", "Filter OSPF LSA during synchronization and flooding");
			intLoopBackC.ip.ospf["database-filter"].addSC("all", "Filter all LSA");
				intLoopBackC.ip.ospf["database-filter"].all.addSC("out", "Outgoing LSA");
		intLoopBackC.ip.ospf.addSC("dead-interval", "Interval after which a neighbor is declared dead");
			intLoopBackC.ip.ospf["dead-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("demand-circuit", "OSPF demand circuit");
		intLoopBackC.ip.ospf.addSC("hello-interval", "Time between HELLO packets");
			intLoopBackC.ip.ospf["hello-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("message-digest-key", "Message digest authentication password (key)");
			intLoopBackC.ip.ospf["message-digest-key"].addSC("<1-255>", "Key ID");
				intLoopBackC.ip.ospf["message-digest-key"]["<1-255>"].addSC("md5", "Use MD5 algorithm");
					intLoopBackC.ip.ospf["message-digest-key"]["<1-255>"].md5.addSC("<0-7>", "Encryption type (0 for not yet encrypted, 7 for proprietary)");
					intLoopBackC.ip.ospf["message-digest-key"]["<1-255>"].md5.addSC("LINE", "The OSPF password (key)");
		intLoopBackC.ip.ospf.addSC("mtu-ignore", "Ignores the MTU in DBD packets");
		intLoopBackC.ip.ospf.addSC("network", "Network type");
			intLoopBackC.ip.ospf.network.addSC("broadcast", "Specify OSPF broadcast multi-access network");
			intLoopBackC.ip.ospf.network.addSC("non-broadcast", "Specify OSPF NBMA network");
			intLoopBackC.ip.ospf.network.addSC("point-to-multipoint", "Specify OSPF point-to-multipoint network");
				intLoopBackC.ip.ospf.network["point-to-multipoint"].addSC("non-broadcast", "Specify non-broadcast point-to-mpoint network");
			intLoopBackC.ip.ospf.network.addSC("point-to-point", "Specify OSPF point-to-point network");
		intLoopBackC.ip.ospf.addSC("priority", "Router priority");
			intLoopBackC.ip.ospf.priority.addSC("<0-255>", "Priority");
		intLoopBackC.ip.ospf.addSC("retransmit-interval", "Time between retransmitting lost link state advertisements");
			intLoopBackC.ip.ospf["retransmit-interval"].addSC("<1-65535>", "Seconds");
		intLoopBackC.ip.ospf.addSC("transmit-delay", "Link state transmit delay");
			intLoopBackC.ip.ospf["transmit-delay"].addSC("<1-65535>", "Seconds");

	intLoopBackC.ip.addSC("pim", "PIM interface commands");
		intLoopBackC.ip.pim.addSC("bsr-border", "Border of PIM domain");
		intLoopBackC.ip.pim.addSC("dense-mode", "Enable PIM dense-mode operation");
			intLoopBackC.ip.pim["dense-mode"].addSC("proxy-register", "Send proxy registers");
				intLoopBackC.ip.pim["dense-mode"]["proxy-register"].addSC("list", "Access list");
					intLoopBackC.ip.pim["dense-mode"]["proxy-register"].list.addSC("<100-199>", "Extended access list number");
					intLoopBackC.ip.pim["dense-mode"]["proxy-register"].list.addSC("<2000-2699>", "Extended access list number (expanded range)");
					intLoopBackC.ip.pim["dense-mode"]["proxy-register"].list.addSC("WORD", "IP named extended access list");
				intLoopBackC.ip.pim["dense-mode"]["proxy-register"].addSC("route-map", "Route-map");
					intLoopBackC.ip.pim["dense-mode"]["proxy-register"]["route-map"].addSC("WORD", "Route-map reference");
		intLoopBackC.ip.pim.addSC("nbma-mode", "Use Non-Broadcast Multi-Access (NBMA) mode on interface");
		intLoopBackC.ip.pim.addSC("neighbor-filter", "PIM peering filter");
			intLoopBackC.ip.pim["neighbor-filter"].addSC("<1-99>", "Access list number");
			intLoopBackC.ip.pim["neighbor-filter"].addSC("WORD", "IP Named Standard Access list");
		intLoopBackC.ip.pim.addSC("query-interval", "PIM router query interval");
			intLoopBackC.ip.pim["query-interval"].addSC("<0-65535>", "Query interval in seconds");
		intLoopBackC.ip.pim.addSC("sparse-dense-mode", "Enable PIM sparse-dense-mode operation");
		intLoopBackC.ip.pim.addSC("sparse-mode", "Enable PIM sparse-mode operation");
		intLoopBackC.ip.pim.addSC("version", "PIM version");
			intLoopBackC.ip.pim.version.addSC("<1-2>", "version number");
	intLoopBackC.ip.addSC("probe", "Enable HP Probe support");
		intLoopBackC.ip.probe.addSC("proxy", "Proxy support");

	intLoopBackC.ip.addSC("rip", "Router Information Protocol");
		intLoopBackC.ip.rip.addSC("authentication", "Authentication control");
			intLoopBackC.ip.rip.authentication.addSC("key-chain", "Authentication key-chain");
				intLoopBackC.ip.rip.authentication["key-chain"].addSC("LINE", "name of key-chain");
			intLoopBackC.ip.rip.authentication.addSC("mode", "Authentication mode");
				intLoopBackC.ip.rip.authentication.mode.addSC("md5", "Keyed message digest");
				intLoopBackC.ip.rip.authentication.mode.addSC("text", "Clear text authentication");
		intLoopBackC.ip.rip.addSC("receive", "advertisement reception");
			intLoopBackC.ip.rip.receive.addSC("version", "version control");
				intLoopBackC.ip.rip.receive.version.addSC("<1-1>", "RIP version 1");
				intLoopBackC.ip.rip.receive.version.addSC("<2-2>", "RIP version 2");

		intLoopBackC.ip.rip.addSC("send", "advertisement transmission");
			intLoopBackC.ip.rip.send.addSC("version", "version control");
				intLoopBackC.ip.rip.send.version.addSC("<1-1>", "RIP version 1");
				intLoopBackC.ip.rip.send.version.addSC("<2-2>", "RIP version 2");


	intLoopBackC.ip.addSC("split-horizon", "Perform split horizon");
		intLoopBackC.ip["split-horizon"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.ip["split-horizon"].eigrp.addSC("<1-65535>", "Autonomous system number");
	intLoopBackC.ip.addSC("summary-address", "Perform address summarization");
		intLoopBackC.ip["summary-address"].addSC("eigrp", "Enhanced Interior Gateway Routing Protocol (EIGRP)");
			intLoopBackC.ip["summary-address"].eigrp.addSC("<1-65535>", "Autonomous system number");
				intLoopBackC.ip["summary-address"].eigrp["<1-65535>"].addSC("A.B.C.D", "IP address");
					intLoopBackC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
						intLoopBackC.ip["summary-address"].eigrp["<1-65535>"]["A.B.C.D"]["A.B.C.D"].addSC("<1-255>", "Administrative distance");
		intLoopBackC.ip["summary-address"].addSC("rip", "Routing Information Protocol (RIP)");
			intLoopBackC.ip["summary-address"].rip.addSC("A.B.C.D", "IP address");
				intLoopBackC.ip["summary-address"].rip["A.B.C.D"].addSC("A.B.C.D", "IP network mask");
	intLoopBackC.ip.addSC("tcp", "TCP header compression parameters");
		intLoopBackC.ip.tcp.addSC("compression-connections", "Maximum number of compressed connections");
			intLoopBackC.ip.tcp["compression-connections"].addSC("<3-256>", "Number of connections");
		intLoopBackC.ip.tcp.addSC("header-compression", "Enable TCP header compression");
			intLoopBackC.ip.tcp["header-compression"].addSC("passive", "Compress only for destinations which send compressed headers");
	intLoopBackC.ip.addSC("unnumbered", "Enable IP processing without an explicit address");
intLoopBackC.addSC("keepalive", "Enable keepalive");
	intLoopBackC.keepalive.addSC("<0-32767>", "Keepalive period (default 10 seconds)");
intLoopBackC.addSC("load-interval", "Specify interval for load calculation for an interface");
	intLoopBackC["load-interval"].addSC("<30-600>", "Load interval delay in seconds");
intLoopBackC.addSC("logging", "Configure logging for interface");
	intLoopBackC.logging.addSC("event", "Interface events");
		intLoopBackC.logging.event.addSC("link-status", "UPDOWN and CHANGE messages");
intLoopBackC.addSC("max-reserved-bandwidth", "Maximum Reservable Bandwidth on an Interface");
	intLoopBackC["max-reserved-bandwidth"].addSC("<1-100>", "Max. reservable bandwidth as % of interface bandwidth");

intLoopBackC.addSC("no", "Negate a command or set its defaults");
	intLoopBackC.no.addSC("arp", "Set arp type (arpa, probe, snap) or timeout");
		intLoopBackC.no.arp.addSC("arpa", "Standard arp protocol");
intLoopBackC.addSC("ntp", "Configure NTP");
intLoopBackC.addSC("rate-limit", "Rate Limit");
	intLoopBackC["rate-limit"].addSC("input", "Rate limit on input");
		intLoopBackC["rate-limit"].input.addSC("<8000-2000000000>", "Bits per second");
		intLoopBackC["rate-limit"].input.addSC("access-group", "Match access list");
		intLoopBackC["rate-limit"].input.addSC("dscp", "Match dscp value");
		intLoopBackC["rate-limit"].input.addSC("qos-group", "Match qos-group ID");
	intLoopBackC["rate-limit"].addSC("output", "Rate limit on output");
		intLoopBackC["rate-limit"].output.addSC("<8000-2000000000>", "Bits per second");
		intLoopBackC["rate-limit"].output.addSC("access-group", "Match access list");
		intLoopBackC["rate-limit"].output.addSC("dscp", "Match dscp value");
		intLoopBackC["rate-limit"].output.addSC("qos-group", "Match qos-group ID");
intLoopBackC.addSC("rmon", "Configure Remote Monitoring on an interface");
intLoopBackC.addSC("service-policy", "Configure QoS Service Policy");


intLoopBackC.addSC("shutdown", "Shutdown the selected interface");
intLoopBackC.addSC("snmp", "Modify SNMP interface parameters");
	intLoopBackC.snmp.addSC("trap", "Allow a specific SNMP trap");
		intLoopBackC.snmp.trap.addSC("link-status", "Allow SNMP LINKUP and LINKDOWN traps");


intLoopBackC.addSC("spanning-tree", "Spanning Tree Subsystem");
	intLoopBackC["spanning-tree"].addSC("cost", "Change an interface's spanning tree port path cost");
		intLoopBackC["spanning-tree"].cost.addSC("<1-200000000>", "port path cost");
	intLoopBackC["spanning-tree"].addSC("guard", "Change an interface's spanning tree guard mode");
		intLoopBackC["spanning-tree"].guard.addSC("none", "Set guard mode to none");
		intLoopBackC["spanning-tree"].guard.addSC("root", "Set guard mode to root guard on interface");
	intLoopBackC["spanning-tree"].addSC("port-priority", "Change an interface's spanning tree port priority");
		intLoopBackC["spanning-tree"]["port-priority"].addSC("<0-240>", "port priority in increments of 16");
	intLoopBackC["spanning-tree"].addSC("portfast", "Enable an interface to move directly to forwarding on link up");
intLoopBackC.addSC("timeout", "Define timeout values for this interface");
	intLoopBackC.timeout.addSC("absolute", "Define session timeout value for this interface");
		intLoopBackC.timeout.absolute.addSC("<0-35790>", "Session lifetime (in minutes)");
intLoopBackC.addSC("transmit-interface", "Assign a transmit interface to a receive-only interface");
	intLoopBackC["transmit-interface"].addSC("Async", "Async interface");
		intLoopBackC["transmit-interface"].Async.addSC("<1-0>", "Async interface number");
	intLoopBackC["transmit-interface"].addSC("Dialer", "Dialer interface");
		intLoopBackC["transmit-interface"].Dialer.addSC("<0-255>", "Dialer interface number");
	intLoopBackC["transmit-interface"].addSC("GE-WAN", "GigabitEthernetWAN IEEE 802.3z");
		intLoopBackC["transmit-interface"]["GE-WAN"].addSC("<1-6>", "GE-WAN interface number");
	intLoopBackC["transmit-interface"].addSC("GigabitEthernet", "GigabitEthernet IEEE 802.3z");
		intLoopBackC["transmit-interface"].GigabitEthernet.addSC("<1-6>", "GigabitEthernet interface number");
	intLoopBackC["transmit-interface"].addSC("Group-Async", "Async Group interface");
		intLoopBackC["transmit-interface"]["Group-Async"].addSC("<0-0>", "Group-Async interface number");
	intLoopBackC["transmit-interface"].addSC("Lex", "Lex interface");
		intLoopBackC["transmit-interface"].Lex.addSC("<0-2147483647>", "Lex interface number");
	intLoopBackC["transmit-interface"].addSC("Loopback", "Loopback interface");
		intLoopBackC["transmit-interface"].Loopback.addSC("<0-2147483647>", "Loopback interface number");
	intLoopBackC["transmit-interface"].addSC("Multilink", "Multilink-group interface");
		intLoopBackC["transmit-interface"].Multilink.addSC("<0-2147483647>", "Multilink interface number");
	intLoopBackC["transmit-interface"].addSC("Null", "Null interface");
		intLoopBackC["transmit-interface"].Null.addSC("<0-0>", "Null interface number");
	intLoopBackC["transmit-interface"].addSC("Port-channel", "Ethernet Channel of interfaces");
		intLoopBackC["transmit-interface"]["Port-channel"].addSC("<1-64>", "Port-channel interface number");
	intLoopBackC["transmit-interface"].addSC("Tunnel", "Tunnel interface");
		intLoopBackC["transmit-interface"].Tunnel.addSC("<0-2147483647>", "Tunnel interface number");
	intLoopBackC["transmit-interface"].addSC("Virtual-Template", "Virtual Template interface");
		intLoopBackC["transmit-interface"]["Virtual-Template"].addSC("<1-25>", "Virtual-Template interface number");
	intLoopBackC["transmit-interface"].addSC("Virtual-TokenRing", "Virtual TokenRing");
		intLoopBackC["transmit-interface"]["Virtual-TokenRing"].addSC("<0-2147483647>", "Virtual-TokenRing interface number");
	intLoopBackC["transmit-interface"].addSC("Vlan", "Catalyst Vlans");
		intLoopBackC["transmit-interface"].Vlan.addSC("<1-1001>", "Vlan interface number");
intLoopBackC.addSC("tx-ring-limit", "Configure PA level transmit ring limit");
	intLoopBackC["tx-ring-limit"].addSC("<1-32767>", "Number (ring limit)");
