
vlanDBC.addSC("abort", "Exit mode without applying the changes");
vlanDBC.addSC("apply", "Apply current changes and bump revision number");
vlanDBC.addSC("exit", "Apply changes, bump revision number, and exit mode");
vlanDBC.addSC("no", "Negate a command or set its defaults");
vlanDBC.addSC("reset", "Abandon current changes and reread current database");
vlanDBC.addSC("show", "Show database information");
	vlanDBC.show.addSC("changes", "Show the changes to the database since modification began (or since 'reset')");
		vlanDBC.show.changes.addSC("<1-1005>", "ID number of the VLAN shown");
	vlanDBC.show.addSC("current", "Show the database installed when modification began (or since 'reset')");
		vlanDBC.show.current.addSC("<1-1005>", "ID number of the VLAN shown");
	vlanDBC.show.addSC("proposed", "Show the database as it would be modified if applied");
		vlanDBC.show.proposed.addSC("<1-1005>", "ID number of the VLAN shown");
vlanDBC.addSC("vlan", "Add, delete, or modify values associated with a single VLAN");
	vlanDBC.vlan.addSC("<1-1005>", "ISL VLAN index");
		vlanDBC.vlan["<1-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
			vlanDBC.vlan["<1-1005>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
		vlanDBC.vlan["<1-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
			vlanDBC.vlan["<1-1005>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
				vlanDBC.vlan["<1-1005>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].backupcrf.disable.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
			vlanDBC.vlan["<1-1005>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
				vlanDBC.vlan["<1-1005>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].backupcrf.enable.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
		vlanDBC.vlan["<1-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
			vlanDBC.vlan["<1-1005>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
				vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].bridge["<0-15>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
			vlanDBC.vlan["<1-1005>"].bridge.addSC("type", "Bridge type");
				vlanDBC.vlan["<1-1005>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
					vlanDBC.vlan["<1-1005>"].bridge.type.srb.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].bridge.type.srb.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
					vlanDBC.vlan["<1-1005>"].bridge.type.srb.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].bridge.type.srb.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].bridge.type.srb.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
				vlanDBC.vlan["<1-1005>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
					vlanDBC.vlan["<1-1005>"].bridge.type.srt.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].bridge.type.srt.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
					vlanDBC.vlan["<1-1005>"].bridge.type.srt.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].bridge.type.srt.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].bridge.type.srt.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("media", "Media type of the VLAN");
			vlanDBC.vlan["<1-1005>"].media.addSC("ethernet", "VLAN type Ethernet");
				vlanDBC.vlan["<1-1005>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media.ethernet.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.ethernet.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.ethernet.backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media.ethernet.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.ethernet.backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.ethernet.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].media.ethernet.bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.ethernet.bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.ethernet.bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].media.ethernet.bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].media.ethernet.bridge.type.addSC("srt", "VLAN Bridge Type SRT");
			vlanDBC.vlan["<1-1005>"].media.addSC("fd-net", "VLAN type FDDI Net");
				vlanDBC.vlan["<1-1005>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media["fd-net"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media["fd-net"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media["fd-net"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media["fd-net"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media["fd-net"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].media["fd-net"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].media["fd-net"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].media["fd-net"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media["fd-net"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].media["fd-net"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].media["fd-net"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
			vlanDBC.vlan["<1-1005>"].media.addSC("fddi", "VLAN type FDDI");
				vlanDBC.vlan["<1-1005>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media.fddi.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.fddi.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.fddi.backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media.fddi.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.fddi.backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.fddi.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].media.fddi.bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.fddi.bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.fddi.bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].media.fddi.bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].media.fddi.bridge.type.addSC("srt", "VLAN Bridge Type SRT");
			vlanDBC.vlan["<1-1005>"].media.addSC("tokenring", "VLAN type Token Ring");
				vlanDBC.vlan["<1-1005>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media.tokenring.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.tokenring.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.tokenring.backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media.tokenring.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.tokenring.backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.tokenring.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].media.tokenring.bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].media.tokenring.bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media.tokenring.bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].media.tokenring.bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].media.tokenring.bridge.type.addSC("srt", "VLAN Bridge Type SRT");
			vlanDBC.vlan["<1-1005>"].media.addSC("tr-net", "VLAN type Token Ring Net");
				vlanDBC.vlan["<1-1005>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media["tr-net"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media["tr-net"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media["tr-net"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].media["tr-net"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].media["tr-net"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].media["tr-net"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].media["tr-net"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].media["tr-net"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].media["tr-net"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].media["tr-net"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].media["tr-net"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
		vlanDBC.vlan["<1-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
			vlanDBC.vlan["<1-1005>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
				vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].mtu["<1500-18190>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("name", "Ascii name of the VLAN");
			vlanDBC.vlan["<1-1005>"].name.addSC("WORD", "The ascii name for the VLAN");
				vlanDBC.vlan["<1-1005>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].name.WORD.bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].name.WORD.bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].name.WORD.bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].name.WORD.addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].name.WORD.media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].name.WORD.media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].name.WORD.media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].name.WORD.mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].name.WORD.mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].name.WORD.mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
			vlanDBC.vlan["<1-1005>"].parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].parent["<0-1005>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
		vlanDBC.vlan["<1-1005>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
			vlanDBC.vlan["<1-1005>"].ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].ring["<1-4095>"].parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
		vlanDBC.vlan["<1-1005>"].addSC("said", "IEEE 802.10 SAID");
			vlanDBC.vlan["<1-1005>"].said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
				vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].said["<1-4294967294>"].ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
		vlanDBC.vlan["<1-1005>"].addSC("state", "Operational state of the VLAN");
			vlanDBC.vlan["<1-1005>"].state.addSC("active", "VLAN Active State");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].state.active.bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].state.active.bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].state.active.bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].state.active.media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].state.active.media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].state.active.media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].state.active.media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].state.active.media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].state.active.mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].state.active.mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.active.name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].state.active.parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].state.active.parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].state.active.parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].state.active.ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"].state.active.addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].state.active.said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].state.active.said["<1-4294967294>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
			vlanDBC.vlan["<1-1005>"].state.addSC("suspend", "VLAN Suspended State");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].state.suspend.bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].state.suspend.bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].state.suspend.bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].state.suspend.media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].state.suspend.media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].state.suspend.mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].state.suspend.mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"].state.suspend.name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].state.suspend.parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].state.suspend.parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].state.suspend.parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].state.suspend.ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"].state.suspend.addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].state.suspend.said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].state.suspend.said["<1-4294967294>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
		vlanDBC.vlan["<1-1005>"].addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
			vlanDBC.vlan["<1-1005>"].ste.addSC("<0-13>", "Maximumn number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].said["<1-4294967294>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"].ste["<0-13>"].addSC("state", "Operational state of the VLAN");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.addSC("active", "VLAN Active State");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.active.addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.addSC("suspend", "VLAN Suspended State");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].ste["<0-13>"].state.suspend.addSC("said", "IEEE 802.10 SAID");
		vlanDBC.vlan["<1-1005>"].addSC("stp", "Spanning tree characteristics of the VLAN");
			vlanDBC.vlan["<1-1005>"].stp.addSC("type", "Spanning tree type of the VLAN");
				vlanDBC.vlan["<1-1005>"].stp.type.addSC("auto", "VLAN STP Type Auto for FDDI Net or Token Ring Net type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.bridge.addSC("type", "Bridge type");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.media.addSC("tr-net", "VLAN type Token Ring Net");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.name.addSC("WORD", "The ascii name for the VLAN");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("said", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("state", "Operational state of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.state.addSC("active", "VLAN Active State");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.state.addSC("suspend", "VLAN Suspended State");
					vlanDBC.vlan["<1-1005>"].stp.type.auto.addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.auto.ste.addSC("<0-13>", "Maximumn number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].stp.type.addSC("ibm", "VLAN STP Type IBM for FDDI Net or Token Ring Net type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.bridge.addSC("type", "Bridge type");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.media.addSC("tr-net", "VLAN type Token Ring Net");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.name.addSC("WORD", "The ascii name for the VLAN");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("said", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("state", "Operational state of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.state.addSC("active", "VLAN Active State");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.state.addSC("suspend", "VLAN Suspended State");
					vlanDBC.vlan["<1-1005>"].stp.type.ibm.addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ibm.ste.addSC("<0-13>", "Maximumn number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"].stp.type.addSC("ieee", "VLAN STP Type IEEE for FDDI Net or Token Ring Net type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.bridge.addSC("type", "Bridge type");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.media.addSC("tr-net", "VLAN type Token Ring Net");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.name.addSC("WORD", "The ascii name for the VLAN");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("said", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("state", "Operational state of the VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.state.addSC("active", "VLAN Active State");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.state.addSC("suspend", "VLAN Suspended State");
					vlanDBC.vlan["<1-1005>"].stp.type.ieee.addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"].stp.type.ieee.ste.addSC("<0-13>", "Maximumn number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
		vlanDBC.vlan["<1-1005>"].addSC("tb-vlan1", "ID number of the first translational VLAN for this VLAN (or zero if none)");
			vlanDBC.vlan["<1-1005>"]["tb-vlan1"].addSC("<0-1005>", "ID number of the first translational VLAN for this VLAN (or zero if none)");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].said["<1-4294967294>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("state", "Operational state of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.addSC("active", "VLAN Active State");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.active.addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.addSC("suspend", "VLAN Suspended State");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].state.suspend.addSC("said", "IEEE 802.10 SAID");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste.addSC("<0-13>", "Maximumn number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("said", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].ste["<0-13>"].addSC("state", "Operational state of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].addSC("stp", "Spanning tree characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].stp.addSC("type", "Spanning tree type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].stp.type.addSC("auto", "VLAN STP Type Auto for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].stp.type.addSC("ibm", "VLAN STP Type IBM for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan1"]["<0-1005>"].stp.type.addSC("ieee", "VLAN STP Type IEEE for FDDI Net or Token Ring Net type VLANs");
		vlanDBC.vlan["<1-1005>"].addSC("tb-vlan2", "ID number of the second translational VLAN for this VLAN (or zero if none)");
			vlanDBC.vlan["<1-1005>"]["tb-vlan2"].addSC("<0-1005>", "ID number of the second translational VLAN for this VLAN (or zero if none)");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].are.addSC("<0-13>", "Maximumn number of All Route Explorer hops for this VLAN (or zero if none specified)");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].backupcrf.addSC("disable", "Disable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].backupcrf.disable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].backupcrf.addSC("enable", "Enable backup CRF mode for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].backupcrf.enable.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].bridge.addSC("<0-15>", "Value of the bridge number for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].bridge["<0-15>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].bridge["<0-15>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].bridge.addSC("type", "Bridge type");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].bridge.type.addSC("srb", "VLAN Bridge Type SRB");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].bridge.type.addSC("srt", "VLAN Bridge Type SRT");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("media", "Media type of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.addSC("ethernet", "VLAN type Ethernet");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.ethernet.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.ethernet.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.ethernet.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.addSC("fd-net", "VLAN type FDDI Net");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media["fd-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media["fd-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media["fd-net"].addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.addSC("fddi", "VLAN type FDDI");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.fddi.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.fddi.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.fddi.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.addSC("tokenring", "VLAN type Token Ring");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.tokenring.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.tokenring.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.tokenring.addSC("bridge", "Bridging characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media.addSC("tr-net", "VLAN type Token Ring Net");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media["tr-net"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media["tr-net"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].media["tr-net"].addSC("bridge", "Bridging characteristics of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].mtu.addSC("<1500-18190>", "Value of VLAN Maximum Tranmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].mtu["<1500-18190>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].mtu["<1500-18190>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].mtu["<1500-18190>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].mtu["<1500-18190>"].addSC("media", "Media type of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("name", "Ascii name of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].name.addSC("WORD", "The ascii name for the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].name.WORD.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].name.WORD.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].name.WORD.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].name.WORD.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].name.WORD.addSC("mtu", "VLAN Maximum Transmission Unit");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent.addSC("<0-1005>", "Value of the ID of the Parent VLAN for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].parent["<0-1005>"].addSC("name", "Ascii name of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring.addSC("<1-4095>", "Value of the ring number for FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ring["<1-4095>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said.addSC("<1-4294967294>", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].said["<1-4294967294>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("state", "Operational state of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.addSC("active", "VLAN Active State");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.active.addSC("said", "IEEE 802.10 SAID");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.addSC("suspend", "VLAN Suspended State");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].state.suspend.addSC("said", "IEEE 802.10 SAID");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste.addSC("<0-13>", "Maximumn number of Spanning Tree Explorer hops for this VLAN (or zero if none specified)");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("said", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].ste["<0-13>"].addSC("state", "Operational state of the VLAN");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("stp", "Spanning tree characteristics of the VLAN");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].stp.addSC("type", "Spanning tree type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].stp.type.addSC("auto", "VLAN STP Type Auto for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].stp.type.addSC("ibm", "VLAN STP Type IBM for FDDI Net or Token Ring Net type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].stp.type.addSC("ieee", "VLAN STP Type IEEE for FDDI Net or Token Ring Net type VLANs");
				vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"].addSC("tb-vlan1", "ID number of the first translational VLAN for this VLAN (or zero if none)");
					vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"].addSC("<0-1005>", "ID number of the first translational VLAN for this VLAN (or zero if none)");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("are", "Maximum number of All Route Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("backupcrf", "Backup CRF mode of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("bridge", "Bridging characteristics of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("media", "Media type of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("mtu", "VLAN Maximum Transmission Unit");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("name", "Ascii name of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("parent", "ID number of the Parent VLAN of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("ring", "Ring number of FDDI or Token Ring type VLANs");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("said", "IEEE 802.10 SAID");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("state", "Operational state of the VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("ste", "Maximum number of Spanning Tree Explorer hops for this VLAN");
						vlanDBC.vlan["<1-1005>"]["tb-vlan2"]["<0-1005>"]["tb-vlan1"]["<0-1005>"].addSC("stp", "Spanning tree characteristics of the VLAN");
vlanDBC.addSC("vtp", "Perform VTP administrative functions.");
	vlanDBC.vtp.addSC("client", "Set the device to client mode.");
	vlanDBC.vtp.addSC("domain", "Set the name of the VTP administrative domain.");
		vlanDBC.vtp.domain.addSC("WORD", "The ascii name for the VTP administrative domain.");
	vlanDBC.vtp.addSC("password", "Set the password for the VTP administrative domain.");
		vlanDBC.vtp.password.addSC("WORD", "The ascii password for the VTP administrative");
		vlanDBC.vtp.password.addSC("domain.", "");
	vlanDBC.vtp.addSC("pruning", "Set the administrative domain to permit pruning.");
	vlanDBC.vtp.addSC("server", "Set the device to server mode.");
	vlanDBC.vtp.addSC("transparent", "Set the device to transparent mode.");
	vlanDBC.vtp.addSC("v2-mode", "Set the administrative domain to V2 mode.");
