Router-A#show ip bgp neighbors
BGP neighbor is 2.0.0.1,  remote AS 300, internal link
  BGP version 4, remote router ID 10.0.0.1
  BGP state = Established, up for 00:56:13
  Last read 00:00:13, hold time is 180, keepalive interval is 60 seconds
  Neighbor capabilities:
    Route refresh: advertised and received
    Address family IPv4 Unicast: advertised and received
  Received 203 messages, 0 notifications, 0 in queue
  Sent 199 messages, 0 notifications, 0 in queue
  Route refresh request: received 0, sent 0
  Minimum time between advertisement runs is 5 seconds

 For address family: IPv4 Unicast
  BGP table version 12, neighbor version 12
  Index 1, Offset 0, Mask 0x2
  2 accepted prefixes consume 72 bytes
  Prefix advertised 4, suppressed 0, withdrawn 2

  Connections established 2; dropped 1
  Last reset 00:56:24, due to Peer closed the session
Connection state is ESTAB, I/O status: 1, unread input bytes: 0
Local host: 2.0.0.2, Local port: 179
Foreign host: 2.0.0.1, Foreign port: 11032

Enqueued packets for retransmit: 0, input: 0  mis-ordered: 0 (0 bytes)

Event Timers (current time is 0xCEE180):
Timer          Starts    Wakeups            Next
Retrans            61          0             0x0
TimeWait            0          0             0x0
AckHold            59         43             0x0
SendWnd             0          0             0x0
KeepAlive           0          0             0x0
GiveUp              0          0             0x0
PmtuAger            0          0             0x0
DeadWait            0          0             0x0

iss: 2595724234  snduna: 2595725431  sndnxt: 2595725431     sndwnd:  15188
irs: 2835463828  rcvnxt: 2835465082  rcvwnd:      15131  delrcvwnd:   1253

SRTT: 300 ms, RTTO: 607 ms, RTV: 3 ms, KRTT: 0 ms
minRTT: 16 ms, maxRTT: 300 ms, ACK hold: 200 ms
Flags: passive open, nagle, gen tcbs

Datagrams (max data segment is 1460 bytes):
Rcvd: 79 (out of order: 0), with data: 59, total data bytes: 1253
Sent: 104 (retransmit: 0), with data: 60, total data bytes: 1196
Router-A#
