Output=Router+A%23show+running%2Dconfig%0ARouter+A+Configuration%0Ainterface+serial+0%0Aip+address+170%2E10%2E62%2E1+255%2E255%2E255%2E0%0A%0Ainterface+serial+1%0Aip+address+170%2E10%2E63%2E1+255%2E255%2E255%2E0%0A%0Ainterface+ethernet+0%0Aip+address+170%2E10%2E8%2E1+255%2E255%2E255%2E0%0A%0Ainterface+tokenring+0%0Aip+address+170%2E10%2E9%2E1+255%2E255%2E255%2E0%0A%0Arouter+rip%0Anetwork+170%2E10%2E0%2E0%0A%0ARouter+A%23%0A++