Content

| Summary

EIGRP, a Cisco proprietary routing protocol, is an advanced distance vector protocol that uses the DUAL algorithm. It includes features such as rapid convergence, reduced bandwidth usage, and multiple network-layer support.

EIGRP converges rapidly, performs incremental updates, routes IP, and summarizes routes. The labs demonstrated how to configure and verify EIGRP configuration for various protocols.