Output=Router+A%23show+running%2Dconfig%0Ainterface+serial+0+%0Aip+address+130%2E10%2E62%2E1+255%2E255%2E255%2E0+%0Ainterface+serial+1+%0Aip+address+130%2E10%2E63%2E1+255%2E255%2E255%2E0+%0Ainterface+ethernet+0+%0Aip+address+130%2E10%2E8%2E1+255%2E255%2E255%2E0+%0Ainterface+tokenring+0+%0Aip+address+130%2E10%2E9%2E1+255%2E255%2E255%2E0+%0A%21+%0Arouter+rip+%0Adefault%2Dmetric+10+%0Anetwork+130%2E10%2E0%2E0+%0Apassive%2Dinterface+serial+0+%0Apassive%2Dinterface+serial+1+%0Aredistribute+ospf+109+match+internal+external+1+external+2+%0A%21+%0Arouter+ospf+109+%0Anetwork+130%2E10%2E62%2E0+0%2E0%2E0%2E255+area+0+%0Anetwork+130%2E10%2E63%2E0+0%2E0%2E0%2E255+area+0+%0Aredistribute+rip+subnets+%0Adistribute%2Dlist+11+out+rip+%0A%21+%0Aaccess%2Dlist+11+permit+130%2E10%2E8%2E0+0%2E0%2E7%2E255+%0Aaccess%2Dlist+11+deny+0%2E0%2E0%2E0+255%2E255%2E255%2E255+%0ARouter+A%23%0A